<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.254" x2="100" y2="0.254" width="0" layer="20"/>
<wire x1="100" y1="0.254" x2="100" y2="50.546" width="0" layer="20"/>
<wire x1="100" y1="50.546" x2="0" y2="50.546" width="0" layer="20"/>
<wire x1="0" y1="50.546" x2="0" y2="0.254" width="0" layer="20"/>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>GND</text>
<text>GND</text>
<text>SCL</text>
<text>VCC</text>
<text>SDA</text>
<text>~IRQ</text>
<text>TOUCHBOARD01A</text>
<text>MLAB</text>
<text>2013</text>
<text>2013</text>
<text>MLAB</text>
<text>TOUCHBOARD01A</text>
<text>JACHO</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QFN-20-0.4MM">
<description>** 20-pin QFN ** 
initially designed for MPR121 | 
0.4mm pitch | 
3x3x0.65mm |
** VERY UNPROVEN **</description>
</package>
</packages>
</library>
<library name="moje_C">
<packages>
<package name="C0805">
</package>
</packages>
</library>
<library name="moje_R">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="moje_hrebinky">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA06-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="moje">
<packages>
<package name="SROUB3M">
</package>
</packages>
</library>
<library name="moje_tlacitka">
<packages>
<package name="PLOSKA10_15">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun" package="QFN-20-0.4MM" value="MPR121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="moje_C" package="C0805" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C1" library="moje_C" package="C0805" value="100nF">
<attribute name="NAME"/>
</element>
<element name="R1" library="moje_R" package="0805" value="75k 1%">
<attribute name="NAME"/>
</element>
<element name="SV1" library="moje_hrebinky" package="MA06-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="moje" package="SROUB3M" value="SROUB3M"/>
<element name="X2" library="moje" package="SROUB3M" value="SROUB3M"/>
<element name="X3" library="moje" package="SROUB3M" value="SROUB3M"/>
<element name="X4" library="moje" package="SROUB3M" value="SROUB3M"/>
<element name="U$1" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$2" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$3" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$4" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$5" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$6" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$7" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$8" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$9" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$10" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$11" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
<element name="U$12" library="moje_tlacitka" package="PLOSKA10_15" value="TL_DOTYK_10_15"/>
</elements>
<signals>
<signal name="VREG">
<contactref element="IC1" pad="5"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="~IRQ">
<contactref element="IC1" pad="1"/>
<contactref element="SV1" pad="12"/>
<contactref element="SV1" pad="11"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="2"/>
<contactref element="SV1" pad="4"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="3"/>
<contactref element="SV1" pad="8"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="REXT">
<contactref element="IC1" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="P$1"/>
<contactref element="X4" pad="P$1"/>
<contactref element="X3" pad="P$1"/>
<contactref element="X2" pad="P$1"/>
<contactref element="SV1" pad="1"/>
<contactref element="SV1" pad="2"/>
<contactref element="SV1" pad="9"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="20"/>
<contactref element="C2" pad="1"/>
<contactref element="SV1" pad="5"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="KEY11">
<contactref element="IC1" pad="19"/>
<contactref element="U$12" pad="P$1"/>
</signal>
<signal name="KEY10">
<contactref element="IC1" pad="18"/>
<contactref element="U$11" pad="P$1"/>
</signal>
<signal name="KEY9">
<contactref element="IC1" pad="17"/>
<contactref element="U$10" pad="P$1"/>
</signal>
<signal name="KEY8">
<contactref element="IC1" pad="16"/>
<contactref element="U$9" pad="P$1"/>
</signal>
<signal name="KEY7">
<contactref element="IC1" pad="15"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="KEY6">
<contactref element="IC1" pad="14"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="KEY5">
<contactref element="IC1" pad="13"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="KEY4">
<contactref element="IC1" pad="12"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="KEY3">
<contactref element="IC1" pad="11"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="KEY2">
<contactref element="IC1" pad="10"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="KEY1">
<contactref element="IC1" pad="9"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="KEY0">
<contactref element="IC1" pad="8"/>
<contactref element="U$1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
