{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["APLIFIER"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"APLIFIER","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["VLF AMPLIFIER"]
["Quantity","Reference","Part","PCB Footprint",null,"Obj. číslo GM","Cena/ks","cena","Popis"]
[1,"C1","15nF","CK050","CF1-15N/J","121-339",2,2,"foliovy kondenzator 15nF"]
[3,"C2,C5,C6","100nF","CK050",null,null,2.5,7.5]
[1,"C3","4,7nF","CK050","CK 4N7/100V2","120-049",6,6]
[1,"C4","100pF","CK050","CK 100P/500V","120-026",2,2]
[1,"C8","330uF","CE035X8","E330M/16V","123-147",2.5,2.5]
[2,"D1,D2","1N4937","DO41","1N4937","220-019",1,2," \tRychlá dioda 600V 1A DO-41"]
[3,"J2, J3, J4","ARK210/2","ARK210/2",null,"821-083",4,12,"svorkovnice"]
[1,"L1","3900uH","LL150","TL.3900","611-037",6,6,"civka 3900uH "]
[1,"Q1","BF245","TO92","BF245B","213-002",3,3,"N J-FET"]
[1,"R1",100,"RL090",null,null,1,1]
[2,"R2,R3","4k7","RL090",null,null,1,2]
[1,"R4","10k","RL090","RR 10K",null,1,1]
[1,"R5","100k","RL090","RR 100K","110-121",1,1]
[1,"U1","NE5534","DIP8_300","NE5534","310-025",7,7,"nizkosumovy operak"]
[{"$nulls":7},55]