{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["MB01B","Objednat GM"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"MB01B","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["MB01B"]
[]
["Počet","Reference","Název","Název GM","Obj. číslo GM","Cena zhruba","Popis"]
["Odpory"]
["1","R15",10,"RR10R","110-025",0.8,"Odpor"]
["2","R4,R1",680,"RR680R","110-069",0.8,"Odpor"]
["1","R11","2k2","RR2K2","110-081",0.8,"Odpor"]
["8","R2,R3,R5,R6,R9,R10,R13,R14","10k","RR10K","110-097",0.8,"Opdor"]
["2","R7,R12","27k","RR27K","110-017",0.8,"Odpor"]
["1","R8","100k","RR100K","110-121",0.8,"Odpor"]
["Opdorové trimry"]
["1","P1","10k","PT10VK010","112-049",8,"Trimr"]
["Kondenzátory"]
["2","C4,C5","22pF","CKS22P/50V","120-125",0.7,"Keramický kondenzátor"]
["1","C14","4n7","CKS4N7/50V","120-142",0.7,"Keramický kondenzátor"]
["5","C3,C6,C7,C8,C9","10nF","CK10N/63V","120-053",2,"Keramický kondenzátor"]
["2","C15,C16","33nF","CK33N/50V","120-077",2,"Keramický kondenzátor"]
["3","C1,C2,C10","100nF","CK100N/63V","120-060",1,"Keramický kondenzátor"]
["1","C13","1M/63V","E1M/63V","123-016",1,"Elektrolyt"]
["1","C12","47uF/16V","E47M/16V","123-092",1,"Elektrolyt"]
["2","C11,C17","330uF/16V","E330M/16V","123-147",2.5,"Elektrolyt"]
["Polovodiče a krystaly"]
["1","D1","1N4005","1N4007","220-002",1,"Dioda 1A"]
["4","D3,D4,D5,D6","1N4148","1N4148","220-003",1,"Dioda"]
["1","D2","BZX83V005.1","BZX83V005.1","220-018",1,"Zenerova dioda 5.1V"]
["1","Q1","BC327","BC327-40","210-014",1.5,"Tranzistor PNP"]
["1","Q2","BC337","BC337-40","210-019",1.5,"Tranzistor NPN"]
["1","Q3","BC640","BC640","210-109",3,"Tranzistor PNP 1A"]
["1","U1","PIC16F819-I/P","PIC16F819-I/P","434-233",75,"Procesor"]
["1","U2","LM386","LM386","313-011",6,"Zesilovač"]
["1","X1","20MHz","QM20MHz","131-080",9.9,"Xtal, může být i Q20M"]
["Mechanické součásti"]
["4","SW1,SW2,SW3,SW4","P-B1720","P-B1720","630-008",3,"Tlačítko 5x5mm"]
["2","J1,J2","JUMP3","nic","nic",0,"Hřebínek 3 piny"]
["1","J3","JUMP5","nic","nic",0,"Hřebínek 5 pinu"]
["1","J5","JUMP2","nic","nic",0,"Hrebinek 2 piny"]
["1","J6","PIC_ISP","S1G20","832-017",4,"Hřebínek 6 pinu (naláme se)"]
["1","J4","DB9M_90","CAN9V90","801-037",8,"Konektor Cannon 9 do plošných spojů, samec"]
["Mechanické součásti další"]
["1",null,"SOKL8","SOKL8","823-011",1,"Sokl DIL8 obyčejný"]
["1",null,"SOKL18","SOKL18","823-003",1.9,"Sokl DIL18 obyčejný"]
["1",null,"JUMP-SW BLACK","JUMP-SW BLACK","832-013",1,"Jumper propojka"]
["1",null,"006-PI","006-PI","819-001",2,"Kontakty na 9V baterii"]
["2",null,"KONPC-SPK-3","KONPC-SPK-3","840-003",1,"Konektor pro 3 pin hřebínek"]
["1",null,"KONPC-SPK-5","KONPC-SPK-5","840-011",2,"Konektor pro 5 pin hřebínek"]
["11",null,"KONPC-SPK-PI","KONPC-SPK-PI","840-004",0.5,"Piny pro konektor KONPC"]
["4",null,"DI5M3X5","DI5M3X5","623-026",2.5,"Distanční matice M3"]
["4",null,"M3x12","Železářství","není",null,"Pozinkovaný šroub M3x12, válcová hlava, křížový"]
["4",null,"M3 podlozka","Železářství","není",null,"Pozinkovaná podložka M3"]
[1,null,"MB01B","Výroba PCB","není",null,"Plošný spoj"]

{"sheet":"Objednat GM","index":1,"n_rows":51,"n_cols":10,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["MB01B",null,null,null,"Počet výrobků",null,20]
[]
["Počet celkem","Rezerva","0 = už máme","Počet na kus","Název","Název GM","Obj. číslo GM","Cena zhruba","Popis","Cena celkem"]
[null,null,null,"Odpory"]
[20,null,1,"1",10,"RR10R","110-025",0.8,"Odpor",16]
[40,null,1,"2",680,"RR680R","110-069",0.8,"Odpor",32]
[20,null,1,"1","2k2","RR2K2","110-081",0.8,"Odpor",16]
[160,null,1,"8","10k","RR10K","110-097",0.8,"Opdor",128]
[40,null,1,"2","27k","RR27K","110-017",0.8,"Odpor",32]
[20,null,1,"1","100k","RR100K","110-121",0.8,"Odpor",16]
[null,null,null,"Opdorové trimry"]
[20,null,1,"1","10k","PT10VK010","112-049",8,"Trimr",160]
[null,null,null,"Kondenzátory"]
[40,null,1,"2","22pF","CKS22P/50V","120-125",0.7,"Keramický kondenzátor",28]
[20,null,1,"1","4n7","CKS4N7/50V","120-142",0.7,"Keramický kondenzátor",14]
[100,null,1,"5","10nF","CK10N/63V","120-053",2,"Keramický kondenzátor",200]
[40,null,1,"2","33nF","CK33N/50V","120-077",2,"Keramický kondenzátor",80]
[60,null,1,"3","100nF","CK100N/63V","120-060",1,"Keramický kondenzátor",60]
[20,null,1,"1","1M/63V","E1M/63V","123-016",1,"Elektrolyt",20]
[20,null,1,"1","47uF/16V","E47M/16V","123-092",1,"Elektrolyt",20]
[40,null,1,"2","330uF/16V","E330M/16V","123-147",2.5,"Elektrolyt",100]
[null,null,null,"Polovodiče a krystaly"]
[20,null,1,"1","1N4005","1N4007","220-002",1,"Dioda 1A",20]
[0,null,0,"4","1N4148","1N4148","220-003",1,"Dioda",0]
[20,null,1,"1","BZX83V005.1","BZX83V005.1","220-018",1,"Zenerova dioda 5.1V",20]
[20,null,1,"1","BC327","BC327-40","210-014",1.5,"Tranzistor PNP",30]
[20,null,1,"1","BC337","BC337-40","210-019",1.5,"Tranzistor NPN",30]
[20,null,1,"1","BC640","BC640","210-109",3,"Tranzistor PNP 1A",60]
[22,2,1,"1","PIC16F819-I/P","PIC16F819-I/P","434-233",75,"Procesor",1650]
[22,2,1,"1","LM386","LM386","313-011",6,"Zesilovač",132]
[20,null,1,"1","20MHz","QM20MHz","131-080",9.9,"Xtal, může být i Q20M",198]
[null,null,null,"Mechanické součásti"]
[80,null,1,"4","P-B1720","P-B1720","630-008",3,"Tlačítko 5x5mm",240]
[40,null,1,"2","JUMP3","nic","nic",0,"Hřebínek 3 piny",0]
[20,null,1,"1","JUMP5","nic","nic",0,"Hřebínek 5 pinu",0]
[20,null,1,"1","JUMP2","nic","nic",0,"Hrebinek 2 piny",0]
[20,null,1,"1","PIC_ISP","S1G20","832-017",4,"Hřebínek 6 pinu (naláme se)",80]
[20,null,1,"1","DB9M_90","CAN9V90","801-037",8,"Konektor Cannon 9 do plošných spojů, samec",160]
[null,null,null,"Mechanické součásti další"]
[20,null,1,"1","SOKL8","SOKL8","823-011",1,"Sokl DIL8 obyčejný",20]
[20,null,1,"1","SOKL18","SOKL18","823-003",1.9,"Sokl DIL18 obyčejný",38]
[0,null,0,"1","JUMP-SW BLACK","JUMP-SW BLACK","832-013",1,"Jumper propojka",0]
[20,null,1,"1","006-PI","006-PI","819-001",2,"Kontakty na 9V baterii",40]
[40,null,1,"2","KONPC-SPK-3","KONPC-SPK-3","840-003",1,"Konektor pro 3 pin hřebínek",40]
[20,null,1,"1","KONPC-SPK-5","KONPC-SPK-5","840-011",2,"Konektor pro 5 pin hřebínek",40]
[220,null,1,"11","KONPC-SPK-PI","KONPC-SPK-PI","840-004",0.5,"Piny pro konektor KONPC",110]
[80,null,1,"4","DI5M3X5","DI5M3X5","623-026",2.5,"Distanční matice M3",200]
[0,null,0,"4","M3x12","Železářství","není",null,"Pozinkovaný šroub M3x12, válcová hlava, křížový",0]
[0,null,0,"4","M3 podlozka","Železářství","není",null,"Pozinkovaná podložka M3",0]
[0,null,0,1,"MB01B","Výroba PCB","není",null,"Plošný spoj",0]
[{"$nulls":8},"Cena celkem",4030]