{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Menič ","CPU a baterie"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Menič ","index":0,"n_rows":63,"n_cols":5,"rows_kept":63,"cut":false,"hidden":false,"merged":[[32,2,35,2],[32,3,35,3],[32,4,35,4],[61,4,62,4],[12,1,12,4],[29,2,30,2],[29,3,30,3],[29,4,30,4]],"flags":["formulas_cached_only"]}
{"$rows_empty":12}
[null,"Měnič - zdroj nabíjecího proudu"]
[null,"Ref","Hodnota","Pouzdro","Poznámka"]
[null,"C1","100nF","C0805"]
[null,"C2","100nF","C0805"]
[null,"C3","330uF/25V","CE035X8/L","nízké ESR, velké proudy  (CERA 330uF/25V 8x15 LXZ  ECOM obj.č 46020)"]
[null,"C4","180uF/50V","CE035X8/L","nízké ESR, velké proudy  (CERA 180uF/50V 8x20 LXZ  ECOM obj.č. 46084)"]
[null,"C5","330uF/25V","CE035X8/L","nízké ESR, velké proudy  (CERA 330uF/25V 8x15 LXZ  ECOM obj.č 46020)"]
[null,"C6","330uF/25V","CE035X8/L","nízké ESR, velké proudy  (CERA 330uF/25V 8x15 LXZ  ECOM obj.č 46020)"]
[null,"C7","330uF/25V","CE035X8/L","nízké ESR, velké proudy  (CERA 330uF/25V 8x15 LXZ  ECOM obj.č 46020)"]
[null,"C8","100nF","C0805"]
[null,"C9","100nF","C0805"]
[null,"C10","100nF","C0805"]
[null,"C11","100nF","C0805"]
[null,"C12","#10nF","C0805","neosazuje se"]
[null,"C13","1nF","C0805"]
[null,"D2","SK36A","SMA"]
[null,"D3","SK36A","SMA"]
[null,"J1","1x K3716A",null,"zásuvka 2,1 mm na panel, značení GM"]
[null,"J2"]
[null,"L1","TL. SMT73 15uF","SMT73","značení GM SMD tlumivka 15uH 2A 7x7,8x5mm"]
[null,"M1","2x60uH","toroid T17","vinuto bifilárně drátem 0.8mm 28závitů na toroidním jádře T17 z materiálu uCool dodá PME Šumperk www.pme.cz \nPři zapojování pozor na smysly vinutí !!!"]
[null,"M2"]
[null,"M3"]
[null,"M4"]
[null,"Q1","IRF7416SMD","SO8_FET"]
[null,"Q2","IRF540","TO220"]
[null,"Q3","BC856SMD","SOT23"]
[null,"R1","8k2","R0805"]
[null,"R001",0,"R0805"]
[null,"R2","1k","R0805"]
[null,"R3","1k","R0805"]
[null,"R4A","3k3","R0805"]
[null,"R4B","#33k","R0805","pro dostavení výstupního napětí měniče na 19V - max 20V"]
[null,"R5",470,"R0805"]
[null,"R6","1j","klasický 0,6W","určuje maximální dobíjecí proud, vhodné zvolit 0,2C"]
[null,"R7","4j7","klasický 0,6W","určuje maximální dobíjecí proud, vhodné zvolit 0,2C"]
[null,"R8","10k","R0805"]
[null,"R9","1k2","R0805"]
[null,"R10","2k2","R0805"]
[null,"R11","220k","R0805"]
[null,"R12","22k","R0805"]
[null,"R13","4k7","R0805"]
[null,"R14","4k7","R0805"]
[null,"R15","220k","R0805"]
[null,"R16","#100","R0805","neosazuje se"]
[null,"R17","12k","R0805"]
[null,"U1","TL494/SO","SO16_150"]
[null,null,"SIS-TO220",null,"izolační podložka pod TO220"]
[null,null,"IB2",null,"izolace šroubu pro TO220"]
[null,null,"šroub M3 plochá hlava",null,"pro přišroubování Q2 k DPS"]
[null,null,"matice M3 nízký profil"]

{"sheet":"CPU a baterie","index":1,"n_rows":63,"n_cols":5,"rows_kept":63,"cut":false,"hidden":false,"merged":[[57,4,59,4],[2,1,2,4],[42,4,46,4],[16,2,18,2],[16,3,18,3],[16,4,18,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"CPU a řídící obvody"]
[null,"Ref","Hodnota","Pouzdro","Poznámka"]
[null,"C100","100nF","C0805"]
[null,"C101","22uF/6.3V","ELYTC"]
[null,"C102","10nF","C0805"]
[null,"C103","100nF","C0805"]
[null,"C104","100nF","C0805"]
[null,"C105","100nF","C0805"]
[null,"D100","1N4148SMD","SOD87"]
[null,"D101","1N4148SMD","SOD87"]
[null,"D102","zelená","LED3mm","s nízkou spotřebou"]
[null,"D103","žlutá","LED3mm","s nízkou spotřebou"]
[null,"D104","žlutá","LED3mm","s nízkou spotřebou"]
[null,"D105","červená","LED3mm","s nízkou spotřebou"]
[null,"J101","1x K3716B",null,"zásuvka 2,5 mm na panel \nJ103 připojit na rozpínací kontakt"]
[null,"J102"]
[null,"J103"]
[null,"J104","JUMP6","PIC_ISP","hřebínek naležato"]
[null,"J105","JUMP2","JUMP2","jen plošky, pro reset CPU"]
[null,"J106","DS18B20","JUMP2","Teploměr připevněn na spodní stranu baterie. POZOR na polaritu.Připojit až po naprogramování CPU"]
[null,"J107","JUMP1","JUMP1","kladný pól baterie"]
[null,"J108","JUMP1","JUMP1","záporný pól baterie"]
[null,"J109","#JUMP1","JUMP1","neosazuje se"]
[null,"Q100","IRF7316SMD","SO8_2FET"]
[null,"Q101","IRF7416SMD","SO8_FET"]
[null,"Q102","BSS138","SOT23"]
[null,"Q103","BSS138","SOT23"]
[null,"Q104","BSS138","SOT23"]
[null,"R104","10k 1%","R0805"]
[null,"R111","10k 1%","R0805"]
[null,"R115","10k 1%","R0805"]
[null,"R117","10k","R0805"]
[null,"R123","2k2","R0805"]
[null,"R122","4k7","R0805"]
[null,"R101","100k","R0805"]
[null,"R102","100k","R0805"]
[null,"R105","100k","R0805"]
[null,"R112","100k 1%","R0805"]
[null,"R113","100k 1%","R0805"]
[null,"R103","68k 1%","klasika"]
[null,"R106","2x1j_parallel_or_j5","R0805","výsledný odpor 0,1 ohm\nsložen z 10 ks 1ohm R0805 1%"]
[null,"R107","2x1j_parallel_or_j5","R0805"]
[null,"R108","2x1j_parallel_or_j5","R0805"]
[null,"R109","2x1j_parallel_or_j5","R0805"]
[null,"R110","2x1j_parallel_or_j5","R0805"]
[null,"R114","2M7","R0805"]
[null,"R116","2k2","RL090"]
[null,"R118",560,"R0805"]
[null,"R119",560,"R0805"]
[null,"R120",560,"R0805"]
[null,"R121",560,"R0805"]
[null,"U100","LP2951CD","SO8_150"]
[null,"U101","PIC16F88/SO","SO18_300"]
[null,"U102","TLC27L2SMD","SO8_150"]
[null,null,"10xNiMh 1,2V/3500mAh","velikost 4/3A"]
[null,null,"2x třmen hliníkový plech ",null,"pro uchycení baterie do krabičky"]
[null,null,"4x M2 šroub"]
[null,null,"4x M2 matice"]
[null,null,"4x GF7",null,"samolepící nožičky, značení GM"]
[null,null,"ALUBOX 3/B",null,"krabička, dodá SOS Electronic"]
[null,null,"oboustranná samolepící páska",null,"pro přilepení DPS do krabičky, nejlépe od fy 3M"]