(kicad_pcb (version 4) (host pcbnew "(2015-12-20 BZR 6390, Git 4e99c98)-product")
  (general
    (links 92)
    (no_connects 0)
    (area 120.178999 74.538999 160.461001 114.821001)
    (thickness 1.6)
    (drawings 17)
    (tracks 352)
    (zones 0)
    (modules 44)
    (nets 27)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 VAA)
  (net 4 GNDA)
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(J4-Pad1)")
  (net 8 "Net-(J5-Pad1)")
  (net 9 "Net-(J6-Pad1)")
  (net 10 "Net-(J7-Pad1)")
  (net 11 "Net-(J8-Pad1)")
  (net 12 "Net-(J9-Pad1)")
  (net 13 "Net-(J10-Pad2)")
  (net 14 "Net-(J11-Pad1)")
  (net 15 "Net-(J12-Pad1)")
  (net 16 "Net-(J13-Pad1)")
  (net 17 "Net-(J14-Pad1)")
  (net 18 "Net-(J15-Pad1)")
  (net 19 "Net-(J16-Pad1)")
  (net 20 "Net-(J17-Pad1)")
  (net 21 "Net-(J18-Pad1)")
  (net 22 "Net-(J20-Pad1)")
  (net 23 "Net-(J21-Pad1)")
  (net 24 "Net-(U1-Pad2)")
  (net 25 "Net-(U1-Pad4)")
  (net 26 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GNDA)
    (add_net VAA)
    (add_net VCC)
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F1324F)
    (at 134.0335 78.932)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0.127 -0.127 90) (layer F.SilkS) hide)
    (fp_text value AIN1- (at 1.143 -3.556 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J5-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J5-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 555EF748)
    (at 143.622 101.792)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C1 (at 3.937 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.7) (layer B.Fab))
    (pad 2 smd rect (at 1.46 0) (size 1.8 2.23) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.46 0) (size 1.8 2.23) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 144.13 96.458 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -2.921 -0.127 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 150.734 83.504 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 2.032 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 132.192 87.822 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0.127 1.905 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer B.Cu) (tedit 552FF239)
    (at 147.432 108.396 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 -2.921 270) (layer B.SilkS))
    (fp_text value M4 (at 0.127 -3.048 270) (layer B.Fab))
    (fp_text user K (at -2.9 -2.95 270) (layer B.SilkS))
    (fp_text user A (at 2.9 -2.9 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer B.Cu) (tedit 569892F8)
    (at 132.7 108.396 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at -0.573 -0.2055 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -4.3 270) (layer B.Fab))
    (fp_text user K (at -3.175 2.794 270) (layer B.SilkS))
    (fp_text user A (at 4.699 0.127 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55F13097)
    (at 142.606 108.142 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0.127 -5.08 180) (layer F.SilkS) hide)
    (fp_text value 3÷5V (at -5.842 -0.127 180) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12EC8)
    (at 156.068 88.838 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ACX (at 0 -4.953 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12ED3)
    (at 156.068 86.298 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ~ACX (at -0.127 -4.953 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J3-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J3-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F1316D)
    (at 131.4935 78.932)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0.127 0.127 90) (layer F.SilkS) hide)
    (fp_text value AIN1+ (at -2.3345 -0.0015 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J4-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J4-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F131E6)
    (at 136.5735 78.932)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0.127 0.127 90) (layer F.SilkS) hide)
    (fp_text value AIN2+ (at 0.127 5.969 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J6-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J6-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F1320B)
    (at 139.1135 78.932 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at -0.127 -0.254 270) (layer F.SilkS) hide)
    (fp_text value AIN2- (at 0 -5.969 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J7-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J7-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F13218)
    (at 146.7485 78.9305 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at -0.1905 -0.1905 270) (layer F.SilkS) hide)
    (fp_text value REFIN- (at -0.127 -6.731 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J8-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J8-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F131FD)
    (at 141.6535 78.932 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at -0.127 0.127 270) (layer F.SilkS) hide)
    (fp_text value REFIN+ (at 0 -6.858 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J9-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J9-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 55F12E1E)
    (at 139.05 98.236 270)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J10 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value POL (at -3.429 -0.254 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -2.54 270) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 0 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 0 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F1314A)
    (at 125.588 86.552 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 0.127 180) (layer F.SilkS) hide)
    (fp_text value ~RESET (at 0.127 6.35 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J11-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J11-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F13147)
    (at 125.588 89.092 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0.127 -0.127 180) (layer F.SilkS) hide)
    (fp_text value ~SYNC (at 0.381 6.096 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J12-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J12-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12EAA)
    (at 156.068 96.458 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J13 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ~RDY (at -0.127 -5.207 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J13-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J13-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12EB3)
    (at 156.068 93.918 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ~CS (at -0.127 -4.445 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J14-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J14-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F13107)
    (at 125.588 96.712 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J15 (at -0.127 -0.127 180) (layer F.SilkS) hide)
    (fp_text value SCLK (at -2.794 0.127 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J15-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J15-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12EA0)
    (at 156.068 101.538 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J16 (at -0.127 0.127 180) (layer F.SilkS) hide)
    (fp_text value DIN (at -0.127 -4.699 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J16-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J16-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12E81)
    (at 156.068 98.998 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J17 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value DOUT (at -0.127 -5.715 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J17-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J17-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F12EBE)
    (at 156.068 91.378 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J18 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ~STANDBY (at -0.127 -7.859 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J18-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J18-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55F02B3D)
    (at 137.526 108.142)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J19 (at -0.127 5.207) (layer F.SilkS) hide)
    (fp_text value +5V (at -5.08 0) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(D2-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(D2-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F1319B)
    (at 125.588 94.172 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J20 (at -0.127 0 180) (layer F.SilkS) hide)
    (fp_text value MCLKIN (at -3.556 -3.683 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J20-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J20-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 55F13198)
    (at 125.588 91.632 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J21 (at 0.127 0.127 180) (layer F.SilkS) hide)
    (fp_text value MCLKOUT (at 4.064 -3.81 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J21-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J21-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 140.1445 113.157)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at 2.921 -0.127) (layer B.SilkS))
    (fp_text value BLM21PG300SN1D (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 132.954 102.808 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L2 (at -0.127 -1.905 270) (layer B.SilkS))
    (fp_text value BLM21PG300SN1D (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 155.56 79.44)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 155.56 109.92)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm locked placed (layer F.Cu) (tedit 5535DB2C)
    (at 125.08 79.44)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 125.08 109.92)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 129.398 85.602 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.733 -0.127 270) (layer B.SilkS))
    (fp_text value 10k (at -0.254 -2.032 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 121.778 90.362 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.794 0 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 152.258 93.664 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.636 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J18-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 148.829 88.33)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.5) (layer B.SilkS))
    (fp_text value MIC4426 (at 0 -3.5) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-24_4.4x7.8mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 138.735001 91.306534)
    (descr "TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0.060999 -5.135534) (layer B.SilkS))
    (fp_text value AD7730 (at 0 -4.95) (layer B.Fab))
    (pad 1 smd rect (at -2.85 3.575) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J15-Pad1)"))
    (pad 2 smd rect (at -2.85 2.925) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J20-Pad1)"))
    (pad 3 smd rect (at -2.85 2.275) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J21-Pad1)"))
    (pad 4 smd rect (at -2.85 1.625) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J10-Pad2)"))
    (pad 5 smd rect (at -2.85 0.975) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J12-Pad1)"))
    (pad 6 smd rect (at -2.85 0.325) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J11-Pad1)"))
    (pad 7 smd rect (at -2.85 -0.325) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -2.85 -0.975) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (pad 9 smd rect (at -2.85 -1.625) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (pad 10 smd rect (at -2.85 -2.275) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J4-Pad1)"))
    (pad 11 smd rect (at -2.85 -2.925) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J5-Pad1)"))
    (pad 12 smd rect (at -2.85 -3.575) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J6-Pad1)"))
    (pad 13 smd rect (at 2.85 -3.575) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J7-Pad1)"))
    (pad 14 smd rect (at 2.85 -2.925) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J9-Pad1)"))
    (pad 15 smd rect (at 2.85 -2.275) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J8-Pad1)"))
    (pad 16 smd rect (at 2.85 -1.625) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U1-Pad2)"))
    (pad 17 smd rect (at 2.85 -0.975) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U1-Pad4)"))
    (pad 18 smd rect (at 2.85 -0.325) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J18-Pad1)"))
    (pad 19 smd rect (at 2.85 0.325) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J14-Pad1)"))
    (pad 20 smd rect (at 2.85 0.975) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J13-Pad1)"))
    (pad 21 smd rect (at 2.85 1.625) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J17-Pad1)"))
    (pad 22 smd rect (at 2.85 2.275) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J16-Pad1)"))
    (pad 23 smd rect (at 2.85 2.925) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 24 smd rect (at 2.85 3.575) (size 1.1 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_SSOP.3dshapes/TSSOP-24_4.4x7.8mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 0)
    (at 131.303 95.188 270)
    (descr "Crystal, Quarz, HC49/U, vertical, stehend,")
    (tags "Crystal, Quarz, HC49/U, vertical, stehend,")
    (fp_text reference Y1 (at -0.381 -3.048 270) (layer F.SilkS))
    (fp_text value "4.9152 MHz" (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0 270) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J21-Pad1)"))
    (pad 2 thru_hole circle (at 2.44094 0 270) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J20-Pad1)"))
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 569892E2)
    (at 146.797 83.504 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C4 (at -0.4595 -0.062 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.7 180) (layer B.Fab))
    (pad 2 smd rect (at 1.46 0 180) (size 1.8 2.23) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (pad 1 smd rect (at -1.46 0 180) (size 1.8 2.23) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 555EF748)
    (at 129.144 101.03 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow")
    (tags "Tantal Capacitor Size-B EIA-3528 Reflow")
    (attr smd)
    (fp_text reference C5 (at -0.127 2.413 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.7 180) (layer B.Fab))
    (pad 2 smd rect (at 1.46 0 180) (size 1.8 2.23) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (pad 1 smd rect (at -1.46 0 180) (size 1.8 2.23) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 569892EA)
    (at 141.6685 82.931 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -0.0635 -0.0635 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VAA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 567A8BCE)
    (at 144.2085 78.9305)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J22 (at 0.127 0.0635 90) (layer F.SilkS) hide)
    (fp_text value VAA (at -0.0635 4.8895 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VAA))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VAA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 567A8BE4)
    (at 149.2885 78.9305)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J23 (at 0.127 0.0635 90) (layer F.SilkS) hide)
    (fp_text value GND (at 2.3495 0.1905 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text MLAB (at 124.9045 105.283) (layer B.Cu))
  (gr_text 2016 (at 125.1585 105.4735) (layer F.SilkS))
  (gr_text BRIDGEADC01A (at 140.0175 100.9015) (layer F.SilkS))
  (gr_text KAKLIK (at 155.194 104.9655) (layer F.SilkS))
  (gr_text MLAB.CZ (at 125.2855 103.378) (layer F.SilkS))
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 164.022 94.68 90) (layer Dwgs.User))
    (feature1 (pts (xy 160.386 74.614) (xy 165.372 74.614)))
    (feature2 (pts (xy 160.386 114.746) (xy 165.372 114.746)))
    (crossbar (pts (xy 162.672 114.746) (xy 162.672 74.614)))
    (arrow1a (pts (xy 162.672 74.614) (xy 163.258421 75.740504)))
    (arrow1b (pts (xy 162.672 74.614) (xy 162.085579 75.740504)))
    (arrow2a (pts (xy 162.672 114.746) (xy 163.258421 113.619496)))
    (arrow2b (pts (xy 162.672 114.746) (xy 162.085579 113.619496)))
  )
  (dimension 40.132201 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 140.328689 71.931727 359.8186848) (layer Dwgs.User))
    (feature1 (pts (xy 160.386 74.741) (xy 160.398961 70.645234)))
    (feature2 (pts (xy 120.254 74.614) (xy 120.266961 70.518234)))
    (crossbar (pts (xy 120.258417 73.21822) (xy 160.390417 73.34522)))
    (arrow1a (pts (xy 160.390417 73.34522) (xy 159.262063 73.928073)))
    (arrow1b (pts (xy 160.390417 73.34522) (xy 159.265775 72.755237)))
    (arrow2a (pts (xy 120.258417 73.21822) (xy 121.383059 73.808203)))
    (arrow2b (pts (xy 120.258417 73.21822) (xy 121.386771 72.635367)))
  )
  (gr_text POWER (at 140.066 113.349) (layer F.SilkS))
  (gr_text Vcc (at 141.717 94.553 90) (layer F.SilkS))
  (gr_text GND (at 136.637 94.553 90) (layer F.SilkS))
  (gr_text GND (at 147.686 105.729) (layer F.SilkS))
  (gr_text GND (at 132.446 105.602) (layer F.SilkS))
  (gr_text Analog|Digital (at 140.081 103.0605) (layer F.SilkS))
  (gr_line (start 120.254 74.614) (end 120.254 114.746) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.386 74.614) (end 120.254 74.614) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.386 114.746) (end 160.386 74.614) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.254 114.746) (end 160.386 114.746) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 69.28) (xy 165.72 69.28) (xy 165.72 115) (xy 120 115)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.64 74.614) (xy 160.64 115.254) (xy 119.746 115.254) (xy 120.127 74.487)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 129.54 76.009473) (xy 150.988 76.011) (xy 150.988 87.915922) (xy 141.9225 96.9645) (xy 134.5565 96.9645)
        (xy 134.5565 101.993214) (xy 140.081 101.965253) (xy 140.081 112.649) (xy 129.54 112.649) (xy 129.54 103.713526)
        (xy 125.73 100.039947) (xy 125.73 85.628763) (xy 129.54 81.618954)
      )
    )
  )
  (zone (net 4) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 125.6665 100.203) (xy 125.6665 85.6615) (xy 129.477434 81.559855) (xy 129.47553 75.93873) (xy 151.765 75.95348)
        (xy 151.765 87.503) (xy 141.605 97.2185) (xy 135.255 97.2185) (xy 135.255 102.2985) (xy 140.0175 102.2985)
        (xy 140.0175 113.6015) (xy 130.556 113.6015) (xy 130.556 104.9655)
      )
    )
  )
)
