(kicad_pcb (version 4) (host pcbnew 0.201509061501+6161~29~ubuntu15.04.1-product)
  (general
    (links 74)
    (no_connects 0)
    (area -8.636 -44.958 40.132001 6.032501)
    (thickness 1.6)
    (drawings 26)
    (tracks 147)
    (zones 0)
    (modules 33)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 VCC)
  (net 5 "Net-(J3-Pad2)")
  (net 6 /CA0)
  (net 7 /CA1)
  (net 8 /SDA)
  (net 9 /SCL)
  (net 10 "Net-(P1-Pad1)")
  (net 11 "Net-(P2-Pad1)")
  (net 12 "Net-(C5-Pad2)")
  (net 13 "Net-(J4-Pad2)")
  (net 14 "Net-(C8-Pad2)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /CA0)
    (add_net /CA1)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net VCC)
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.844 -16.256 180)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.652 -16.256 180)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.59 -24.13 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 19.05 -24.13 270)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 55485D51)
    (at 8.128 -20.574 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0.127 0.0635 180) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 54BBE081)
    (at 15.748 -18.542 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 2.54 180) (layer B.SilkS))
    (fp_text value BAT46 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 180) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.75006 0 180) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 54BBE081)
    (at 15.748 -21.336)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 2.54) (layer B.SilkS))
    (fp_text value BAT46 (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOT-23 (layer B.Cu) (tedit 55DD869B)
    (at 7.493 -28.956 90)
    (tags SOT23)
    (fp_text reference D4 (at 1.99898 0.09906 360) (layer B.SilkS))
    (fp_text value LM4041-adj (at 0.0635 0 90) (layer B.SilkS) hide)
    (pad 3 smd rect (at 0 1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C8-Pad2)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 554851D4)
    (at 5.08 -12.954)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C5-Pad2)"))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C5-Pad2)"))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 21.336 -21.082 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J3-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 25.146 -26.924 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /CA0))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 25.146 -29.464 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /CA1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 5549D8AD)
    (at 15.24 -35.4965 270)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J7 (at 0 -7.62 270) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 0 7.62 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA))
    (pad 4 thru_hole rect (at 1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA))
    (pad 5 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC))
    (pad 6 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC))
    (pad 7 thru_hole rect (at -1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCL))
    (pad 8 thru_hole rect (at 1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCL))
    (pad 9 thru_hole rect (at -1.27 5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole rect (at 1.27 5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55485B08)
    (at 18.288 -7.874 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P1 (at -4.826 -3.556 90) (layer F.SilkS) hide)
    (fp_text value _ (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad1)"))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55485B0A)
    (at 13.208 -7.874 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P2 (at -4.826 -3.556 90) (layer F.SilkS) hide)
    (fp_text value _ (at 0.254 4.064 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad1)"))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 18.288 -15.24 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.208 -15.24 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 6.604 -24.384 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 3K3 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 16.764 -30.988 180)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /SDA))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.2715 -30.988)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 /SCL))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-10-1EP_3x3mm_Pitch0.5mm (layer B.Cu) (tedit 55485DE4)
    (at 15.4305 -26.162 90)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 0.0635 90) (layer B.SilkS))
    (fp_text value LTC2485 (at 0 -2.575 90) (layer B.Fab))
    (pad 1 smd rect (at -1.55 1 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at -1.55 0.5 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 3 smd rect (at -1.55 0 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at -1.55 -0.5 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 5 smd rect (at -1.55 -1 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at 1.55 -1 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /SCL))
    (pad 7 smd rect (at 1.55 -0.5 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /SDA))
    (pad 8 smd rect (at 1.55 0 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 1.55 0.5 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /CA1))
    (pad 10 smd rect (at 1.55 1 90) (size 0.65 0.3) (layers B.Cu B.Paste B.Mask)
      (net 6 /CA0))
    (pad 11 smd rect (at 0.3875 -0.62 90) (size 0.775 1.24) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at 0.3875 0.62 90) (size 0.775 1.24) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.3875 -0.62 90) (size 0.775 1.24) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (pad 11 smd rect (at -0.3875 0.62 90) (size 0.775 1.24) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 554851CF)
    (at 3.8735 -27.305)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J4 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCC))
    (pad 2 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C8-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 21.336 -28.194 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 55DD86A3)
    (at 3.048 -21.082 90)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value BLM21PG300SN1D (at 0.127 -0.381 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 4.953 -17.907 180)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.525 -23.622 180)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.398 -10.16 90)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.398 -26.543 90)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 22nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.652 -13.97)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 20.7772 -39.0652) (layer F.SilkS))
  (gr_text "ADR. 0x24" (at 10.541 -19.304) (layer F.SilkS))
  (gr_text GND (at 19.05 -28.194 90) (layer F.SilkS))
  (gr_text I2CADC01A (at 27.686 -14.478 90) (layer B.Cu))
  (gr_text MLAB.CZ (at 25.4 -14.732 90) (layer B.Cu))
  (gr_text POWER (at 1.524 -12.954 90) (layer F.SilkS))
  (gr_text I2CADC01A (at 27.178 -14.478 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 24.892 -14.478 90) (layer F.SilkS))
  (gr_text IN+ (at 22.098 -8.128 90) (layer F.SilkS))
  (gr_text IN- (at 9.398 -8.128 90) (layer F.SilkS))
  (gr_text VCC (at 3.81 -22.098) (layer F.SilkS))
  (gr_text REF+ (at 1.524 -27.432 90) (layer F.SilkS))
  (gr_text Vref (at 5.588 -29.718) (layer F.SilkS))
  (gr_text CA1 (at 23.749 -31.75) (layer F.SilkS))
  (gr_text GND (at 26.416 -21.844) (layer F.SilkS))
  (gr_text VCC (at 28.956 -28.194 90) (layer F.SilkS))
  (gr_text CA0 (at 23.749 -24.384) (layer F.SilkS))
  (gr_text REF- (at 18.288 -21.59) (layer F.SilkS))
  (gr_text SDA (at 17.78 -31.496) (layer F.SilkS))
  (gr_text VDD (at 15.24 -39.116) (layer F.SilkS))
  (gr_text SCL (at 12.7 -31.496) (layer F.SilkS))
  (gr_text GND (at 10.16 -39.116) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.226 -0.254) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.226 -40.386) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -40.386) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.667 -41.656) (xy 33.528 -41.656) (xy 32.9565 2.667) (xy -3.81 1.778)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.7945 -44.958) (xy 40.132 -44.7675) (xy 38.5445 6.0325) (xy -8.636 5.207)
      )
    )
  )
)
