(kicad_pcb (version 4) (host pcbnew 0.201503110816+5502~22~ubuntu14.10.1-product)
  (general
    (links 43)
    (no_connects 0)
    (area 104.4448 30.8356 164.109401 63.017401)
    (thickness 1.6)
    (drawings 18)
    (tracks 76)
    (zones 0)
    (modules 22)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 102.3366 65.7098)
    (grid_origin 102.3366 65.7098)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x01060_80000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +1.8V)
  (net 4 /GPIO199)
  (net 5 /GPIO200)
  (net 6 /GPIO204)
  (net 7 /UART_TX)
  (net 8 /UART_RX)
  (net 9 /SCLK)
  (net 10 /MISO)
  (net 11 "Net-(J10-Pad1)")
  (net 12 "Net-(J11-Pad3)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.15)
    (trace_width 0.3)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /GPIO199)
    (add_net /GPIO200)
    (add_net /GPIO204)
    (add_net /MISO)
    (add_net /SCLK)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad3)")
  )
  (net_class Power ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +1.8V)
    (add_net +5V)
    (add_net GND)
  )
  (module MLAB_hreb:2mm_Pin_Header_Straight_2x04 (layer F.Cu) (tedit 55007440)
    (at 146.3166 54.9498 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at -0.2952 -5.4228 180) (layer F.SilkS))
    (fp_text value IOS_PORT_#1 (at 0 5.334 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1 -3 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 +1.8V))
    (pad 2 thru_hole rect (at 1 -3 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO199))
    (pad 3 thru_hole rect (at -1 -1 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 /UART_RX))
    (pad 4 thru_hole rect (at 1 -1 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO200))
    (pad 5 thru_hole rect (at -1 1 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 /UART_TX))
    (pad 6 thru_hole rect (at 1 1 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO204))
    (pad 7 thru_hole rect (at -1 3 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 8 thru_hole rect (at 1 3 90) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7874 0.7874 0.7874))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 55005C2F)
    (at 138.684 56.1086 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C2 (at -0.20066 3.29946 180) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.59918 180) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 +1.8V))
    (model Capacitors_Tantalum_SMD/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5472F1F7)
    (at 137.668 40.005)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value GPIO199 (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO199))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /GPIO199))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5472F1F7)
    (at 142.748 40.005)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at 0 -3.81) (layer F.SilkS))
    (fp_text value GPIO200 (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO200))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GPIO200))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5472F1F7)
    (at 147.828 40.005)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS))
    (fp_text value GPIO204 (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO204))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 /GPIO204))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5472F1F7)
    (at 140.208 40.005)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS))
    (fp_text value UART_RX (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 /UART_RX))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 /UART_RX))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 5472F1F7)
    (at 145.288 40.005)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J8 (at 0 -3.81) (layer F.SilkS))
    (fp_text value UART_TX (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 /UART_TX))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 /UART_TX))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 55007496)
    (at 118.0846 40.0558)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J9 (at -1.2192 -3.6322) (layer F.SilkS))
    (fp_text value SCLK (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCLK))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCLK))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 550074A7)
    (at 120.6246 40.0558)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J10 (at -1.1176 -3.6576) (layer F.SilkS))
    (fp_text value MOSI (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J10-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J10-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:2mm_Pin_Header_Straight_2x02 (layer F.Cu) (tedit 550074DF)
    (at 117.8166 54.9498)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J11 (at 4.2558 0.0412) (layer F.SilkS))
    (fp_text value IO_PORT_#2 (at 0 3.302) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1 -1) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCLK))
    (pad 2 thru_hole rect (at 1 -1) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J10-Pad1)"))
    (pad 3 thru_hole rect (at -1 1) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J11-Pad3)"))
    (pad 4 thru_hole rect (at 1 1) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MISO))
    (model Pin_Headers/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.7874 0.7874 0.7874))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 550074AC)
    (at 125.7046 40.0558)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J12 (at 0.381 -3.5052) (layer F.SilkS))
    (fp_text value "#SS" (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J11-Pad3)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J11-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_hreb:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 550074AA)
    (at 123.1646 40.0558)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J13 (at -0.4318 -3.5052) (layer F.SilkS))
    (fp_text value MISO (at 0 0) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MISO))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MISO))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_dira:MountingHole_3mm placed (layer F.Cu) (tedit 55007470)
    (at 153.1366 40.1098)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference J14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M3 (at 1 5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_dira:MountingHole_3mm placed (layer F.Cu) (tedit 5500745C)
    (at 112.4966 40.1098)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference J15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M3 (at 1 5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_dira:MountingHole_3mm placed (layer F.Cu) (tedit 55007468)
    (at 153.3166 55.5498)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference J16 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M3 (at 1 5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_dira:MountingHole_3mm placed (layer F.Cu) (tedit 55007453)
    (at 112.3166 55.5498)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference J17 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M3 (at 1 5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_dira:MountingHole_3mm placed (layer F.Cu) (tedit 5500748A)
    (at 132.8166 50.2698)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference J18 (at 0 0) (layer F.SilkS) hide)
    (fp_text value M3 (at 1 5) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Diodes_SMD:Diode-SMA_Standard (layer B.Cu) (tedit 5403E41A)
    (at 124.2568 56.8706 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Diodes_SMD/Diode-SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:Diode-MiniMELF_Standard (layer B.Cu) (tedit 55005B0E)
    (at 126.0856 47.1932 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 +1.8V))
    (model Diodes_SMD/Diode-MiniMELF_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Reflow (layer B.Cu) (tedit 55005C2F)
    (at 128.4224 57.4294 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C1 (at -0.20066 3.29946 90) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936 90) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Capacitors_Tantalum_SMD/TantalC_SizeB_EIA-3528_Reflow.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55007572)
    (at 153.1366 47.4218 270)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value "5V POWER" (at 0 5.08 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 4 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 5 thru_hole rect (at -1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 550060C5)
    (at 131.6736 41.5798 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J5 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value "1,8V CPU Core" (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 +1.8V))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 +1.8V))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text GPIO200 (at 142.8496 47.6758 90) (layer F.SilkS))
  (gr_text "ODROID-U3 MLAB BREAKOUT BOARD" (at 132.3086 59.436) (layer F.SilkS))
  (gr_text "MLAB\n2015" (at 112.4712 47.8028) (layer F.SilkS))
  (gr_text +5V (at 152.6286 51.4858) (layer F.SilkS))
  (gr_text POWER (at 153.1874 44.0436) (layer F.SilkS))
  (gr_text GPIO204 (at 147.9296 47.6758 90) (layer F.SilkS))
  (gr_text TX (at 145.3896 44.3738 90) (layer F.SilkS))
  (gr_text RX (at 140.3096 44.5008 90) (layer F.SilkS))
  (gr_text GPIO199 (at 137.7696 47.8028 90) (layer F.SilkS))
  (gr_text 1.8V (at 131.5466 36.4998) (layer F.SilkS))
  (gr_text "#SS\n" (at 125.7046 45.5168 90) (layer F.SilkS))
  (gr_text MISO (at 123.2916 46.0248 90) (layer F.SilkS))
  (gr_text MOSI (at 120.6246 46.0248 90) (layer F.SilkS))
  (gr_text SCLK (at 118.0846 46.0248 90) (layer F.SilkS))
  (gr_line (start 107.6726 35.2858) (end 157.9606 35.2858) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.9606 61.0616) (end 157.9606 35.2858) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.6726 61.0616) (end 157.9606 61.0616) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.6726 35.2858) (end 107.6726 61.0616) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.3846 30.8356) (xy 163.4998 30.8356) (xy 164.1094 62.3062) (xy 130.7338 63.0174) (xy 104.4448 62.6364)
      )
    )
  )
)
