(kicad_pcb (version 4) (host pcbnew 0.201509201831+6203~30~ubuntu15.04.1-product)
  (general
    (links 176)
    (no_connects 0)
    (area 22.501453 9.768615 79.568853 105.526616)
    (thickness 1.6)
    (drawings 30)
    (tracks 669)
    (zones 0)
    (modules 80)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.15)
    (zone_clearance 0.35)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.5)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C4-Pad1)")
  (net 9 "Net-(C5-Pad1)")
  (net 10 "Net-(C5-Pad2)")
  (net 11 "Net-(C6-Pad1)")
  (net 12 "Net-(C6-Pad2)")
  (net 13 "Net-(C7-Pad1)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C8-Pad1)")
  (net 16 "Net-(C8-Pad2)")
  (net 17 "Net-(C9-Pad1)")
  (net 18 "Net-(C9-Pad2)")
  (net 19 "Net-(C10-Pad1)")
  (net 20 "Net-(C10-Pad2)")
  (net 21 GNDA)
  (net 22 +5V)
  (net 23 /AINR-)
  (net 24 /AINR+)
  (net 25 /AINL+)
  (net 26 /AINL-)
  (net 27 DGND)
  (net 28 +3.3V)
  (net 29 /VMIO)
  (net 30 /VREF)
  (net 31 /AVDD/2)
  (net 32 "Net-(D1-Pad2)")
  (net 33 /MSO)
  (net 34 /AUDIOF1)
  (net 35 /OSR1)
  (net 36 /OSR0)
  (net 37 /AUDIOF0)
  (net 38 /BCLK)
  (net 39 /LRCLK)
  (net 40 /DOUT)
  (net 41 /MCLK)
  (net 42 /VCC)
  (net 43 "Net-(J4-Pad2)")
  (net 44 /VCC1)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.15)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.5)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /AINL+)
    (add_net /AINL-)
    (add_net /AINR+)
    (add_net /AINR-)
    (add_net /AUDIOF0)
    (add_net /AUDIOF1)
    (add_net /AVDD/2)
    (add_net /BCLK)
    (add_net /DOUT)
    (add_net /LRCLK)
    (add_net /MCLK)
    (add_net /MSO)
    (add_net /OSR0)
    (add_net /OSR1)
    (add_net /VCC)
    (add_net /VCC1)
    (add_net /VMIO)
    (add_net /VREF)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J4-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.889)
    (via_drill 0.5)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3.3V)
    (add_net +5V)
    (add_net DGND)
    (add_net GNDA)
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 549148B6)
    (at 65.043253 77.078615 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C1 (at -0.127 -0.127 270) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 270) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 450) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 549148B0)
    (at 60.725253 77.078615 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C2 (at -0.127 -0.127 270) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 270) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 450) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54914894)
    (at 43.326253 76.951615 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C3 (at -0.254 -0.127 270) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 270) (layer B.SilkS) hide)
    (fp_text user + (at 3.63982 -6.08838 450) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54914896)
    (at 38.881253 76.951615 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C4 (at -0.254 -0.127 270) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 270) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 450) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C4-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 62.757253 69.077615 180)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 470p (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.040253 69.204615 180)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 470p (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 69.615253 61.330615 270)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180p (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 55.518253 62.600615 270)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180p (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 48.533253 61.330615 270)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180p (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C9-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.674253 62.092615 270)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180p (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 5491488F)
    (at 36.976253 52.186615 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C11 (at -0.381 0.127 90) (layer B.SilkS))
    (fp_text value 47u (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 44 /VCC1))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 54914711)
    (at 57.931253 53.075615 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C12 (at -0.127 0.127 90) (layer B.SilkS))
    (fp_text value 47u (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 42 /VCC))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 36.468253 57.774615 180)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 44 /VCC1))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 58.693253 58.409615)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 /VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 63.011253 52.694615 180)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2n2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /AINR-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /AINR+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.548253 52.313615 180)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2n2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /AINL+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /AINL-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 54.248253 38.089615 90)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 4U7 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.167253 26.278615 90)
    (attr smd)
    (fp_text reference C18 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10n (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 40.532253 40.502615 270)
    (attr smd)
    (fp_text reference C19 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 4u7 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 65.744293 41.213815 90)
    (attr smd)
    (fp_text reference C20 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 549148BE)
    (at 68.599253 40.248615 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C21 (at -0.127 -0.127 90) (layer B.SilkS))
    (fp_text value 47u (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 65.424253 48.122615 270)
    (attr smd)
    (fp_text reference C22 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 549148BB)
    (at 68.599253 50.789615 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C23 (at 0 0.127 270) (layer B.SilkS))
    (fp_text value 47u (at -0.09906 -3.59918 270) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 270) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at -2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54914889)
    (at 46.628253 55.488615)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C24 (at 0 0.254) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 29 /VMIO))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 5491471B)
    (at 52.978253 47.487615 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C25 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 180) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 360) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 30 /VREF))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 549148F0)
    (at 57.931253 34.025615 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C26 (at 0 0.127 270) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 270) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 450) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 1 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54914732)
    (at 46.628253 51.424615)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C27 (at 0 -0.127) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 29 /VMIO))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54914718)
    (at 52.978253 51.551615 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C28 (at 0 0.254 180) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 180) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 360) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 30 /VREF))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 5491472E)
    (at 46.628253 47.360615)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C29 (at 0 0.127) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 29 /VMIO))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54914715)
    (at 52.978253 55.615615 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C30 (at 0 -0.127 180) (layer B.SilkS))
    (fp_text value 10u (at 0.254 -3.556 180) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 360) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 30 /VREF))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 48.152253 69.839615 270)
    (attr smd)
    (fp_text reference C31 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 51.581253 43.931615)
    (attr smd)
    (fp_text reference C32 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /VREF))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 47.176893 44.429455 180)
    (attr smd)
    (fp_text reference C33 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100n (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /VMIO))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 549148AC)
    (at 53.232253 70.982615 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C34 (at 0.127 0 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.254 -3.556 90) (layer B.SilkS) hide)
    (fp_text user + (at 3.59918 -2.49936 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.5494 0 270) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 1 smd rect (at 1.5494 0 270) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_D:Diode-SMA_Standard (layer B.Cu) (tedit 549148CF)
    (at 61.233253 28.564615 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0.127 -0.127 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D1-Pad2)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x04 placed (layer F.Cu) (tedit 547B59AF)
    (at 57.550253 84.444615)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at -1.905 9.144) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 1.27 0) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at -3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (pad 2 thru_hole rect (at -1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 thru_hole rect (at 3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (pad 5 thru_hole rect (at 3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (pad 7 thru_hole rect (at -1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 8 thru_hole rect (at -3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x04 placed (layer F.Cu) (tedit 547B59B2)
    (at 46.247253 84.444615)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at -0.889 7.62) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 1.27 0) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad1)"))
    (pad 1 thru_hole rect (at -3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (pad 2 thru_hole rect (at -1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C4-Pad1)"))
    (pad 4 thru_hole rect (at 3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (pad 5 thru_hole rect (at 3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (pad 7 thru_hole rect (at -1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C4-Pad1)"))
    (pad 8 thru_hole rect (at -3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 21 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 547B59BF)
    (at 66.821253 31.993615 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at 5.969 -11.557 270) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(D1-Pad2)"))
    (pad 3 thru_hole rect (at 2.54 1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 4 thru_hole rect (at 2.54 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 5 thru_hole rect (at 0 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(D1-Pad2)"))
    (pad 6 thru_hole rect (at -2.54 -1.27 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x04 placed (layer F.Cu) (tedit 547B59B6)
    (at 36.595253 35.041615 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J5 (at 1.397 -12.7 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 1.27 0 90) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 1.27 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 38 /BCLK))
    (pad 6 thru_hole rect (at 1.27 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 38 /BCLK))
    (pad 1 thru_hole rect (at -3.81 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 39 /LRCLK))
    (pad 2 thru_hole rect (at -1.27 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 40 /DOUT))
    (pad 4 thru_hole rect (at 3.81 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MCLK))
    (pad 5 thru_hole rect (at 3.81 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MCLK))
    (pad 7 thru_hole rect (at -1.27 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 40 /DOUT))
    (pad 8 thru_hole rect (at -3.81 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 39 /LRCLK))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 547B59BC)
    (at 48.660253 23.357615 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at 2.413 7.366 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_5X2 (at 1.27 0 180) (layer F.SilkS) hide)
    (pad 9 thru_hole rect (at -2.54 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 36 /OSR0))
    (pad 5 thru_hole rect (at 5.08 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 27 DGND))
    (pad 3 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 6 thru_hole rect (at 5.08 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 33 /MSO))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 2 thru_hole rect (at -2.54 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 4 thru_hole rect (at 2.54 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (pad 10 thru_hole rect (at -5.08 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 35 /OSR1))
    (pad 7 thru_hole rect (at 2.54 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 37 /AUDIOF0))
    (pad 8 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 34 /AUDIOF1))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 549148F6)
    (at 61.995253 45.074615 270)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value BLM21PG300SN1D (at 1.651 -1.397 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 64.027253 72.125615 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 61.614253 72.168795 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 42.437253 72.252615 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.770253 72.252615 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C4-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 64.662253 66.791615 180)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 60.852253 66.791615)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 42.945253 66.791615 180)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.135253 66.791615)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 63.265253 58.663615 180)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.802253 58.663615 180)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 67.710253 61.330615 270)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 57.804253 62.600615 270)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 5479E823)
    (at 46.374253 61.330615 270)
    (attr smd)
    (fp_text reference R13 (at 0.127 0.381 270) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C9-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.960253 62.092615 270)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54914917)
    (at 64.154253 55.615615 270)
    (attr smd)
    (fp_text reference R15 (at 0 0 270) (layer B.SilkS))
    (fp_text value 22R (at 0.127 -0.381 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /AINR-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54914919)
    (at 61.809833 55.539415 270)
    (attr smd)
    (fp_text reference R16 (at 0.0762 -0.05842 270) (layer B.SilkS))
    (fp_text value 22R (at 0.127 -0.381 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /AINR+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 42.846193 55.508935 270)
    (attr smd)
    (fp_text reference R17 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 22R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /AINL+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C9-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 40.303653 55.508935 270)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 22R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /AINL-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 44.088253 27.294615)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 33 /MSO))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 47.771253 27.802615 90)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 /AUDIOF0))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 49.803253 27.802615 90)
    (attr smd)
    (fp_text reference R21 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 /AUDIOF1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 52.597253 27.802615 90)
    (attr smd)
    (fp_text reference R22 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 36 /OSR0))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 54.375253 27.802615 90)
    (attr smd)
    (fp_text reference R23 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 35 /OSR1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 50.184253 66.410615 270)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 50.184253 69.839615 270)
    (attr smd)
    (fp_text reference R25 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /AVDD/2))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SO-8 (layer B.Cu) (tedit 5479A0C5)
    (at 62.884253 62.600615 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 270) (layer B.SilkS))
    (fp_text value LT6231CS (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C7-Pad1)"))
    (pad 2 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 3 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (pad 4 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 5 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C5-Pad2)"))
    (pad 6 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C8-Pad2)"))
    (pad 7 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C8-Pad1)"))
    (pad 8 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 42 /VCC))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SO-8 (layer B.Cu) (tedit 5479A0C5)
    (at 41.167253 62.473615 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U2 (at 0 0 270) (layer B.SilkS))
    (fp_text value LT6231CS (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C9-Pad1)"))
    (pad 2 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C9-Pad2)"))
    (pad 3 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C6-Pad1)"))
    (pad 4 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 5 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C6-Pad2)"))
    (pad 6 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C10-Pad2)"))
    (pad 7 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C10-Pad1)"))
    (pad 8 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 44 /VCC1))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SO-8 (layer B.Cu) (tedit 5479A0C5)
    (at 60.979253 40.248615 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U4 (at 0 0 90) (layer B.SilkS))
    (fp_text value LE33CD (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.905 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 2 smd oval (at -0.635 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 3 smd oval (at 0.635 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 4 smd oval (at 1.905 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd oval (at 1.905 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 6 smd oval (at 0.635 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 7 smd oval (at -0.635 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 8 smd oval (at -1.905 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_L:FIR1 (layer B.Cu) (tedit 549148CB)
    (at 61.868253 35.041615 270)
    (fp_text reference F1 (at 0 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at -15.748 3.302 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 36.468253 23.357615 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0.1778 -0.0762 90) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 27 DGND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 66.948253 23.357615 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0.1778 -0.0762 90) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 27 DGND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 66.948253 84.317615 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.1778 -0.0762 90) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 36.468253 84.317615 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0.1778 -0.0762 90) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module MLAB_IO:SSOP-20_5.3x7.2mm_Pitch0.65mm (layer B.Cu) (tedit 5491492B)
    (at 47.136253 38.280115)
    (descr "20-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0.127 -0.9525) (layer B.SilkS))
    (fp_text value WM8786 (at 1.778 -5.0165) (layer B.SilkS) hide)
    (pad 1 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 25 /AINL+))
    (pad 2 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 26 /AINL-))
    (pad 3 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 4 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 5 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 GNDA))
    (pad 6 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 39 /LRCLK))
    (pad 7 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 40 /DOUT))
    (pad 8 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 38 /BCLK))
    (pad 9 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 41 /MCLK))
    (pad 10 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 /MSO))
    (pad 11 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 37 /AUDIOF0))
    (pad 12 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 34 /AUDIOF1))
    (pad 13 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 36 /OSR0))
    (pad 14 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 /OSR1))
    (pad 15 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
    (pad 16 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 17 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 29 /VMIO))
    (pad 18 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 30 /VREF))
    (pad 19 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 /AINR-))
    (pad 20 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers B.Cu B.Paste B.Mask)
      (net 24 /AINR+))
    (model Housings_SSOP/SSOP-20_5.3x7.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.801253 54.218615 270)
    (attr smd)
    (fp_text reference R26 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 44 /VCC1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 54.883253 59.044615)
    (attr smd)
    (fp_text reference R27 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 /VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x01 placed (layer F.Cu) (tedit 547B59B8)
    (at 36.595253 28.691615 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at 2.921 -10.795 90) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 DGND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module graphics:qrcode (layer F.Cu) (tedit 54E667CA)
    (at 51.454253 66.918615 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Mlab_Xtal:ASFL1 (layer B.Cu) (tedit 55BEF5A0)
    (at 42.799 31.242 270)
    (fp_text reference X1 (at 0 2.794 270) (layer B.SilkS))
    (fp_text value ASFL1-24.576MHZ-EK (at 0 -2.794 270) (layer B.SilkS) hide)
    (fp_text user * (at -1.7399 -1.1938 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.27 -1.1 270) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 1.27 -1.1 270) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 27 DGND))
    (pad 3 smd rect (at 1.27 1.1 270) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 41 /MCLK))
    (pad 4 smd rect (at -1.27 1.1 270) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 28 +3.3V))
  )
  (dimension 70.612 (width 0.3) (layer Dwgs.User)
    (gr_text "2,7800 in" (at 78.7438 53.848 90) (layer Dwgs.User))
    (feature1 (pts (xy 71.7804 18.542) (xy 80.0938 18.542)))
    (feature2 (pts (xy 71.7804 89.154) (xy 80.0938 89.154)))
    (crossbar (pts (xy 77.3938 89.154) (xy 77.3938 18.542)))
    (arrow1a (pts (xy 77.3938 18.542) (xy 77.980221 19.668504)))
    (arrow1b (pts (xy 77.3938 18.542) (xy 76.807379 19.668504)))
    (arrow2a (pts (xy 77.3938 89.154) (xy 77.980221 88.027496)))
    (arrow2b (pts (xy 77.3938 89.154) (xy 76.807379 88.027496)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 51.7144 13.255) (layer Dwgs.User))
    (feature1 (pts (xy 71.7804 18.542) (xy 71.7804 11.905)))
    (feature2 (pts (xy 31.6484 18.542) (xy 31.6484 11.905)))
    (crossbar (pts (xy 31.6484 14.605) (xy 71.7804 14.605)))
    (arrow1a (pts (xy 71.7804 14.605) (xy 70.653896 15.191421)))
    (arrow1b (pts (xy 71.7804 14.605) (xy 70.653896 14.018579)))
    (arrow2a (pts (xy 31.6484 14.605) (xy 32.774904 15.191421)))
    (arrow2b (pts (xy 31.6484 14.605) (xy 32.774904 14.018579)))
  )
  (gr_text LRCLK (at 39.516253 38.851615 180) (layer F.SilkS))
  (gr_text + (at 56.280253 80.761615 90) (layer F.SilkS))
  (gr_text - (at 58.947253 80.761615 90) (layer F.SilkS))
  (gr_text - (at 45.231253 80.634615 270) (layer F.SilkS))
  (gr_text + (at 47.771253 80.507615 270) (layer F.SilkS))
  (gr_text ADCaudio01B (at 69.742253 74.411615 90) (layer B.Cu))
  (gr_text MLAB.CZ (at 33.420253 76.697615 90) (layer B.Cu))
  (gr_text ADCaudio01B (at 52.343253 49.392615 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 48.914253 49.646615 90) (layer F.SilkS))
  (gr_text "KAKLIK, JACHO 2015" (at 69.996253 70.347615 90) (layer F.SilkS))
  (gr_text ENCLK (at 32.912253 25.389615 90) (layer F.SilkS))
  (gr_text GND (at 48.660253 19.674615 180) (layer F.SilkS))
  (gr_text MCLK (at 39.516253 31.231615 180) (layer F.SilkS))
  (gr_text BCLK (at 39.516253 33.771615 180) (layer F.SilkS))
  (gr_text DOUT (at 39.516253 36.311615 180) (layer F.SilkS))
  (gr_text MSO (at 43.580253 26.278615 90) (layer F.SilkS))
  (gr_text AUDIOF0 (at 46.374253 26.278615 90) (layer F.SilkS))
  (gr_text AUDIOF1 (at 48.787253 26.278615 90) (layer F.SilkS))
  (gr_text OSR0 (at 51.200253 26.278615 90) (layer F.SilkS))
  (gr_text OSR1 (at 53.867253 26.278615 90) (layer F.SilkS))
  (gr_text +5V (at 70.377253 31.993615 90) (layer F.SilkS))
  (gr_text POWER (at 63.011253 31.993615 90) (layer F.SilkS))
  (gr_text "AUDIO L" (at 46.120253 88.000615 180) (layer F.SilkS))
  (gr_text "AUDIO R" (at 57.649313 87.878695 180) (layer F.SilkS))
  (gr_line (start 71.772253 89.141615) (end 31.644253 89.141615) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.772253 89.141615) (end 71.772253 18.533615) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.772253 18.533615) (end 31.644253 18.533615) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31.644253 89.141615) (end 31.644253 18.533615) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 27) (net_name DGND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.568253 38.978615) (xy 71.774253 45.328615) (xy 58.439253 45.328615) (xy 58.820253 45.328615) (xy 52.343253 38.978615)
        (xy 47.644253 38.978615) (xy 47.644253 38.216615) (xy 47.644253 38.216615) (xy 45.612253 38.216615) (xy 44.723253 38.216615)
        (xy 44.723253 38.216615) (xy 39.262253 38.216615) (xy 39.262253 40.756615) (xy 29.356253 40.756615) (xy 31.115 16.764)
        (xy 72.517 15.875)
      )
    )
  )
  (zone (net 27) (net_name DGND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.060253 43.804615) (xy 71.774253 45.328615) (xy 58.693253 45.328615) (xy 52.216253 38.978615) (xy 47.644253 38.978615)
        (xy 47.644253 38.216615) (xy 47.644253 38.216615) (xy 46.501253 38.216615) (xy 40.278253 38.216615) (xy 40.278253 40.121615)
        (xy 36.976253 43.423615) (xy 29.737253 43.423615) (xy 30.48 15.875) (xy 73.025 17.018)
      )
    )
  )
  (zone (net 21) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 73.171253 90.413615) (xy 72.282253 45.328615) (xy 58.820253 45.328615) (xy 52.343253 38.978615) (xy 47.644253 38.978615)
        (xy 47.644253 38.851615) (xy 47.644253 38.343615) (xy 46.628253 38.343615) (xy 46.628253 38.343615) (xy 45.739253 38.343615)
        (xy 42.818253 38.343615) (xy 39.389253 38.343615) (xy 39.389253 40.883615) (xy 29.356253 40.883615) (xy 29.337 90.424)
      )
    )
  )
  (zone (net 21) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.092253 90.540615) (xy 72.282253 45.328615) (xy 58.947253 45.328615) (xy 52.470253 38.851615) (xy 47.517253 38.851615)
        (xy 47.517253 38.343615) (xy 47.517253 38.343615) (xy 46.755253 38.343615) (xy 40.405253 38.343615) (xy 40.405253 40.121615)
        (xy 37.103253 43.423615) (xy 31.261253 43.423615) (xy 30.607 92.075)
      )
    )
  )
)
