(kicad_pcb (version 4) (host pcbnew 0.201510140731+6267~30~ubuntu15.04.1-product)
  (general
    (links 174)
    (no_connects 0)
    (area -0.635 -68.89 123.875715 1.016001)
    (thickness 1.6)
    (drawings 6)
    (tracks 746)
    (zones 0)
    (modules 69)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00000_80000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror true)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_DOC/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 +3V3)
  (net 5 "Net-(C5-Pad1)")
  (net 6 VCC)
  (net 7 "Net-(C10-Pad2)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C11-Pad2)")
  (net 10 "Net-(C12-Pad1)")
  (net 11 "Net-(C15-Pad1)")
  (net 12 "Net-(C15-Pad2)")
  (net 13 "Net-(C16-Pad1)")
  (net 14 "Net-(C16-Pad2)")
  (net 15 "Net-(C17-Pad1)")
  (net 16 "Net-(C17-Pad2)")
  (net 17 "Net-(C18-Pad1)")
  (net 18 "Net-(C18-Pad2)")
  (net 19 "Net-(C19-Pad1)")
  (net 20 "Net-(C19-Pad2)")
  (net 21 "Net-(C20-Pad1)")
  (net 22 "Net-(C20-Pad2)")
  (net 23 "Net-(J1-Pad2)")
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J4-Pad1)")
  (net 26 "Net-(J5-Pad1)")
  (net 27 "Net-(J6-Pad1)")
  (net 28 "Net-(J7-Pad1)")
  (net 29 "Net-(J8-Pad1)")
  (net 30 "Net-(J9-Pad1)")
  (net 31 "Net-(J10-Pad1)")
  (net 32 "Net-(J11-Pad2)")
  (net 33 "Net-(J15-Pad1)")
  (net 34 "Net-(J15-Pad3)")
  (net 35 "Net-(J16-Pad1)")
  (net 36 "Net-(J16-Pad3)")
  (net 37 "Net-(L2-Pad1)")
  (net 38 "Net-(L4-Pad1)")
  (net 39 VDD)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J15-Pad3)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J16-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net VDD)
  )
  (net_class Power3v3 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (net_class Power_path ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(L4-Pad1)")
    (add_net VCC)
  )
  (module Mlab_Pin_Headers:Straight_2x02 (layer F.Cu) (tedit 560404C7)
    (at 7.4295 -20.6375)
    (descr "pin header straight 2x02")
    (tags "pin header straight 2x02")
    (fp_text reference J16 (at -4.7625 0.4445) (layer F.SilkS) hide)
    (fp_text value OUT4 (at 0.0635 3.8735) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J16-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J16-Pad1)"))
    (pad 3 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J16-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J16-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x02 (layer F.Cu) (tedit 5454C210)
    (at 41.6 -5.7 90)
    (descr "pin header straight 2x02")
    (tags "pin header straight 2x02")
    (fp_text reference J15 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value OUT3 (at 0 3.81 90) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J15-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J15-Pad1)"))
    (pad 3 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J15-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J15-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5604056E)
    (at 7.4295 -37.1475 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value RESET (at -0.0635 5.9055 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C12-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C12-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 39.6 -40.5)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SA (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J11-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 VDD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 560404EE)
    (at 7.4295 -29.5275 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -4.7625 180) (layer F.SilkS) hide)
    (fp_text value BICKI (at 0 5.3975 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J10-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J10-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 560404DB)
    (at 7.4295 -26.9875 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at -0.1905 -4.0005 180) (layer F.SilkS) hide)
    (fp_text value XTI (at -0.0635 4.3815 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J9-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J9-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56040538)
    (at 7.4295 -32.0675 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at -0.0635 -4.1275 180) (layer F.SilkS) hide)
    (fp_text value LRCKI (at -0.0635 5.7785 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J8-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J8-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5604053F)
    (at 7.4295 -34.6075 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at -0.3175 -4.2545 180) (layer F.SilkS) hide)
    (fp_text value SDI (at -0.0635 4.5085 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J7-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J7-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56040568)
    (at 7.4295 -44.7675 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SCL (at -0.0635 4.7625 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J6-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J6-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5604055D)
    (at 7.4295 -42.2275 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SDA (at 0 4.6355 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J5-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J5-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56040553)
    (at 7.4295 -39.6875 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value INT_LINE (at -0.1905 7.1755 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J4-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J4-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 560404D3)
    (at 7.4295 -24.4475 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -4.0005 180) (layer F.SilkS) hide)
    (fp_text value PWRDN (at 0.0635 6.6675 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J3-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J3-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 5454C210)
    (at 16.407 -51.077 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J2 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value "DIGITAL POWER" (at 0 5.08 90) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 5454C210)
    (at 42.6 -17.24 180)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J1 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value CONFIG (at 0 5.08 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -2.54 180) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 VDD))
    (pad 2 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_WAGO_256_RM5mm_1pol (layer F.Cu) (tedit 54BBE4E3)
    (at 81.738 -38.088 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J20 (at -8.686 -0.242 270) (layer F.SilkS))
    (fp_text value OUT2A (at 14.301 -0.369 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C19-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C19-Pad2)"))
  )
  (module Terminal_Blocks:TerminalBlock_WAGO_256_RM5mm_1pol (layer F.Cu) (tedit 54BBE4E3)
    (at 81.738 -43.088 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J19 (at -8.686 0.219 270) (layer F.SilkS))
    (fp_text value OUT2B (at 14.301 -0.035 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C20-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C20-Pad2)"))
  )
  (module Terminal_Blocks:TerminalBlock_WAGO_256_RM5mm_1pol (layer F.Cu) (tedit 54BBE4E3)
    (at 81.738 -23.088 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J18 (at -8.686 0.026 270) (layer F.SilkS))
    (fp_text value OUT1B (at 14.174 -0.482 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C18-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C18-Pad2)"))
  )
  (module Terminal_Blocks:TerminalBlock_WAGO_256_RM5mm_1pol (layer F.Cu) (tedit 54BBE4E3)
    (at 81.738 -18.088 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J17 (at -8.686 -0.181 270) (layer F.SilkS))
    (fp_text value OUT1A (at 14.428 -0.308 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C17-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C17-Pad2)"))
  )
  (module Terminal_Blocks:TerminalBlock_WAGO_256_RM5mm_1pol (layer F.Cu) (tedit 54BBE4E3)
    (at 81.75 -28.1 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J13 (at -8.674 -0.162 270) (layer F.SilkS))
    (fp_text value -VS (at 13.17 -0.414 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Terminal_Blocks:TerminalBlock_WAGO_256_RM5mm_1pol (layer F.Cu) (tedit 54BBE4E3)
    (at 81.75 -33.1 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J12 (at -8.547 -0.207 270) (layer F.SilkS))
    (fp_text value +VS (at 13.158 0.52 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
  )
  (module Power_Packages_SMD:PowerSSO-36 placed (layer B.Cu) (tedit 56029F5A)
    (at 32.512 -30.3658 180)
    (descr http://www.icbuy.com/education/package/mode_name/upload/education/package/061104/1157210448562001162612641.pdf)
    (fp_text reference U1 (at 0 -8.455 180) (layer B.SilkS))
    (fp_text value STA350BW (at 0 8.455 180) (layer B.SilkS))
    (pad 1 smd rect (at -6.8625 5.525 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -6.8625 4.875 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J11-Pad2)"))
    (pad 3 smd rect (at -6.8625 4.225 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -6.8625 3.575 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (pad 5 smd rect (at -6.8625 2.925 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 6 smd rect (at -6.8625 2.275 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(L4-Pad1)"))
    (pad 7 smd rect (at -6.8625 1.625 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -6.8625 0.975 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 9 smd rect (at -6.8625 0.325 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C16-Pad1)"))
    (pad 10 smd rect (at -6.8625 -0.325 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(L2-Pad1)"))
    (pad 11 smd rect (at -6.8625 -0.975 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 12 smd rect (at -6.8625 -1.625 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -6.8625 -2.275 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 14 smd rect (at -6.8625 -2.925 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 15 smd rect (at -6.8625 -3.575 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 39 VDD))
    (pad 16 smd rect (at -6.8625 -4.225 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J1-Pad2)"))
    (pad 17 smd rect (at -6.8625 -4.875 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J15-Pad3)"))
    (pad 18 smd rect (at -6.8625 -5.525 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J15-Pad1)"))
    (pad 36 smd rect (at 6.8625 5.525 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 35 smd rect (at 6.8625 4.875 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 34 smd rect (at 6.8625 4.225 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J6-Pad1)"))
    (pad 33 smd rect (at 6.8625 3.575 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J5-Pad1)"))
    (pad 32 smd rect (at 6.8625 2.925 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J4-Pad1)"))
    (pad 31 smd rect (at 6.8625 2.275 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 30 smd rect (at 6.8625 1.625 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J7-Pad1)"))
    (pad 29 smd rect (at 6.8625 0.975 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J8-Pad1)"))
    (pad 28 smd rect (at 6.8625 0.325 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J10-Pad1)"))
    (pad 27 smd rect (at 6.8625 -0.325 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J9-Pad1)"))
    (pad 26 smd rect (at 6.8625 -0.975 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 6.8625 -1.625 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 24 smd rect (at 6.8625 -2.275 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 23 smd rect (at 6.8625 -2.925 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (pad 22 smd rect (at 6.8625 -3.575 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 21 smd rect (at 6.8625 -4.225 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 20 smd rect (at 6.8625 -4.875 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J16-Pad1)"))
    (pad 19 smd rect (at 6.8625 -5.525 180) (size 1.125 0.46) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J16-Pad3)"))
    (pad 37 smd rect (at 0 0 180) (size 6.3 9.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 37 thru_hole rect (at -2.65 4.25 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (pad 37 thru_hole rect (at 2.65 4.25 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 4.25 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 0 4.25 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 4.25 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 2.833334 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 2.65 2.833334 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -2.65 2.833334 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (pad 37 thru_hole rect (at 0 2.833334 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 2.833334 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 0 1.416668 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 2.65 1.416668 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 1.416668 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 0.000002 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 2.65 0.000002 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 0 0.000002 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 0.000002 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 1.416668 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -2.65 1.416668 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -2.65 0.000002 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 2.65 -4.249996 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 2.65 -1.416664 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 -2.83333 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 2.65 -2.83333 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 -1.416664 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 1.325 -4.249996 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -2.65 -2.83333 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 -1.416664 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 0 -2.83333 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 0 -1.416664 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 -2.83333 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -2.65 -1.416664 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -2.65 -4.249996 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at -1.325 -4.249996 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
    (pad 37 thru_hole rect (at 0 -4.249996 180) (size 1 1) (drill 0.75) (layers *.Cu)
      (net 2 GND))
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5415CFA7)
    (at 68.453 -45.7835 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 2.3 180) (layer B.SilkS))
    (fp_text value 4R7 (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(C20-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5415CFA7)
    (at 68.3155 -43.1165 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 2.3 180) (layer B.SilkS))
    (fp_text value 4R7 (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C19-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5415CFA7)
    (at 68.58 -17.2085 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 2.3 180) (layer B.SilkS))
    (fp_text value 4R7 (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5415CFA7)
    (at 68.58 -14.4145 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 2.3 180) (layer B.SilkS))
    (fp_text value 4R7 (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5415CFA7)
    (at 46.99 -45.974 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 2.3 90) (layer B.SilkS))
    (fp_text value 20 (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C16-Pad2)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(L4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5415CFA7)
    (at 47.5615 -18.4785 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 2.3 90) (layer B.SilkS))
    (fp_text value 20 (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(L2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 3.175 -37.084)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.778) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 22.6695 -26.858 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 2R2 (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 3.241 -42.164)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 13.782 -28.1305 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 2k2 (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 3.302 -44.704)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 86.36 -55.88)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 86.36 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -55.88)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h6mm (layer B.Cu) (tedit 556FDB7E)
    (at 56.388 -51.689)
    (descr "Choke, SMD, 12x12mm 6mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L4 (at 0 8.89) (layer B.SilkS))
    (fp_text value 15uH (at 0 -8.89) (layer B.Fab))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(L4-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C20-Pad2)"))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h6mm (layer B.Cu) (tedit 556FDB7E)
    (at 56.388 -37.5073)
    (descr "Choke, SMD, 12x12mm 6mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L3 (at 0 8.89) (layer B.SilkS))
    (fp_text value 15uH (at 0 -8.89) (layer B.Fab))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C19-Pad2)"))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h6mm (layer B.Cu) (tedit 556FDB7E)
    (at 56.388 -23.3257)
    (descr "Choke, SMD, 12x12mm 6mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L2 (at 0 8.89) (layer B.SilkS))
    (fp_text value 15uH (at 0 -8.89) (layer B.Fab))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h6mm (layer B.Cu) (tedit 556FDB7E)
    (at 56.388 -9.144)
    (descr "Choke, SMD, 12x12mm 6mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L1 (at 0 8.89) (layer B.SilkS))
    (fp_text value 15uH (at 0 -8.89) (layer B.Fab))
    (pad 1 smd rect (at -4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 4.95046 0) (size 2.90068 5.40004) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C17-Pad2)"))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer B.Cu) (tedit 552FF239)
    (at 17.042 -45.87)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81) (layer B.SilkS))
    (fp_text value M4 (at 0 -4.3) (layer B.Fab))
    (fp_text user K (at -2.9 -2.95) (layer B.SilkS))
    (fp_text user A (at 2.9 -2.9) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 75.819 -40.513 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C27 (at 0 0.127 90) (layer B.SilkS))
    (fp_text value 680nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C19-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 87.769 -30.6 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C26 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 75.565 -20.574 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C25 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 680nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C17-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 68.437 -48.26 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C24 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(C20-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 68.5165 -40.386 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C19-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 68.5005 -19.812 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 68.453 -11.557 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 65.024 -48.514 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 65.278 -39.878 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 65.024 -20.32 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 65.151 -10.795 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 46.9265 -40.894 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 330p (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C16-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 47.498 -13.6365 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 330p (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5415D7BD)
    (at 45.974 -30.353 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 0 2.3 270) (layer B.SilkS))
    (fp_text value 1uF/35V (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 5415D7BD)
    (at 68.453 -30.734 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at 0 2.3 270) (layer B.SilkS))
    (fp_text value 1uF/35V (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 11.938 -38.1 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 1nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 43 -39.4 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 43.053 -23.495 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 39 VDD))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 42.799 -29.083)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 42.799 -31.623)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 23.114 -37.211 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D12.5_L25_P5 (layer F.Cu) (tedit 0)
    (at 48.26 -32.813 270)
    (descr "Radial Electrolytic Capacitor Diameter 12.5mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C6 (at 2.5 -7.6 270) (layer F.SilkS))
    (fp_text value 1000uF/35V (at 2.5 7.6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D12.5_L25_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 19.812 -28.956 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 19.8755 -24.765 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 17.145 -27.305 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 680p (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 16.915 -41.933)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.1) (layer B.SilkS))
    (fp_text value 22uF/6.3V (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 13.6525 -25.9715)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMB_Handsoldering (layer B.Cu) (tedit 552FF2F0)
    (at 72.39 -30.734 270)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 0 3.1 270) (layer B.SilkS))
    (fp_text value M4 (at 0.1 -4.75 270) (layer B.Fab))
    (fp_text user K (at -3.5 -3.1 270) (layer B.SilkS))
    (fp_text user A (at 3 -3.05 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.70002 0 270) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 2.70002 0 270) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (dimension 60.96 (width 0.3) (layer Dwgs.User)
    (gr_text "2,4000 in" (at 118.19 -30.48 90) (layer Dwgs.User))
    (feature1 (pts (xy 111.76 -60.96) (xy 119.54 -60.96)))
    (feature2 (pts (xy 111.76 0) (xy 119.54 0)))
    (crossbar (pts (xy 116.84 0) (xy 116.84 -60.96)))
    (arrow1a (pts (xy 116.84 -60.96) (xy 117.426421 -59.833496)))
    (arrow1b (pts (xy 116.84 -60.96) (xy 116.253579 -59.833496)))
    (arrow2a (pts (xy 116.84 0) (xy 117.426421 -1.126504)))
    (arrow2b (pts (xy 116.84 0) (xy 116.253579 -1.126504)))
  )
  (dimension 111.76 (width 0.3) (layer Dwgs.User)
    (gr_text "4,4000 in" (at 55.88 -67.39) (layer Dwgs.User))
    (feature1 (pts (xy 111.76 -60.96) (xy 111.76 -68.74)))
    (feature2 (pts (xy 0 -60.96) (xy 0 -68.74)))
    (crossbar (pts (xy 0 -66.04) (xy 111.76 -66.04)))
    (arrow1a (pts (xy 111.76 -66.04) (xy 110.633496 -65.453579)))
    (arrow1b (pts (xy 111.76 -66.04) (xy 110.633496 -66.626421)))
    (arrow2a (pts (xy 0 -66.04) (xy 1.126504 -65.453579)))
    (arrow2b (pts (xy 0 -66.04) (xy 1.126504 -66.626421)))
  )
  (gr_line (start 91.44 -60.96) (end 91.44 0) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0 -60.96) (end 91.44 -60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0 0) (end 0 -60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0 0) (end 91.44 0) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.381 -61.468) (xy 112.014 -61.341) (xy 112.141 0.381) (xy -0.381 0.254)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.508 -61.595) (xy 112.268 -61.595) (xy 112.268 0.508) (xy -0.635 1.016)
      )
    )
  )
  (zone (net 6) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.481 -32.512) (xy 42.672 -32.512) (xy 42.672 -27.813) (xy 38.608 -27.813) (xy 38.608 -32.512)
      )
    )
  )
  (zone (net 20) (net_name "Net-(C19-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 59.563 -40.513) (xy 63.5 -40.513) (xy 63.881 -39.751) (xy 71.247 -39.497) (xy 73.406 -40.767)
        (xy 86.36 -40.64) (xy 86.36 -35.814) (xy 76.073 -35.941) (xy 65.278 -35.941) (xy 63.627 -34.417)
        (xy 59.563 -34.417)
      )
    )
  )
  (zone (net 22) (net_name "Net-(C20-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 59.817 -54.483) (xy 69.723 -54.483) (xy 77.597 -46.609) (xy 86.36 -46.609) (xy 86.36 -41.021)
        (xy 74.676 -41.021) (xy 74.676 -44.196) (xy 70.358 -48.768) (xy 59.817 -48.768)
      )
    )
  )
  (zone (net 6) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 86.741 -35.433) (xy 65.532 -35.433) (xy 64.008 -33.909) (xy 45.085 -33.909) (xy 45.085 -31.242)
        (xy 47.625 -31.242) (xy 47.879 -30.988) (xy 86.614 -30.988)
      )
    )
  )
  (zone (net 16) (net_name "Net-(C17-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 59.182 -12.7) (xy 59.182 -5.715) (xy 69.215 -5.715) (xy 77.724 -14.224) (xy 86.36 -14.347371)
        (xy 86.36 -20.193) (xy 74.168 -20.193) (xy 74.168 -15.494) (xy 69.025512 -10.234638) (xy 63.5 -10.287)
        (xy 63.5 -12.7)
      )
    )
  )
  (zone (net 18) (net_name "Net-(C18-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 86.36 -25.4) (xy 86.36 -20.574) (xy 73.787 -20.574) (xy 73.279 -21.082) (xy 64.008 -21.082)
        (xy 63.5 -20.447) (xy 59.563 -20.447) (xy 59.563 -26.416) (xy 63.933701 -26.416) (xy 64.754817 -25.341484)
      )
    )
  )
  (zone (net 38) (net_name "Net-(L4-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 48.006 -46.609) (xy 49.403 -46.609) (xy 53.34 -48.768) (xy 53.34 -54.991) (xy 49.022 -54.991)
        (xy 43.942 -45.72) (xy 43.942 -37.338) (xy 40.64 -34.163) (xy 41.656 -33.02) (xy 46.609 -37.973)
        (xy 46.609 -45.212)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C16-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 53.086 -40.386) (xy 53.086 -34.29) (xy 45.847 -34.29) (xy 43.053 -31.75) (xy 42.037 -32.766)
        (xy 47.752 -38.481) (xy 49.784 -38.481) (xy 49.784 -40.386)
      )
    )
  )
  (zone (net 37) (net_name "Net-(L2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 43.053 -28.448) (xy 44.704 -28.448) (xy 46.795765 -26.416) (xy 53.213 -26.416) (xy 53.213 -20.193)
        (xy 50.292 -20.193) (xy 49.149 -19.304) (xy 46.609 -19.177) (xy 46.609 -24.166871) (xy 43.780364 -27.178)
        (xy 42.291 -27.178) (xy 42.291 -28.448)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C15-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 53.34 -6.096) (xy 53.34 -11.938) (xy 50.419 -11.938) (xy 46.482 -15.875) (xy 46.482 -24.277319)
        (xy 43.561 -27.432) (xy 41.402 -27.432) (xy 41.402 -25.146) (xy 43.688 -25.146) (xy 44.196 -24.638)
        (xy 44.196 -11.926095) (xy 50.038 -6.096)
      )
    )
  )
)
