(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 62)
    (no_connects 0)
    (area -8.659285 -46.736 50.315286 7.620001)
    (thickness 1.6)
    (drawings 29)
    (tracks 146)
    (zones 0)
    (modules 31)
    (nets 31)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 GNDA)
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J3-Pad2)")
  (net 9 "Net-(J4-Pad1)")
  (net 10 "Net-(J4-Pad2)")
  (net 11 "Net-(J5-Pad1)")
  (net 12 "Net-(J5-Pad2)")
  (net 13 "Net-(J6-Pad1)")
  (net 14 "Net-(J6-Pad2)")
  (net 15 /AIN-)
  (net 16 /AIN+)
  (net 17 /BIN-)
  (net 18 /BIN+)
  (net 19 /AOUT-)
  (net 20 /AOUT+)
  (net 21 /BOUT-)
  (net 22 /BOUT+)
  (net 23 /B2+)
  (net 24 /B2-)
  (net 25 /A2+)
  (net 26 /A2-)
  (net 27 /B3+)
  (net 28 /B3-)
  (net 29 /A3+)
  (net 30 /A3-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /A2+)
    (add_net /A2-)
    (add_net /A3+)
    (add_net /A3-)
    (add_net /AIN+)
    (add_net /AIN-)
    (add_net /AOUT+)
    (add_net /AOUT-)
    (add_net /B2+)
    (add_net /B2-)
    (add_net /B3+)
    (add_net /B3-)
    (add_net /BIN+)
    (add_net /BIN-)
    (add_net /BOUT+)
    (add_net /BOUT-)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
  )
  (module Mlab_TR:H110X_H1121_HX1188 (layer B.Cu) (tedit 5890279D)
    (at 26.924 -20.32 90)
    (fp_text reference TR1 (at 0 -0.5 90) (layer B.SilkS))
    (fp_text value H1102NL (at 0 0.5 90) (layer B.Fab))
    (pad 1 smd rect (at -4.46 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 29 /A3+))
    (pad 2 smd rect (at -3.19 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 3 smd rect (at -1.92 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 30 /A3-))
    (pad 4 smd rect (at -0.635 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0.635 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 1.92 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 27 /B3+))
    (pad 7 smd rect (at 3.19 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J4-Pad1)"))
    (pad 8 smd rect (at 4.46 -3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 28 /B3-))
    (pad 9 smd rect (at 4.46 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 21 /BOUT-))
    (pad 10 smd rect (at 3.19 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J6-Pad1)"))
    (pad 11 smd rect (at 1.92 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 22 /BOUT+))
    (pad 12 smd rect (at 0.635 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at -0.635 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at -1.92 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 19 /AOUT-))
    (pad 15 smd rect (at -3.19 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (pad 16 smd rect (at -4.46 3.64 90) (size 0.76 2.92) (layers B.Cu B.Paste B.Mask)
      (net 20 /AOUT+))
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 10.5156 -27.1272 180)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /B2-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /BIN-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 14.3764 -25.908 90)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /B2+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /B2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 17.9705 -27.1272 180)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 /B3-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /B2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 placed (layer F.Cu) (tedit 5890279D)
    (at 5.08 -25.908)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J2 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value HEADER_2x04_PARALLEL (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /BIN-))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /BIN-))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /BIN+))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /BIN+))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 placed (layer F.Cu) (tedit 5890279D)
    (at 36.576 -14.732)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J7 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value HEADER_2x04_PARALLEL (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /AOUT-))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /AOUT-))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /AOUT+))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /AOUT+))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 placed (layer F.Cu) (tedit 5890279D)
    (at 36.576 -25.908)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J8 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value HEADER_2x04_PARALLEL (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /BOUT-))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /BOUT-))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /BOUT+))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /BOUT+))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5890279D)
    (at 35.56 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 22.86 -6.096)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 300 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 5890279D)
    (at 23.876 -10.668 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value HEADER_1x02 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J3-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J3-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 27.432 -6.096 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 300 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J5-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 26.416 -3.048 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 26.416 -37.592 90)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 17.9197 -13.462 180)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /A3+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /A2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 27.432 -34.544 180)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 300 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J6-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 10.4648 -15.9512 180)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /A2-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /AIN-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 14.3256 -14.732 90)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /A2+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /A2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 10.4648 -13.5128 180)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /A2+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /AIN+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 17.9197 -16.002 180)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /A3-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /A2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5890279D)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5890279D)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 23.876 -37.592 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 22.86 -34.544)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 300 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 5890279D)
    (at 26.416 -10.668 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value HEADER_1x02 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J5-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J5-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5890279D)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 23.876 -3.048 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 placed (layer F.Cu) (tedit 5890279D)
    (at 5.08 -14.732)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value HEADER_2x04_PARALLEL (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /AIN-))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /AIN-))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /AIN+))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /AIN+))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 10.5156 -24.6888 180)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /B2+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 /BIN+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 5890279D)
    (at 26.416 -30.48 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value HEADER_1x02 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J6-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J6-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 5890279D)
    (at 23.876 -30.48 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value HEADER_1x02 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J4-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J4-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 5890279D)
    (at 17.9705 -24.6888 180)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 /B3+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /B2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text CGND (at 25.0444 -6.5532) (layer F.SilkS))
  (gr_text CGND (at 25.0952 -34.5948) (layer F.SilkS))
  (gr_text BIAS (at 25.1968 -16.1544 90) (layer F.SilkS))
  (gr_text BIAS (at 25.2476 -24.7904 90) (layer F.SilkS))
  (gr_text 2017 (at 14.732 -4.572) (layer B.Cu))
  (gr_text MLAB.CZ (at 14.732 -7.62) (layer B.Cu))
  (gr_text "JACHO 2017" (at 16.2052 -2.8956) (layer F.SilkS))
  (gr_text MLAB.CZ (at 16.256 -21.336 90) (layer F.SilkS))
  (gr_text SYMTRANS01A (at 18.796 -20.828 90) (layer F.SilkS))
  (gr_text + (at 33.528 -24.638 180) (layer F.SilkS))
  (gr_text GND (at 8.128 -10.922) (layer F.SilkS))
  (gr_text GND (at 8.128 -18.542) (layer F.SilkS))
  (gr_text GND (at 8.128 -22.098) (layer F.SilkS))
  (gr_text GND (at 8.128 -29.718) (layer F.SilkS))
  (gr_text - (at 8.128 -16.002) (layer F.SilkS))
  (gr_text + (at 8.128 -13.462) (layer F.SilkS))
  (gr_text - (at 8.128 -27.178) (layer F.SilkS))
  (gr_text "OUT A" (at 30.48 -14.732 90) (layer F.SilkS))
  (gr_text - (at 33.528 -15.748 180) (layer F.SilkS))
  (gr_text - (at 33.528 -26.924 180) (layer F.SilkS))
  (gr_text + (at 33.528 -13.208 180) (layer F.SilkS))
  (gr_text + (at 8.128 -24.638) (layer F.SilkS))
  (gr_text "OUT B" (at 30.48 -25.908 90) (layer F.SilkS))
  (gr_text "IN A" (at 1.524 -14.732 90) (layer F.SilkS))
  (gr_text "IN B" (at 1.524 -25.908 90) (layer F.SilkS))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.386 -40.386) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 40.386 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.688 -42.672) (xy 43.18 3.048) (xy -4.064 4.064) (xy -3.048 -43.688)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.244 -45.212) (xy 47.752 5.588) (xy -8.128 7.62) (xy -7.112 -46.736)
      )
    )
  )
  (zone (net 5) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.4 1.016) (xy 25.4 -27.432) (xy 25.4 -41.656) (xy 40.64 -41.656) (xy 40.132 1.524)
      )
    )
  )
)
