(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 58)
    (no_connects 0)
    (area -6.604 -43.18 24.384001 7.112001)
    (thickness 1.6)
    (drawings 13)
    (tracks 76)
    (zones 0)
    (modules 21)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /EN)
  (net 4 /OUT)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /EN)
    (add_net /OUT)
    (add_net GND)
    (add_net VCC)
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 14.224 -26.416 90)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.272 -25.4)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 12.192 -15.748)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55DC1460)
    (at 3.556 -14.732)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55DC1460)
    (at 3.556 -26.416)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J3 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /OUT))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /OUT))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 15.24 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 15.24 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.128 -24.4475 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.0645 -21.336)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value R (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_XTAL:ASFL1 (layer B.Cu) (tedit 57D290C2)
    (at 14.224 -20.828 180)
    (fp_text reference X1 (at 0 2.794 180) (layer B.SilkS) hide)
    (fp_text value "ASFL1, ASFLK" (at 0 -2.794 180) (layer B.SilkS) hide)
    (fp_text user * (at -1.7399 -1.1938 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.27 -1.1 180) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 1.27 -1.1 180) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.27 1.1 180) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -1.27 1.1 180) (size 1.7 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:CFPS-72,73 (layer B.Cu) (tedit 57D290D2)
    (at 14.224 -20.828 180)
    (tags CFPS-72,73)
    (fp_text reference X2 (at 1.1811 1.4351 180) (layer B.SilkS) hide)
    (fp_text value CFPS-72,CFPS-73 (at 1.1557 -0.254 180) (layer B.SilkS) hide)
    (fp_text user * (at -2.5781 -1.905 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -2.1 180) (size 1.8 2) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 2.54 -2.1 180) (size 1.8 2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.54 2.1 180) (size 1.8 2) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -2.54 2.1 180) (size 1.8 2) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:ISM92 (layer B.Cu) (tedit 57D290B6)
    (at 14.224 -20.828 180)
    (tags ISM92)
    (fp_text reference X3 (at 0.3048 2.7178 180) (layer B.SilkS) hide)
    (fp_text value ISM92 (at 1.5494 -2.794 180) (layer B.SilkS) hide)
    (fp_text user * (at -1.8034 -1.2065 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.45 -1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 1.45 -1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.45 1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -1.45 1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:ISM97 (layer B.Cu) (tedit 57D290DA)
    (at 14.224 -20.828 180)
    (tags ISM97)
    (fp_text reference X4 (at 0.9144 1.9177 180) (layer B.SilkS) hide)
    (fp_text value ISM97 (at 1.4351 -2.0066 180) (layer B.SilkS) hide)
    (fp_text user * (at -1.0033 -1.0033 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.3 -1 180) (size 1.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 1.3 -1 180) (size 1.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.3 1 180) (size 1.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -1.3 1 180) (size 1.4 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:I533_1534_1733_1734 (layer B.Cu) (tedit 57D290C9)
    (at 14.224 -20.828 180)
    (tags I533/1534/1733/1734)
    (fp_text reference X6 (at 0.254 0.5334 180) (layer B.SilkS) hide)
    (fp_text value I533_I534_I733_I734_Series (at 0.889 -3.1496 180) (layer B.SilkS) hide)
    (fp_text user * (at -1.7653 -1.2827 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 -1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 2 -1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2 1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -2 1.25 180) (size 1.6 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:ISM81 (layer B.Cu) (tedit 57D290CE)
    (at 14.224 -20.828 180)
    (tags ISM81)
    (fp_text reference X7 (at -0.127 1.5113 180) (layer B.SilkS) hide)
    (fp_text value ISM81 (at 0.6096 -0.635 180) (layer B.SilkS) hide)
    (fp_text user * (at -2.5781 -1.9812 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.54 -1.85 180) (size 2.4 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 2.54 -1.85 180) (size 2.4 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.54 1.85 180) (size 2.4 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -2.54 1.85 180) (size 2.4 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:ISM95 (layer B.Cu) (tedit 57D290D6)
    (at 14.224 -20.828 180)
    (tags ISM95)
    (fp_text reference X8 (at 0.9144 1.9177 180) (layer B.SilkS) hide)
    (fp_text value ISM95 (at 1.4351 -2.0066 180) (layer B.SilkS) hide)
    (fp_text user * (at -0.7493 -0.762 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.825 -0.625 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /EN))
    (pad 2 smd rect (at 0.825 -0.625 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.825 0.625 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT))
    (pad 4 smd rect (at -0.825 0.625 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
  )
  (module Mlab_XTAL:OSC-F (layer F.Cu) (tedit 57D64AB1)
    (at 13.208 -20.828 90)
    (tags OSC-F)
    (fp_text reference X9 (at 9.144 0 180) (layer F.SilkS))
    (fp_text value OSC-F (at 0.6731 1.0033 90) (layer F.SilkS) hide)
    (fp_text user * (at -9.4742 6.1087 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 3.81 90) (size 3.5 3.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 /EN))
    (pad 2 thru_hole circle (at 7.62 3.81 90) (size 3.5 3.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.62 -3.81 90) (size 3.5 3.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /OUT))
    (pad 4 thru_hole circle (at -7.62 -3.81 90) (size 3.5 3.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 3.556 -21.336 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /EN))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /EN))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:Diode-MiniMELF_Standard (layer B.Cu) (tedit 57D29160)
    (at 8.636 -17.78 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 2.54 270) (layer B.SilkS))
    (fp_text value BZV55C (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text CLKGEN02A (at 14.224 -20.32 90) (layer F.SilkS))
  (gr_text 2016 (at 10.16 -35.56 90) (layer F.SilkS))
  (gr_text JACHO (at 10.16 -5.08 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 12.192 -20.32 90) (layer F.SilkS))
  (gr_text GND (at 1.524 -31.496) (layer F.SilkS))
  (gr_text OUT (at 7.112 -25.4) (layer F.SilkS))
  (gr_text GND (at 7.112 -23.368) (layer F.SilkS))
  (gr_text EN (at 7.112 -21.336) (layer F.SilkS))
  (gr_text POWER (at 4.572 -9.652) (layer F.SilkS))
  (gr_line (start 0.254 -40.386) (end 20.066 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.066 -0.254) (end 20.066 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 20.066 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.016 -41.148) (xy 20.828 -41.148) (xy 19.304 1.524) (xy -2.032 2.032)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21.844 7.112) (xy -6.604 4.064) (xy -2.54 -42.672) (xy 24.384 -43.18)
      )
    )
  )
)
