(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 44)
    (no_connects 0)
    (area -8.128 -46.228 48.260001 7.620001)
    (thickness 1.6)
    (drawings 20)
    (tracks 188)
    (zones 0)
    (modules 21)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(D2-Pad1)")
  (net 5 /SDA)
  (net 6 /SCL)
  (net 7 /INTA)
  (net 8 "Net-(J2-Pad2)")
  (net 9 /CLK)
  (net 10 /TS)
  (net 11 "Net-(U1-Pad1)")
  (net 12 "Net-(U1-Pad2)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /CLK)
    (add_net /INTA)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TS)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net VCC)
  )
  (module Mlab_Batery:CH28-2032 locked placed (layer F.Cu) (tedit 57E3C867)
    (at 20.32 -20.32)
    (descr "Baterka 2032")
    (fp_text reference BT1 (at 0 0.5) (layer F.SilkS))
    (fp_text value CH28-2032 (at 0 -0.5) (layer F.Fab))
    (fp_text user + (at -10.4394 -0.1524) (layer F.SilkS))
    (pad 2 smd rect (at 15 0) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -15 0) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 57E3C867)
    (at 25.908 -20.828)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 57E3C867)
    (at 25.908 -18.796)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-MiniMELF_Standard placed (layer B.Cu) (tedit 57E3C867)
    (at 14.224 -30.48)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 2.54) (layer B.SilkS))
    (fp_text value BZV55C (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at 1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 placed (layer B.Cu) (tedit 57E3C867)
    (at 27.94 -35.56 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 0 270) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 270) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -2 0 270) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 placed (layer F.Cu) (tedit 57E3C867)
    (at 16.764 -35.814 270)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J1 (at 0 -7.62 270) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 0 7.62 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 270) (layer F.SilkS))
    (pad 10 thru_hole rect (at 1.27 5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole rect (at -1.27 5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole rect (at 1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL))
    (pad 7 thru_hole rect (at -1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL))
    (pad 6 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 5 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 4 thru_hole rect (at 1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SDA))
    (pad 3 thru_hole rect (at -1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SDA))
    (pad 2 thru_hole rect (at 1.27 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -1.27 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 57E3C867)
    (at 18.288 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /INTA))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 57E3C867)
    (at 15.748 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /INTA))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /INTA))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 57E3C867)
    (at 13.208 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /CLK))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /CLK))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 placed (layer F.Cu) (tedit 57E3C867)
    (at 20.828 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TS))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57E3C867)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57E3C867)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57E3C867)
    (at 35.56 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57E3C867)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 57E3C867)
    (at 27.94 -30.988 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 57E3C867)
    (at 27.432 -7.112 90)
    (fp_text reference SW1 (at 0 0 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at -3.15 2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -3.15 -2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TS))
    (pad 2 thru_hole rect (at 3.15 2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 3.15 -2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TS))
  )
  (module Mlab_XTAL:ABS07 placed (layer B.Cu) (tedit 57E3C867)
    (at 14.224 -19.304 90)
    (fp_text reference Y1 (at 0.127 0.0127 90) (layer B.SilkS))
    (fp_text value ABS07-120-32.768KHZ-T (at -0.1397 2.6035 90) (layer B.Fab) hide)
    (pad 2 smd rect (at -1.25 0 90) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U1-Pad1)"))
    (pad 1 smd rect (at 1.25 0 90) (size 1 1.8) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U1-Pad2)"))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57E3C867)
    (at 18.8595 -25.908 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57E3C867)
    (at 22.4155 -25.908)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /SDA))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57E3C867)
    (at 10.668 -4.572 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:TSSOP-10_3x3mm_Pitch0.5mm placed (layer B.Cu) (tedit 57E3C867)
    (at 19.304 -21.336)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 2.55) (layer B.SilkS))
    (fp_text value PCF85263A (at 0 -2.55) (layer B.Fab))
    (pad 10 smd rect (at 2.15 1) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 9 smd rect (at 2.15 0.5) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /INTA))
    (pad 8 smd rect (at 2.15 0) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /CLK))
    (pad 7 smd rect (at 2.15 -0.5) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL))
    (pad 6 smd rect (at 2.15 -1) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /SDA))
    (pad 5 smd rect (at -2.15 -1) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.15 -0.5) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /TS))
    (pad 3 smd rect (at -2.15 0) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at -2.15 0.5) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -2.15 1) (size 1.1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U1-Pad1)"))
    (model Housings_SSOP.3dshapes/TSSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RTC02A (at 1.524 -28.448 90) (layer B.Cu))
  (gr_text MLAB.CZ (at 1.524 -12.7 90) (layer B.Cu))
  (gr_text 2016 (at 38.608 -27.432 90) (layer F.SilkS))
  (gr_text JACHO (at 36.068 -27.432 90) (layer F.SilkS))
  (gr_text RTC02A (at 4.572 -13.716 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 2.032 -13.208 90) (layer F.SilkS))
  (gr_text GND (at 11.684 -33.02 90) (layer F.SilkS))
  (gr_text GND (at 21.844 -33.02 90) (layer F.SilkS))
  (gr_text SDA (at 19.304 -33.02 90) (layer F.SilkS))
  (gr_text VCC (at 16.764 -33.02 90) (layer F.SilkS))
  (gr_text TS (at 20.828 -7.62 90) (layer F.SilkS))
  (gr_text LED (at 18.288 -7.62 90) (layer F.SilkS))
  (gr_text INTA (at 15.748 -7.62 90) (layer F.SilkS))
  (gr_text CLK (at 13.208 -7.62 90) (layer F.SilkS))
  (gr_text GND (at 10.668 -7.62 90) (layer F.SilkS))
  (gr_text SCL (at 14.224 -33.02 90) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 40.386 -0.254) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.386 -40.386) (end 40.386 -0.254) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 40.386 -40.386) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 43.688 6.096) (xy -5.588 5.588) (xy -2.54 -43.18) (xy 45.72 -43.688)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -6.604 -45.72) (xy 48.26 -46.228) (xy 48.26 7.62) (xy -8.128 7.112)
      )
    )
  )
)
