(kicad_pcb (version 20160815) (host pcbnew no-vcs-found-7409~56~ubuntu16.04.1)
  (general
    (links 159)
    (no_connects 0)
    (area -1.016 -61.595 61.341001 1.3125)
    (thickness 1.6)
    (drawings 67)
    (tracks 1065)
    (zones 0)
    (modules 74)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 VCC)
  (net 4 /RESET)
  (net 5 "Net-(C8-Pad1)")
  (net 6 "Net-(C9-Pad1)")
  (net 7 "Net-(C10-Pad1)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 /ADC1)
  (net 10 "Net-(D2-Pad1)")
  (net 11 "Net-(D2-Pad2)")
  (net 12 "Net-(D3-Pad1)")
  (net 13 "Net-(D3-Pad2)")
  (net 14 /PWR_ON)
  (net 15 /DSR)
  (net 16 /RI)
  (net 17 /DCD)
  (net 18 /DTR)
  (net 19 /RTS)
  (net 20 /CTS)
  (net 21 /TXD)
  (net 22 /RXD)
  (net 23 /HS_DET)
  (net 24 "Net-(J13-Pad1)")
  (net 25 /GPIO01)
  (net 26 /GPIO02)
  (net 27 /GPIO03)
  (net 28 /GPIO04)
  (net 29 /SPK_N)
  (net 30 /SPK_P)
  (net 31 /HS_P)
  (net 32 /I2S_RXD)
  (net 33 /I2S_CLK)
  (net 34 /I2S_TXD)
  (net 35 /I2S_WA)
  (net 36 /MIC_BIAS1)
  (net 37 /MIC_GND1)
  (net 38 /MIC_GND2)
  (net 39 /MIC_BIAS2)
  (net 40 "Net-(J30-Pad1)")
  (net 41 /SDA)
  (net 42 /SCL)
  (net 43 "Net-(J36-Pad2)")
  (net 44 "Net-(J37-Pad2)")
  (net 45 "Net-(L1-Pad2)")
  (net 46 "Net-(Q1-PadG)")
  (net 47 "Net-(Q2-PadG)")
  (net 48 /V_BCKP)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /ADC1)
    (add_net /CTS)
    (add_net /DCD)
    (add_net /DSR)
    (add_net /DTR)
    (add_net /GPIO01)
    (add_net /GPIO02)
    (add_net /GPIO03)
    (add_net /GPIO04)
    (add_net /HS_DET)
    (add_net /HS_P)
    (add_net /I2S_CLK)
    (add_net /I2S_RXD)
    (add_net /I2S_TXD)
    (add_net /I2S_WA)
    (add_net /MIC_BIAS1)
    (add_net /MIC_BIAS2)
    (add_net /MIC_GND1)
    (add_net /MIC_GND2)
    (add_net /PWR_ON)
    (add_net /RESET)
    (add_net /RI)
    (add_net /RTS)
    (add_net /RXD)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SPK_N)
    (add_net /SPK_P)
    (add_net /TXD)
    (add_net /V_BCKP)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J30-Pad1)")
    (add_net "Net-(J36-Pad2)")
    (add_net "Net-(J37-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(Q1-PadG)")
    (add_net "Net-(Q2-PadG)")
    (add_net VCC)
  )
  (net_class ant ""
    (clearance 0.2)
    (trace_width 0.860506)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net "Net-(J13-Pad1)")
  )
  (module Mlab_C:TantalC_SizeD_Reflow placed (layer B.Cu) (tedit 586A2771)
    (at 44.704 -4.826)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C2 (at -0.20066 3.29946) (layer B.SilkS))
    (fp_text value 470uF/6.3V (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 12.954 -37.846 90)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 47pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 37.846 -6.858)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 37.846 -9.144)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 34.544 -3.556 270)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 39pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 37.338 -3.556 270)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 42.418 -30.607)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 47pF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 42.418 -34.671)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 47pF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 42.418 -32.639)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 47pF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 42.418 -27.432)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 47pF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 45.593 -28.321 270)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-MiniMELF_Standard placed (layer B.Cu) (tedit 586A2771)
    (at 13.462 -17.78 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value BZV55C-3,6V (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 9 /ADC1))
    (pad 2 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 placed (layer B.Cu) (tedit 586A2771)
    (at 38.608 -44.196)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at -2 0) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 placed (layer B.Cu) (tedit 586A2771)
    (at 38.608 -48.006)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at -2 0) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D3-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -36.83 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J1 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PWR_ON))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PWR_ON))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 586A2771)
    (at 5.08 -39.37 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /RESET))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /RESET))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -13.97 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /DSR))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /DSR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -16.51 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /RI))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /RI))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -19.05 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /DCD))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /DCD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -21.59 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /DTR))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /DTR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -24.13 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RTS))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -26.67 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /CTS))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /CTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -29.21 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /TXD))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /TXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -31.75 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /RXD))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /RXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -34.29 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 /HS_DET))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 /HS_DET))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 21.844 -48.514 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:SMA6251A13G50 placed (layer F.Cu) (tedit 586A2771)
    (at 44.45 -13.462)
    (fp_text reference J13 (at 0 4.699) (layer F.SilkS))
    (fp_text value SMA (at 0 5.1) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "Net-(J13-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -11.43 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /ADC1))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /ADC1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -41.91 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J15 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /GPIO01))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /GPIO01))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -44.45 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J16 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GPIO02))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GPIO02))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -46.99 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J17 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /GPIO03))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /GPIO03))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -49.53 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J18 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /GPIO04))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /GPIO04))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -24.892 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J19 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 /SPK_N))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 /SPK_N))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -27.432 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J20 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /SPK_P))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /SPK_P))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -29.972 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J21 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /HS_P))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /HS_P))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 49.022 -55.88 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J22 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 /I2S_RXD))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 /I2S_RXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 46.482 -55.88 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J23 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 /I2S_CLK))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 /I2S_CLK))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 43.942 -55.88 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J24 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 /I2S_TXD))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 /I2S_TXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 41.402 -55.88 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J25 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 /I2S_WA))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 /I2S_WA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -14.732 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J26 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 /MIC_BIAS1))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 /MIC_BIAS1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -17.272 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J27 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 /MIC_GND1))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 /MIC_GND1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -19.812 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J28 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 /MIC_GND2))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 /MIC_GND2))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -22.352 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J29 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 /MIC_BIAS2))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 /MIC_BIAS2))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -40.386 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J30 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J30-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J30-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -37.846 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J31 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 /SDA))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 /SDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -42.926 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J32 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 /SCL))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 /SCL))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -45.466 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J33 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -35.306 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J34 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 21.844 -43.434 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J36 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J36-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /GPIO01))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 placed (layer F.Cu) (tedit 586A2771)
    (at 21.844 -45.974 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J37 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J37-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /GPIO02))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 placed (layer F.Cu) (tedit 586A2771)
    (at 23.876 -5.08 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J38 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 14.986 -34.798)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value BLM21PG300SN1 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /RESET))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(L1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -55.88)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A2771)
    (at 55.88 -55.88)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A2771)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_T:SOT-23 placed (layer B.Cu) (tedit 586A2771)
    (at 33.274 -44.196 90)
    (tags SOT23)
    (fp_text reference Q1 (at 0.1905 -1.2065 90) (layer B.SilkS))
    (fp_text value MMBF170LT1G (at 0.0635 0 90) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad S smd rect (at 0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad G smd rect (at -0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(Q1-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 placed (layer B.Cu) (tedit 586A2771)
    (at 33.274 -48.006 90)
    (tags SOT23)
    (fp_text reference Q2 (at 0 -1.2065 90) (layer B.SilkS))
    (fp_text value MMBF170LT1G (at 0.0635 0 90) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D3-Pad1)"))
    (pad S smd rect (at 0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad G smd rect (at -0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(Q2-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 13.462 -11.938 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 48 /V_BCKP))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 15.24 -30.48 90)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 48 /V_BCKP))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /PWR_ON))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 50.038 -42.672)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J30-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 50.038 -37.846)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J30-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 41 /SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 43.688 -44.196 180)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 43.688 -48.006 180)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D3-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 29.972 -44.196 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 330k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(Q1-PadG)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 29.972 -47.752 270)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 330k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(Q2-PadG)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 26.924 -43.434)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(J36-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(Q1-PadG)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 placed (layer B.Cu) (tedit 586A2771)
    (at 26.924 -45.974)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(J37-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(Q2-PadG)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 586A2771)
    (at 29.718 -55.118)
    (fp_text reference SW1 (at 0 -0.762) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PWR_ON))
    (pad 1 thru_hole rect (at -3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at -3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /PWR_ON))
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 586A2771)
    (at 16.256 -55.118)
    (fp_text reference SW2 (at 0 -0.762) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 /RESET))
    (pad 1 thru_hole rect (at -3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at -3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 /RESET))
  )
  (module Mlab_IO:LEON-G1 placed (layer B.Cu) (tedit 586A2771)
    (at 27.432 -24.892)
    (tags "GSM, LEON-G1")
    (fp_text reference U1 (at 0.0889 2.7432) (layer B.SilkS))
    (fp_text value LEON100 (at 0.0254 -1.6764) (layer B.Fab))
    (pad 1 smd trapezoid (at -9.35 13.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at -9.35 12.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 48 /V_BCKP))
    (pad 3 smd trapezoid (at -9.35 11) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd trapezoid (at -9.35 9.9) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd trapezoid (at -9.35 8.8) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 /ADC1))
    (pad 6 smd trapezoid (at -9.35 7.7) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd trapezoid (at -9.35 6.6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd trapezoid (at -9.35 5.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd trapezoid (at -9.35 4.4) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 /DSR))
    (pad 10 smd trapezoid (at -9.35 3.3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 16 /RI))
    (pad 11 smd trapezoid (at -9.35 2.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 17 /DCD))
    (pad 12 smd trapezoid (at -9.35 1.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 /DTR))
    (pad 13 smd trapezoid (at -9.35 0) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 /RTS))
    (pad 14 smd trapezoid (at -9.35 -1.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 /CTS))
    (pad 15 smd trapezoid (at -9.35 -2.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 /TXD))
    (pad 16 smd trapezoid (at -9.35 -3.3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 22 /RXD))
    (pad 17 smd trapezoid (at -9.35 -4.4) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 18 smd trapezoid (at -9.35 -5.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 23 /HS_DET))
    (pad 19 smd trapezoid (at -9.35 -6.6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 14 /PWR_ON))
    (pad 20 smd trapezoid (at -9.35 -7.7) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 25 /GPIO01))
    (pad 21 smd trapezoid (at -9.35 -8.8) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 26 /GPIO02))
    (pad 22 smd trapezoid (at -9.35 -9.9) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(L1-Pad2)"))
    (pad 23 smd trapezoid (at -9.35 -11) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 27 /GPIO03))
    (pad 24 smd trapezoid (at -9.35 -12.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 /GPIO04))
    (pad 25 smd trapezoid (at -9.35 -13.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 26 smd trapezoid (at 9.35 -13.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 35 /I2S_WA))
    (pad 27 smd trapezoid (at 9.35 -12.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 34 /I2S_TXD))
    (pad 28 smd trapezoid (at 9.35 -11) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 /I2S_CLK))
    (pad 29 smd trapezoid (at 9.35 -9.9) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 32 /I2S_RXD))
    (pad 30 smd trapezoid (at 9.35 -8.8) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 42 /SCL))
    (pad 31 smd trapezoid (at 9.35 -7.7) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 41 /SDA))
    (pad 32 smd trapezoid (at 9.35 -6.6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 33 smd trapezoid (at 9.35 -5.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 34 smd trapezoid (at 9.35 -4.4) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 35 smd trapezoid (at 9.35 -3.3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 36 smd trapezoid (at 9.35 -2.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 37 smd trapezoid (at 9.35 -1.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 31 /HS_P))
    (pad 38 smd trapezoid (at 9.35 0) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 /SPK_P))
    (pad 39 smd trapezoid (at 9.35 1.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 /SPK_N))
    (pad 40 smd trapezoid (at 9.35 2.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 41 smd trapezoid (at 9.35 3.3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 39 /MIC_BIAS2))
    (pad 42 smd trapezoid (at 9.35 4.4) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 38 /MIC_GND2))
    (pad 43 smd trapezoid (at 9.35 5.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 /MIC_GND1))
    (pad 44 smd trapezoid (at 9.35 6.6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 /MIC_BIAS1))
    (pad 45 smd trapezoid (at 9.35 7.7) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 46 smd trapezoid (at 9.35 8.8) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 47 smd trapezoid (at 9.35 9.9) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J13-Pad1)"))
    (pad 48 smd trapezoid (at 9.35 11) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 49 smd trapezoid (at 9.35 12.1) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 50 smd trapezoid (at 9.35 13.2) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
  )
  (module Mlab_C:C_Radial_D8_L11.5_P3.5 placed (layer F.Cu) (tedit 586A2771)
    (at 12.954 -5.08)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 11.5mm, Pitch 3.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.75 -5.3) (layer F.SilkS))
    (fp_text value 1F (at 1.75 5.3) (layer F.Fab))
    (fp_text user + (at -0.0127 -1.8415) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L11.5_P3.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_CON:SIMCN-8P (layer F.Cu) (tedit 586A2771)
    (at 27.432 -24.384 90)
    (tags SIM)
    (fp_text reference J35 (at 0.1905 -1.5748 90) (layer F.SilkS))
    (fp_text value SIMCN-8P (at 0.0889 1.8923 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -12.6 3.81 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 3 smd trapezoid (at -12.6 -1.27 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 2 smd trapezoid (at -12.6 1.27 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 4 smd trapezoid (at -12.6 -3.81 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd trapezoid (at 12.6 3.81 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd trapezoid (at 12.6 1.27 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 7 smd trapezoid (at 12.6 -1.27 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 8 smd trapezoid (at 12.6 -3.81 90) (size 2 1.2) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 7.9 6 90) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.9 -6 90) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 586A2771)
    (at 31.242 -5.334 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D4 (at 0.127 0.127 90) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 2 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "2,3800 in" (at 30.48 -65.104) (layer Dwgs.User))
    (feature1 (pts (xy 60.706 -60.706) (xy 60.706 -66.454)))
    (feature2 (pts (xy 0.254 -60.706) (xy 0.254 -66.454)))
    (crossbar (pts (xy 0.254 -63.754) (xy 60.706 -63.754)))
    (arrow1a (pts (xy 60.706 -63.754) (xy 59.579496 -63.167579)))
    (arrow1b (pts (xy 60.706 -63.754) (xy 59.579496 -64.340421)))
    (arrow2a (pts (xy 0.254 -63.754) (xy 1.380504 -63.167579)))
    (arrow2b (pts (xy 0.254 -63.754) (xy 1.380504 -64.340421)))
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "2,3800 in" (at 64.596 -30.48 90) (layer Dwgs.User))
    (feature1 (pts (xy 60.706 -60.706) (xy 65.946 -60.706)))
    (feature2 (pts (xy 60.706 -0.254) (xy 65.946 -0.254)))
    (crossbar (pts (xy 63.246 -0.254) (xy 63.246 -60.706)))
    (arrow1a (pts (xy 63.246 -60.706) (xy 63.832421 -59.579496)))
    (arrow1b (pts (xy 63.246 -60.706) (xy 62.659579 -59.579496)))
    (arrow2a (pts (xy 63.246 -0.254) (xy 63.832421 -1.380504)))
    (arrow2b (pts (xy 63.246 -0.254) (xy 62.659579 -1.380504)))
  )
  (gr_text JACHO (at 54.991 -48.895) (layer B.Cu))
  (gr_text GSM01B (at 54.991 -51.181) (layer B.Cu))
  (gr_text 2016 (at 9.906 -56.007 90) (layer B.Cu))
  (gr_text MLAB (at 56.134 -10.033) (layer B.Cu))
  (gr_text SIM (at 16.891 -25.146 90) (layer F.SilkS))
  (gr_text GND (at 20.32 -50.927) (layer F.SilkS))
  (gr_text 2017 (at 44.069 -4.572) (layer F.SilkS))
  (gr_text JACHO (at 44.069 -6.731) (layer F.SilkS))
  (gr_text GSM01B (at 41.91 -34.29 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 39.624 -34.29 90) (layer F.SilkS))
  (gr_text GND (at 55.88 -47.752) (layer F.SilkS))
  (gr_text ANT (at 39.497 -13.589 90) (layer F.SilkS))
  (gr_text "MAX 5.5V" (at 23.876 -1.397) (layer F.SilkS))
  (gr_text "POWER IN" (at 23.876 -8.763) (layer F.SilkS))
  (gr_text BIAS1 (at 52.07 -15.621 90) (layer F.SilkS))
  (gr_text MIC (at 59.563 -16.002 90) (layer F.SilkS))
  (gr_text GND1 (at 49.53 -18.288 90) (layer F.SilkS))
  (gr_text MIC_GND2 (at 53.086 -19.812) (layer F.SilkS))
  (gr_text MIC_BIAS2 (at 53.086 -22.352) (layer F.SilkS))
  (gr_text SPK_N (at 53.086 -24.892) (layer F.SilkS))
  (gr_text SPK_P (at 53.086 -27.432) (layer F.SilkS))
  (gr_text HS_P (at 53.086 -29.972) (layer F.SilkS))
  (gr_text SDA (at 52.832 -37.846) (layer F.SilkS))
  (gr_text SCL (at 52.832 -42.037) (layer F.SilkS))
  (gr_text I2C (at 59.563 -40.513 90) (layer F.SilkS))
  (gr_text PWR (at 23.622 -55.118 90) (layer F.SilkS))
  (gr_text RESET (at 10.541 -55.372 90) (layer F.SilkS))
  (gr_text I2S (at 45.212 -59.436) (layer F.SilkS))
  (gr_text RXD (at 49.022 -53.086 270) (layer F.SilkS))
  (gr_text CLK (at 46.482 -53.086 270) (layer F.SilkS))
  (gr_text TXD (at 43.942 -53.086 270) (layer F.SilkS))
  (gr_text WA (at 41.402 -53.086 270) (layer F.SilkS))
  (gr_text "LED1 ON" (at 24.638 -43.434) (layer F.SilkS))
  (gr_text "LED2 ON" (at 24.638 -45.847) (layer F.SilkS))
  (gr_text GPIO02 (at 40.894 -47.244) (layer F.SilkS))
  (gr_text GPIO04 (at 7.874 -49.53) (layer F.SilkS))
  (gr_text GPIO03 (at 7.874 -46.99) (layer F.SilkS))
  (gr_text GPIO02 (at 7.874 -44.45) (layer F.SilkS))
  (gr_text GPIO01 (at 7.874 -41.91) (layer F.SilkS))
  (gr_text RESET (at 7.874 -39.37) (layer F.SilkS))
  (gr_text PWR (at 7.874 -36.83) (layer F.SilkS))
  (gr_text ADC1 (at 7.874 -34.29) (layer F.SilkS))
  (gr_text TXD (at 7.874 -29.21) (layer F.SilkS))
  (gr_text RXD (at 7.874 -31.75) (layer F.SilkS))
  (gr_text CTS (at 7.874 -26.67) (layer F.SilkS))
  (gr_text RTS (at 7.874 -24.13) (layer F.SilkS))
  (gr_text DTR (at 7.874 -21.59) (layer F.SilkS))
  (gr_text DCD (at 7.874 -19.05) (layer F.SilkS))
  (gr_text RI (at 7.874 -16.51) (layer F.SilkS))
  (gr_text DSR (at 7.874 -13.97) (layer F.SilkS))
  (gr_text ADC1 (at 7.874 -11.43) (layer F.SilkS))
  (gr_text NETWORK (at 40.894 -44.196) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -60.706) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -60.706) (end 60.706 -60.706) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.706 -0.254) (end 60.706 -60.706) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 60.706 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.127 -61.087) (xy 60.96 -60.96) (xy 60.96 0.127) (xy -0.127 0.254)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.016 -61.595) (xy 61.214 -61.341) (xy 61.341 0.381) (xy -0.508 0.635)
      )
    )
  )
)
