(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 88)
    (no_connects 0)
    (area -6.985 -50.3988 44.7792 5.588001)
    (thickness 1.6)
    (drawings 33)
    (tracks 194)
    (zones 0)
    (modules 45)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 /A0)
  (net 4 /A1)
  (net 5 /SDA)
  (net 6 /SCL)
  (net 7 "Net-(J5-Pad1)")
  (net 8 /LED0)
  (net 9 "Net-(J6-Pad2)")
  (net 10 /LED1)
  (net 11 "Net-(J7-Pad2)")
  (net 12 /LED2)
  (net 13 "Net-(J8-Pad2)")
  (net 14 /LED3)
  (net 15 "Net-(J9-Pad2)")
  (net 16 /LED4)
  (net 17 "Net-(J10-Pad2)")
  (net 18 /LED5)
  (net 19 "Net-(J11-Pad2)")
  (net 20 /LED6)
  (net 21 "Net-(J12-Pad2)")
  (net 22 /LED7)
  (net 23 "Net-(J13-Pad2)")
  (net 24 /A2)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /LED0)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LED3)
    (add_net /LED4)
    (add_net /LED5)
    (add_net /LED6)
    (add_net /LED7)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J11-Pad2)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J9-Pad2)")
    (add_net VDD)
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 5546B42E)
    (at 18.923 -4.699 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J3 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -27.305)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /LED1))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J7-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.668 -10.541 180)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 11.43 -20.193 270)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 3.55 270) (layer B.SilkS))
    (fp_text value PCA9531 (at 0 -3.55 270) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 /A0))
    (pad 2 smd rect (at -2.95 1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 /A1))
    (pad 3 smd rect (at -2.95 0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 24 /A2))
    (pad 4 smd rect (at -2.95 0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /LED0))
    (pad 5 smd rect (at -2.95 -0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 /LED1))
    (pad 6 smd rect (at -2.95 -0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 /LED2))
    (pad 7 smd rect (at -2.95 -1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /LED3))
    (pad 8 smd rect (at -2.95 -2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.95 -2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 /LED4))
    (pad 10 smd rect (at 2.95 -1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 18 /LED5))
    (pad 11 smd rect (at 2.95 -0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 20 /LED6))
    (pad 12 smd rect (at 2.95 -0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 /LED7))
    (pad 13 smd rect (at 2.95 0.325 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J5-Pad1)"))
    (pad 14 smd rect (at 2.95 0.975 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL))
    (pad 15 smd rect (at 2.95 1.625 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /SDA))
    (pad 16 smd rect (at 2.95 2.275 270) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -11.938 180)
    (attr smd)
    (fp_text reference R15 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -14.478 180)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J12-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -17.018 180)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -19.558 180)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -22.098 180)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J9-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -24.638 180)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -27.178 180)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J7-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -29.718 180)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J6-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.398 -13.97 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.716 -13.97 90)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J5-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 11.684 -13.843 90)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.208 -30.226 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /A2))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.779 -27.178)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /A2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.779 -29.464)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /A1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.779 -31.623)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /A0))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -12.065)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J21 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LED7))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LED7))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -14.605)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J20 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LED6))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LED6))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -17.145)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J19 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LED5))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LED5))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -19.685)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J18 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LED4))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LED4))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -22.225)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J17 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /LED3))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /LED3))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -24.765)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J16 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /LED2))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /LED2))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -27.305)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J15 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /LED1))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /LED1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.272 -29.845)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J14 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /LED0))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /LED0))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -12.065)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J13 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LED7))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J13-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -14.605)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J12 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LED6))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J12-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -17.145)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LED5))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J11-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -19.685)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LED4))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J10-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -22.225)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /LED3))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J9-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -24.765)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /LED2))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J8-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 23.114 -29.845)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /LED0))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J6-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 17.018 -35.56 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J5-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J5-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 5546B434)
    (at 5.08 -22.098 180)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J4 (at 0 -7.62 180) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 0 7.62 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SDA))
    (pad 4 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SDA))
    (pad 5 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 6 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 7 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL))
    (pad 8 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL))
    (pad 9 thru_hole rect (at -1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole rect (at 1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 14.478 -35.56 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /A1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 11.938 -35.56 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J1 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /A0))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 54BBE0AF)
    (at 12.827 -5.715 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81 90) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.559 -9.652 180)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 5.588 -14.097 180)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text MLAB (at 25.146 -9.144) (layer F.SilkS))
  (gr_text LED5 (at 14.224 -17.145) (layer F.SilkS))
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 38.1292 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 39.4792 -40.386)))
    (feature2 (pts (xy 30.226 -0.254) (xy 39.4792 -0.254)))
    (crossbar (pts (xy 36.7792 -0.254) (xy 36.7792 -40.386)))
    (arrow1a (pts (xy 36.7792 -40.386) (xy 37.365621 -39.259496)))
    (arrow1b (pts (xy 36.7792 -40.386) (xy 36.192779 -39.259496)))
    (arrow2a (pts (xy 36.7792 -0.254) (xy 37.365621 -1.380504)))
    (arrow2b (pts (xy 36.7792 -0.254) (xy 36.192779 -1.380504)))
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "29,972 mm" (at 15.24 -48.8988) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 30.226 -50.2488)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -50.2488)))
    (crossbar (pts (xy 0.254 -47.5488) (xy 30.226 -47.5488)))
    (arrow1a (pts (xy 30.226 -47.5488) (xy 29.099496 -46.962379)))
    (arrow1b (pts (xy 30.226 -47.5488) (xy 29.099496 -48.135221)))
    (arrow2a (pts (xy 0.254 -47.5488) (xy 1.380504 -46.962379)))
    (arrow2b (pts (xy 0.254 -47.5488) (xy 1.380504 -48.135221)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 v" (at 34.5732 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 35.9232 -40.386)))
    (feature2 (pts (xy 30.226 -0.254) (xy 35.9232 -0.254)))
    (crossbar (pts (xy 33.2232 -0.254) (xy 33.2232 -40.386)))
    (arrow1a (pts (xy 33.2232 -40.386) (xy 33.809621 -39.259496)))
    (arrow1b (pts (xy 33.2232 -40.386) (xy 32.636779 -39.259496)))
    (arrow2a (pts (xy 33.2232 -0.254) (xy 33.809621 -1.380504)))
    (arrow2b (pts (xy 33.2232 -0.254) (xy 32.636779 -1.380504)))
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "1,1800 v" (at 15.24 -44.53) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 30.226 -45.88)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -45.88)))
    (crossbar (pts (xy 0.254 -43.18) (xy 30.226 -43.18)))
    (arrow1a (pts (xy 30.226 -43.18) (xy 29.099496 -42.593579)))
    (arrow1b (pts (xy 30.226 -43.18) (xy 29.099496 -43.766421)))
    (arrow2a (pts (xy 0.254 -43.18) (xy 1.380504 -42.593579)))
    (arrow2b (pts (xy 0.254 -43.18) (xy 1.380504 -43.766421)))
  )
  (gr_text MLAB (at 4.572 -10.16) (layer B.Cu))
  (gr_text "I2CPWM\n01A" (at 4.7752 -11.684) (layer F.SilkS))
  (gr_text ":: 0x63" (at 15.875 -1.778) (layer F.SilkS))
  (gr_text "X: 0x62" (at 15.875 -3.556) (layer F.SilkS))
  (gr_text ":Y 0x61" (at 15.9512 -5.3848) (layer F.SilkS))
  (gr_text "XY 0x60" (at 15.9004 -7.2136) (layer F.SilkS))
  (gr_text ADDR. (at 12.192 -9.2964) (layer F.SilkS))
  (gr_text ADDR. (at 9.525 -36.703 90) (layer F.SilkS))
  (gr_text Y (at 14.478 -39.116) (layer F.SilkS))
  (gr_text X (at 11.938 -39.116) (layer F.SilkS))
  (gr_text "#RES" (at 19.812 -35.56 90) (layer F.SilkS))
  (gr_text GND (at 5.08 -29.972) (layer F.SilkS))
  (gr_text SDA (at 1.524 -19.558 90) (layer F.SilkS))
  (gr_text SCL (at 1.524 -24.892 90) (layer F.SilkS))
  (gr_text POWER (at 18.923 -9.525) (layer F.SilkS))
  (gr_text LED7 (at 14.224 -12.065) (layer F.SilkS))
  (gr_text LED6 (at 14.224 -14.605) (layer F.SilkS))
  (gr_text LED4 (at 14.224 -20.701) (layer F.SilkS))
  (gr_text LED0 (at 14.224 -30.988) (layer F.SilkS))
  (gr_text LED1 (at 14.224 -28.448) (layer F.SilkS))
  (gr_text LED2 (at 14.097 -25.908) (layer F.SilkS))
  (gr_text LED3 (at 14.224 -23.368) (layer F.SilkS))
  (gr_text PULL-UP (at 27.559 -20.955 90) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 30.226 -0.254) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -40.386) (end 30.226 -40.386) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.226 -0.254) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.274 -43.307) (xy 31.623 2.032) (xy -4.318 3.175) (xy -3.937 -43.307)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.35 -45.339) (xy 37.338 -45.339) (xy 35.052 4.953) (xy -6.985 5.588)
      )
    )
  )
)
