(kicad_pcb (version 4) (host pcbnew 0.201503110816+5502~22~ubuntu14.04.1-product)
  (general
    (links 65)
    (no_connects 0)
    (area -6.096 -51.0508 52.952172 3.429001)
    (thickness 1.6)
    (drawings 45)
    (tracks 136)
    (zones 0)
    (modules 22)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.4)
    (user_trace_width 0.508)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 111.125 136.525)
    (visible_elements 7FFCFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 /MISO)
  (net 4 /MOSI)
  (net 5 /SPICLK)
  (net 6 "Net-(J2-Pad3)")
  (net 7 /#SS3)
  (net 8 /#SS0)
  (net 9 /#INT)
  (net 10 /#SS1)
  (net 11 /#SS2)
  (net 12 /#RES)
  (net 13 /A1)
  (net 14 /A2)
  (net 15 /A0)
  (net 16 /SCL)
  (net 17 /SDA)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /#INT)
    (add_net /#RES)
    (add_net /#SS0)
    (add_net /#SS1)
    (add_net /#SS2)
    (add_net /#SS3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SPICLK)
    (add_net GND)
    (add_net "Net-(J2-Pad3)")
  )
  (net_class vdd ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net VDD)
  )
  (module Pin_Header_Straight_1x03:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 54730F6C)
    (at 25.4 -22.733 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 20.447 3.556 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 26.924 -6.35 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SPICLK))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /MISO))
    (pad 3 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /MOSI))
    (pad 4 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /MOSI))
    (pad 5 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /MISO))
    (pad 6 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SPICLK))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 17.018 -31.242 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /SCL))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 16.51 -13.589 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 19.304 -13.589 270)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 13.335 -31.242)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /SDA))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 13.589 -11.303)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0R (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /A0))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 20.701 -17.78 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /#RES))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 53FC49F2)
    (at 13.589 -13.716 180)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /A0))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:TSSOP-16 (layer B.Cu) (tedit 54745064)
    (at 15.1511 -19.9136)
    (attr smd)
    (fp_text reference U1 (at 0 0.7493) (layer B.SilkS))
    (fp_text value SC18IS602B (at 30.6959 -21.3614) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.27584 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 8 /#SS0))
    (pad 2 smd rect (at -1.6256 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 10 /#SS1))
    (pad 3 smd rect (at -0.97536 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /#RES))
    (pad 4 smd rect (at -0.32512 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.32512 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 3 /MISO))
    (pad 6 smd rect (at 0.97536 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 4 /MOSI))
    (pad 7 smd rect (at 1.6256 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 17 /SDA))
    (pad 8 smd rect (at 2.27584 -2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 16 /SCL))
    (pad 9 smd rect (at 2.27584 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 9 /#INT))
    (pad 10 smd rect (at 1.6256 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 11 /#SS2))
    (pad 11 smd rect (at 0.97536 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 5 /SPICLK))
    (pad 12 smd rect (at 0.32512 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 13 smd rect (at -0.32512 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 7 /#SS3))
    (pad 14 smd rect (at -0.97536 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 15 /A0))
    (pad 15 smd rect (at -1.6256 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 13 /A1))
    (pad 16 smd rect (at -2.27584 2.79908) (size 0.381 1.27) (layers B.Cu B.Paste B.Mask)
      (net 14 /A2))
    (model smd\smd_dil\tssop-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 54745060)
    (at 25.4 -13.335 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at -1.27 23.622 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 3 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 6 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x07 placed (layer F.Cu) (tedit 5474505B)
    (at 5.207 -20.574 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J3 (at -9.144 41.402 90) (layer F.SilkS) hide)
    (fp_text value JUMP_7X2 (at 5.08 0 90) (layer F.SilkS) hide)
    (pad 7 thru_hole rect (at 7.62 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 14 thru_hole rect (at -7.62 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 /#SS3))
    (pad 6 thru_hole rect (at 5.08 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 /#RES))
    (pad 12 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 9 /#INT))
    (pad 9 thru_hole rect (at 5.08 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 /#RES))
    (pad 5 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 10 /#SS1))
    (pad 3 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /#INT))
    (pad 11 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 /#SS0))
    (pad 1 thru_hole rect (at -7.62 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 /#SS3))
    (pad 2 thru_hole rect (at -5.08 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 11 /#SS2))
    (pad 4 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 /#SS0))
    (pad 10 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 10 /#SS1))
    (pad 13 thru_hole rect (at -5.08 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 11 /#SS2))
    (pad 8 thru_hole rect (at 7.62 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x07.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 5474505D)
    (at 15.24 -35.687 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J2 (at -36.322 -18.415 180) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 1.27 0 180) (layer F.SilkS) hide)
    (pad 9 thru_hole rect (at -2.54 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SCL))
    (pad 5 thru_hole rect (at 5.08 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at 0 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-Pad3)"))
    (pad 6 thru_hole rect (at 5.08 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at -2.54 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SCL))
    (pad 4 thru_hole rect (at 2.54 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SDA))
    (pad 10 thru_hole rect (at -5.08 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole rect (at 2.54 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 17 /SDA))
    (pad 8 thru_hole rect (at 0 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5475E0F9)
    (at 18.034 -28.067)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J5 (at 17.526 -0.254) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-Pad3)"))
    (pad 2 thru_hole rect (at 1.27 0.127) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5475FB9A)
    (at 12.7 -5.207 270)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at 0 -2.286 270) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A2))
    (pad 2 thru_hole rect (at 1.27 0.127 270) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5475FB96)
    (at 14.986 -5.207 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J7 (at 0 -2.286 90) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5475F96B)
    (at 11.049 -9.144 180)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /A2))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-0805 (layer B.Cu) (tedit 5475F96B)
    (at 16.129 -9.144)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /A1))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_D:Diode-MiniMELF_Standard (layer B.Cu) (tedit 547A2A5B)
    (at 20.066 -9.144 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at -0.381 2.159 90) (layer B.SilkS))
    (fp_text value BZV55C-3,6V (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 v" (at 38.307 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 39.657 -40.386)))
    (feature2 (pts (xy 30.226 -0.254) (xy 39.657 -0.254)))
    (crossbar (pts (xy 36.957 -0.254) (xy 36.957 -40.386)))
    (arrow1a (pts (xy 36.957 -40.386) (xy 37.543421 -39.259496)))
    (arrow1b (pts (xy 36.957 -40.386) (xy 36.370579 -39.259496)))
    (arrow2a (pts (xy 36.957 -0.254) (xy 37.543421 -1.380504)))
    (arrow2b (pts (xy 36.957 -0.254) (xy 36.370579 -1.380504)))
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "1,1800 v" (at 15.24 -49.229) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 30.226 -50.579)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -50.579)))
    (crossbar (pts (xy 0.254 -47.879) (xy 30.226 -47.879)))
    (arrow1a (pts (xy 30.226 -47.879) (xy 29.099496 -47.292579)))
    (arrow1b (pts (xy 30.226 -47.879) (xy 29.099496 -48.465421)))
    (arrow2a (pts (xy 0.254 -47.879) (xy 1.380504 -47.292579)))
    (arrow2b (pts (xy 0.254 -47.879) (xy 1.380504 -48.465421)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 33.989 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 35.339 -40.386)))
    (feature2 (pts (xy 30.226 -0.254) (xy 35.339 -0.254)))
    (crossbar (pts (xy 32.639 -0.254) (xy 32.639 -40.386)))
    (arrow1a (pts (xy 32.639 -40.386) (xy 33.225421 -39.259496)))
    (arrow1b (pts (xy 32.639 -40.386) (xy 32.052579 -39.259496)))
    (arrow2a (pts (xy 32.639 -0.254) (xy 33.225421 -1.380504)))
    (arrow2b (pts (xy 32.639 -0.254) (xy 32.052579 -1.380504)))
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "29,972 mm" (at 15.24 -45.165) (layer Dwgs.User))
    (feature1 (pts (xy 30.226 -40.386) (xy 30.226 -46.515)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -46.515)))
    (crossbar (pts (xy 0.254 -43.815) (xy 30.226 -43.815)))
    (arrow1a (pts (xy 30.226 -43.815) (xy 29.099496 -43.228579)))
    (arrow1b (pts (xy 30.226 -43.815) (xy 29.099496 -44.401421)))
    (arrow2a (pts (xy 0.254 -43.815) (xy 1.380504 -43.228579)))
    (arrow2b (pts (xy 0.254 -43.815) (xy 1.380504 -44.401421)))
  )
  (gr_text VCC (at 12.192 -27.94) (layer F.SilkS))
  (gr_text I2CSPI01A (at 9.398 -30.607) (layer B.Cu))
  (gr_text MLAB.CZ (at 21.844 -1.778) (layer B.Cu))
  (gr_text JACHO (at 24.638 -30.48) (layer F.SilkS))
  (gr_text 2015 (at 25.146 -28.829) (layer F.SilkS))
  (gr_text I2CSPI01A (at 20.574 -5.08 90) (layer F.SilkS))
  (gr_text MLAB.cz (at 18.796 -5.08 90) (layer F.SilkS))
  (gr_text VDD (at 21.209 -27.94) (layer F.SilkS))
  (gr_text ADDRESS (at 13.208 -18.034) (layer F.SilkS))
  (gr_text "SET ADR" (at 13.716 -8.636) (layer F.SilkS))
  (gr_text "#SS2" (at 8.255 -15.494) (layer F.SilkS))
  (gr_text GND (at 20.32 -29.718 90) (layer F.SilkS))
  (gr_text "POWER IN" (at 28.956 -13.208 90) (layer F.SilkS))
  (gr_text "#SS1" (at 8.255 -23.114) (layer F.SilkS))
  (gr_text SPI (at 28.956 -21.59 90) (layer F.SilkS))
  (gr_text "XY 0X28" (at 13.462 -11.684) (layer F.SilkS))
  (gr_text "X: 0X2A" (at 13.716 -13.208) (layer F.SilkS))
  (gr_text ":Y 0X2C" (at 13.716 -14.732) (layer F.SilkS))
  (gr_text ":: 0X2E" (at 14.224 -16.256) (layer F.SilkS))
  (gr_text Y (at 14.732 -1.524) (layer F.SilkS))
  (gr_text X (at 12.192 -1.524) (layer F.SilkS))
  (gr_text "MAX 3.6V" (at 21.844 -13.208 90) (layer F.SilkS))
  (gr_text "#SS0" (at 8.255 -20.574) (layer F.SilkS))
  (gr_text "#INT" (at 8.255 -18.034) (layer F.SilkS))
  (gr_text "#SS3" (at 8.255 -12.954) (layer F.SilkS))
  (gr_text CLK (at 19.685 -20.066) (layer F.SilkS))
  (gr_text MOSI (at 18.923 -25.146) (layer F.SilkS))
  (gr_text MISO (at 18.923 -22.733) (layer F.SilkS))
  (gr_text "#RES\n" (at 8.255 -25.654) (layer F.SilkS))
  (gr_text I2C (at 14.097 -38.989) (layer F.SilkS))
  (gr_text "GND\n" (at 8.128 -28.194) (layer F.SilkS))
  (gr_text SCL (at 17.78 -29.972 90) (layer F.SilkS))
  (gr_text SDA (at 12.7 -29.718 90) (layer F.SilkS))
  (gr_text GND (at 10.16 -29.718 90) (layer F.SilkS))
  (gr_line (start 30.224 -40.384) (end 0.256 -40.384) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.224 -0.256) (end 30.224 -40.384) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -0.256) (end 30.224 -0.256) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -40.384) (end 0.256 -0.256) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.889 -41.656) (xy 31.496 -41.656) (xy 31.623 0.508) (xy -1.651 0.635)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -5.461 -44.323) (xy -5.461034 -44.320543) (xy -5.588 -44.323)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.909 3.429) (xy -6.096 2.032) (xy -5.461034 -44.320543) (xy 33.782 -43.561)
      )
    )
  )
)
