(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 209)
    (no_connects 0)
    (area -7.239 -44.831 81.026001 4.572001)
    (thickness 1.6)
    (drawings 40)
    (tracks 826)
    (zones 0)
    (modules 94)
    (nets 69)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_7ffffffe)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 +3V3)
  (net 6 "Net-(C5-Pad1)")
  (net 7 +1V8)
  (net 8 +5V)
  (net 9 "Net-(C10-Pad1)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(D4-Pad2)")
  (net 13 "Net-(D5-Pad2)")
  (net 14 "Net-(D6-Pad2)")
  (net 15 "Net-(D7-Pad2)")
  (net 16 "Net-(D8-Pad2)")
  (net 17 "Net-(D9-Pad2)")
  (net 18 "Net-(F1-Pad1)")
  (net 19 /RES)
  (net 20 /A_TXD)
  (net 21 /A_RXD)
  (net 22 /A_RTS)
  (net 23 /A_CTS)
  (net 24 /A_DTR)
  (net 25 /A_DSR)
  (net 26 /A_DCD)
  (net 27 /A_RI)
  (net 28 /B_TXD)
  (net 29 /B_RXD)
  (net 30 /B_RTS)
  (net 31 /B_CTS)
  (net 32 /B_DTR)
  (net 33 /B_DSR)
  (net 34 /B_DCD)
  (net 35 /B_RI)
  (net 36 /C_TXD)
  (net 37 /C_RXD)
  (net 38 /C_RTS)
  (net 39 /C_CTS)
  (net 40 /C_DTR)
  (net 41 /C_DSR)
  (net 42 /C_DCD)
  (net 43 /C_RI)
  (net 44 /D_TXD)
  (net 45 /D_RXD)
  (net 46 /D_RTS)
  (net 47 /D_CTS)
  (net 48 /D_DTR)
  (net 49 /D_DSR)
  (net 50 /D_DCD)
  (net 51 /D_RI)
  (net 52 /SUSPEND)
  (net 53 "Net-(R1-Pad1)")
  (net 54 /EEDATA)
  (net 55 /EECLK)
  (net 56 /EECS)
  (net 57 "Net-(R6-Pad1)")
  (net 58 /A)
  (net 59 /B)
  (net 60 /C)
  (net 61 /D)
  (net 62 /E)
  (net 63 /F)
  (net 64 /G)
  (net 65 /H)
  (net 66 /#PWREN)
  (net 67 /D+)
  (net 68 /D-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.25)
    (add_net +1V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net /#PWREN)
    (add_net /A)
    (add_net /A_CTS)
    (add_net /A_DCD)
    (add_net /A_DSR)
    (add_net /A_DTR)
    (add_net /A_RI)
    (add_net /A_RTS)
    (add_net /A_RXD)
    (add_net /A_TXD)
    (add_net /B)
    (add_net /B_CTS)
    (add_net /B_DCD)
    (add_net /B_DSR)
    (add_net /B_DTR)
    (add_net /B_RI)
    (add_net /B_RTS)
    (add_net /B_RXD)
    (add_net /B_TXD)
    (add_net /C)
    (add_net /C_CTS)
    (add_net /C_DCD)
    (add_net /C_DSR)
    (add_net /C_DTR)
    (add_net /C_RI)
    (add_net /C_RTS)
    (add_net /C_RXD)
    (add_net /C_TXD)
    (add_net /D)
    (add_net /D+)
    (add_net /D-)
    (add_net /D_CTS)
    (add_net /D_DCD)
    (add_net /D_DSR)
    (add_net /D_DTR)
    (add_net /D_RI)
    (add_net /D_RTS)
    (add_net /D_RXD)
    (add_net /D_TXD)
    (add_net /E)
    (add_net /EECLK)
    (add_net /EECS)
    (add_net /EEDATA)
    (add_net /F)
    (add_net /G)
    (add_net /H)
    (add_net /RES)
    (add_net /SUSPEND)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R6-Pad1)")
  )
  (module Connect:USB_B (layer F.Cu) (tedit 582EB4C5)
    (at 15.24 -19.431 180)
    (descr "USB B connector")
    (tags "USB_B USB_DEV")
    (fp_text reference P1 (at 11.049 1.27 270) (layer F.SilkS))
    (fp_text value USB_B (at 4.699 1.27 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 68 /D-))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (pad 4 thru_hole circle (at 1.99898 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 1.99898 2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 67 /D+))
    (pad 5 thru_hole circle (at 4.699 7.26948 90) (size 2.70002 2.70002) (drill 2.30124) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 4.699 -4.72948 90) (size 2.70002 2.70002) (drill 2.30124) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connect.3dshapes/USB_B.wrl
      (at (xyz 0.185 -0.05 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm (layer B.Cu) (tedit 582EB878)
    (at 44.069 -25.146 270)
    (descr "64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 2.54 -1.016 360) (layer B.SilkS))
    (fp_text value FT4232HL (at 0 -7.2 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -5.7 3.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -5.7 3.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -5.7 2.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at -5.7 2.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -5.7 1.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.7 1.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R6-Pad1)"))
    (pad 7 smd rect (at -5.7 0.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 68 /D-))
    (pad 8 smd rect (at -5.7 0.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 67 /D+))
    (pad 9 smd rect (at -5.7 -0.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 10 smd rect (at -5.7 -0.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -5.7 -1.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -5.7 -1.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 13 smd rect (at -5.7 -2.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -5.7 -2.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 /RES))
    (pad 15 smd rect (at -5.7 -3.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -5.7 -3.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 20 /A_TXD))
    (pad 17 smd rect (at -3.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 21 /A_RXD))
    (pad 18 smd rect (at -3.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 22 /A_RTS))
    (pad 19 smd rect (at -2.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 23 /A_CTS))
    (pad 20 smd rect (at -2.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 21 smd rect (at -1.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 24 /A_DTR))
    (pad 22 smd rect (at -1.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 25 /A_DSR))
    (pad 23 smd rect (at -0.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 26 /A_DCD))
    (pad 24 smd rect (at -0.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 27 /A_RI))
    (pad 25 smd rect (at 0.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 0.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 /B_TXD))
    (pad 27 smd rect (at 1.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 /B_RXD))
    (pad 28 smd rect (at 1.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 30 /B_RTS))
    (pad 29 smd rect (at 2.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 31 /B_CTS))
    (pad 30 smd rect (at 2.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 32 /B_DTR))
    (pad 31 smd rect (at 3.25 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 32 smd rect (at 3.75 -5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 /B_DSR))
    (pad 33 smd rect (at 5.7 -3.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 /B_DCD))
    (pad 34 smd rect (at 5.7 -3.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 /B_RI))
    (pad 35 smd rect (at 5.7 -2.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 5.7 -2.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 52 /SUSPEND))
    (pad 37 smd rect (at 5.7 -1.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 38 smd rect (at 5.7 -1.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 36 /C_TXD))
    (pad 39 smd rect (at 5.7 -0.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 37 /C_RXD))
    (pad 40 smd rect (at 5.7 -0.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 /C_RTS))
    (pad 41 smd rect (at 5.7 0.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 39 /C_CTS))
    (pad 42 smd rect (at 5.7 0.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 43 smd rect (at 5.7 1.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 40 /C_DTR))
    (pad 44 smd rect (at 5.7 1.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 41 /C_DSR))
    (pad 45 smd rect (at 5.7 2.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 42 /C_DCD))
    (pad 46 smd rect (at 5.7 2.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 43 /C_RI))
    (pad 47 smd rect (at 5.7 3.25 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 48 smd rect (at 5.7 3.75 270) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 44 /D_TXD))
    (pad 49 smd rect (at 3.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 50 smd rect (at 3.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 51 smd rect (at 2.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 52 smd rect (at 2.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 45 /D_RXD))
    (pad 53 smd rect (at 1.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 46 /D_RTS))
    (pad 54 smd rect (at 1.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 47 /D_CTS))
    (pad 55 smd rect (at 0.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 48 /D_DTR))
    (pad 56 smd rect (at 0.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 57 smd rect (at -0.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 49 /D_DSR))
    (pad 58 smd rect (at -0.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 50 /D_DCD))
    (pad 59 smd rect (at -1.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 51 /D_RI))
    (pad 60 smd rect (at -1.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 66 /#PWREN))
    (pad 61 smd rect (at -2.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 54 /EEDATA))
    (pad 62 smd rect (at -2.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 55 /EECLK))
    (pad 63 smd rect (at -3.25 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 56 /EECS))
    (pad 64 smd rect (at -3.75 5.7 180) (size 1 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (model Housings_QFP.3dshapes/LQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 54.229 -25.7175 270)
    (attr smd)
    (fp_text reference C20 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 582EB4C5)
    (at 66.04 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 582EB4C5)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 582EB4C5)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 582EB4C5)
    (at 66.04 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 31.115 -20.5105 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 48.006 -34.7345 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 37.592 -37.084)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 27pF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 52.451 -34.7345 90)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 41.021 -37.084 180)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 27pF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 45.72 -34.7345 90)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 35.433 -19.685 180)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 50.419 -34.7345 90)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 20.701 -13.335 270)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 24.892 -13.335 90)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 27.94 -14.097)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 41.8465 -15.748 180)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 47.8155 -17.018)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 27.94 -12.065)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 51.943 -18.7325 270)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 53.0225 -32.131)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 35.433 -30.48 90)
    (attr smd)
    (fp_text reference C18 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 18.669 -19.3675 270)
    (attr smd)
    (fp_text reference C19 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 582EB4C5)
    (at 18.923 -5.842 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81 90) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 1 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 10.9855 -36.8935 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 14.1605 -36.8935 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 17.272 -36.957 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D4 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 20.447 -36.957 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D5 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D5-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 23.622 -36.957 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D6 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 26.797 -36.957 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D7 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D7-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 29.972 -36.957 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D8 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D8-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 582EB4C5)
    (at 33.147 -36.957 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D9 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:1812 (layer B.Cu) (tedit 582EB4C5)
    (at 17.145 -14.224 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F1 (at 0.13462 3.15468 270) (layer B.SilkS))
    (fp_text value 750mA (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.95 0 270) (size 1.9 3.4) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 1 smd rect (at -1.95 0 270) (size 1.9 3.4) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.182 -35.433)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RES))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /RES))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -29.083 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A_TXD))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A_TXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -26.543 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A_RXD))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A_RXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -24.003 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A_RTS))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A_RTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -21.463 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A_CTS))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A_CTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -18.923 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A_DTR))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A_DTR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -16.383 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A_DSR))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A_DSR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -13.843 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A_DCD))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A_DCD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 59.055 -11.303 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A_RI))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A_RI))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -29.083 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /B_TXD))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /B_TXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -26.543 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 /B_RXD))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 /B_RXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -24.003 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /B_RTS))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /B_RTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -21.463 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J13 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /B_CTS))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /B_CTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -18.923 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 /B_DTR))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 /B_DTR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -16.383 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J15 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 /B_DSR))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 /B_DSR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -13.843 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J16 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 /B_DCD))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 /B_DCD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 66.294 -11.303 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J17 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 /B_RI))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 /B_RI))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 49.8475 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J18 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 /C_TXD))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 /C_TXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 47.3075 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J19 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 /C_RXD))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 /C_RXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 44.7675 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J20 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 /C_RTS))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 /C_RTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 42.2275 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J21 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 /C_CTS))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 /C_CTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 39.6875 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J22 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 /C_DTR))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 /C_DTR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 37.1475 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J23 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 /C_DSR))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 41 /C_DSR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 34.6075 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J24 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 /C_DCD))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 42 /C_DCD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 32.0675 -11.3665)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J25 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 43 /C_RI))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 43 /C_RI))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 49.8475 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J26 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D_TXD))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D_TXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 47.3075 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J27 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D_RXD))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 45 /D_RXD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 44.7675 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J28 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 46 /D_RTS))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 46 /D_RTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 42.2275 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J29 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 47 /D_CTS))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 47 /D_CTS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 39.6875 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J30 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 /D_DTR))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 /D_DTR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 37.1475 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J31 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 /D_DSR))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 /D_DSR))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 34.6075 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J32 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 /D_DCD))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 /D_DCD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 32.0675 -4.2545)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J33 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 /D_RI))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 /D_RI))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 582EB4C5)
    (at 54.229 -4.191)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J34 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 52 /SUSPEND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 52 /SUSPEND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 582EB4C5)
    (at 13.462 -6.223)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J35 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 +5V))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 582EB4C5)
    (at 25.527 -18.542 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J36 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB7FE)
    (at 51.7525 -37.719)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value BLM21PG300SN1 (at 0.127 -0.381) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB7F7)
    (at 48.0695 -37.719 180)
    (attr smd)
    (fp_text reference L2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value BLM21PG300SN1 (at 0.127 -0.381 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB80D)
    (at 22.86 -13.335 270)
    (attr smd)
    (fp_text reference L3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value BLM21PG300SN1 (at 0.127 -0.381 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 +5V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 31.75 -29.464)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 31.75 -27.559 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 54 /EEDATA))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 35.433 -23.749)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 /EECLK))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 35.433 -25.781)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 56 /EECS))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 55.88 -36.8935 90)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 /RES))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 44.45 -37.719)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 12k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 11.049 -32.385 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 58 /A))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 14.097 -32.385 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 59 /B))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 17.272 -32.385 90)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 60 /C))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 20.447 -32.385 90)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 61 /D))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 23.622 -32.385 90)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 62 /E))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D6-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 26.67 -32.385 90)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 63 /F))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 29.972 -32.385 90)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 64 /G))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 33.147 -32.385 90)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 300R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 65 /H))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D9-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 20.701 -19.3675 270)
    (attr smd)
    (fp_text reference R15 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 66 /#PWREN))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOT-23-6 (layer B.Cu) (tedit 582EB8A1)
    (at 31.75 -24.257)
    (fp_text reference U1 (at -0.127 0 180) (layer B.SilkS))
    (fp_text value 93LC56BT-I/OT (at 0.0635 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.9525 -1.27) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0 -1.27) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.9525 -1.27) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 54 /EEDATA))
    (pad 4 smd rect (at 0.9525 1.27) (size 0.50104 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 55 /EECLK))
    (pad 5 smd rect (at 0 1.27) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 56 /EECS))
    (pad 6 smd rect (at -0.9525 1.27) (size 0.5 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model MLAB_3D/IO/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOT-223 (layer B.Cu) (tedit 582EB4C5)
    (at 25.654 -7.112 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0 0.762 90) (layer B.SilkS))
    (fp_text value LM1117_3V3 (at 0 -0.762 90) (layer B.Fab))
    (pad 1 smd rect (at -2.286 -3.302 90) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.286 -3.302 90) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0 -3.302 90) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 4 smd rect (at 0 3.302 90) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-N (layer B.Cu) (tedit 582EB4C5)
    (at 23.495 -25.654)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 0.127 1.27) (layer B.SilkS))
    (fp_text value SN74HC595D (at 0 -1.27) (layer B.Fab))
    (pad 16 smd rect (at -4.445 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 14 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 54 /EEDATA))
    (pad 13 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 66 /#PWREN))
    (pad 12 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 56 /EECS))
    (pad 11 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 55 /EECLK))
    (pad 10 smd rect (at 3.175 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 9 smd rect (at 4.445 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 4.445 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.175 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 65 /H))
    (pad 6 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 64 /G))
    (pad 5 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 63 /F))
    (pad 4 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 62 /E))
    (pad 3 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 61 /D))
    (pad 2 smd rect (at -3.175 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 60 /C))
    (pad 1 smd rect (at -4.445 -3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 59 /B))
    (pad 15 smd rect (at -3.175 3.175) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 58 /A))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_XTAL:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 582EB4C5)
    (at 40.132 -34.417)
    (descr "Crystal, Quarz, HC49/U, vertical, stehend,")
    (tags "Crystal, Quarz, HC49/U, vertical, stehend,")
    (fp_text reference Y1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 12MHz (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at -2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad1)"))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 582EB4C5)
    (at 35.433 -21.59 180)
    (attr smd)
    (fp_text reference C21 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "#RTS" (at 44.831 -14.351 270) (layer F.SilkS))
  (gr_text H (at 33.274 -33.274) (layer F.SilkS))
  (gr_text G (at 29.972 -33.274) (layer F.SilkS))
  (gr_text F (at 26.67 -33.274) (layer F.SilkS))
  (gr_text E (at 23.622 -33.274) (layer F.SilkS))
  (gr_text D (at 20.32 -33.274) (layer F.SilkS))
  (gr_text C (at 17.272 -33.274) (layer F.SilkS))
  (gr_text B (at 13.97 -33.274) (layer F.SilkS))
  (gr_text A (at 10.922 -33.274) (layer F.SilkS))
  (gr_text "MLAB.CZ\nUSB4xUART01A" (at 39.878 -25.146) (layer F.SilkS))
  (gr_text +3V3 (at 25.4 -22.606) (layer F.SilkS))
  (gr_text +5V (at 17.78 -6.35 270) (layer F.SilkS))
  (gr_text "#RES" (at 61.722 -35.56 270) (layer F.SilkS))
  (gr_text "#SUS" (at 56.896 -4.318 270) (layer F.SilkS))
  (gr_text D (at 28.956 -4.318) (layer F.SilkS))
  (gr_text C (at 28.956 -11.43) (layer F.SilkS))
  (gr_text "#RI" (at 32.004 -14.478 270) (layer F.SilkS))
  (gr_text "#DCD" (at 34.544 -14.478 270) (layer F.SilkS))
  (gr_text "#DSR" (at 56.134 -16.256) (layer F.SilkS))
  (gr_text "#DTR" (at 39.624 -14.478 270) (layer F.SilkS))
  (gr_text "#CTS" (at 42.418 -14.478 270) (layer F.SilkS))
  (gr_text RXD (at 47.371 -14.224 270) (layer F.SilkS))
  (gr_text TXD (at 49.784 -14.224 270) (layer F.SilkS))
  (gr_text "#RI" (at 56.134 -11.176) (layer F.SilkS))
  (gr_text "#DCD" (at 56.388 -13.716) (layer F.SilkS))
  (gr_text "#DSR" (at 37.084 -14.478 270) (layer F.SilkS))
  (gr_text "#DTR" (at 56.134 -18.796) (layer F.SilkS))
  (gr_text "#CTS" (at 56.134 -21.336) (layer F.SilkS))
  (gr_text "#RTS" (at 56.134 -23.876) (layer F.SilkS))
  (gr_text TXD (at 56.134 -28.956) (layer F.SilkS))
  (gr_text RXD (at 56.134 -26.416) (layer F.SilkS))
  (gr_text B (at 66.294 -31.496) (layer F.SilkS))
  (gr_text A (at 59.055 -31.496) (layer F.SilkS))
  (gr_text "JACHO\n2016" (at 4.826 -11.43) (layer F.SilkS))
  (gr_text 2016 (at 5.715 -20.828 90) (layer B.Cu))
  (gr_text MLAB.CZ (at 2.667 -21.209 90) (layer B.Cu))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 70.866 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.866 -40.386) (end 70.866 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 70.866 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.026 -44.196) (xy 75.946 4.572) (xy -7.239 3.556) (xy -4.572 -44.831)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.676 -42.545) (xy 73.66 1.524) (xy -2.921 1.524) (xy -1.651 -43.434)
      )
    )
  )
)
