(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 44)
    (no_connects 0)
    (area 0.178999 -40.461001 30.301001 -0.178999)
    (thickness 1.6)
    (drawings 19)
    (tracks 235)
    (zones 0)
    (modules 21)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 1.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /IN1)
  (net 4 /IN2)
  (net 5 /OUT1)
  (net 6 /OUT2)
  (net 7 "Net-(R1-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /IN1)
    (add_net /IN2)
    (add_net /OUT1)
    (add_net /OUT2)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net VCC)
  )
  (module Mlab_IO:HSOP-8 (layer B.Cu) (tedit 589027DC)
    (at 18.034 -19.939 180)
    (fp_text reference U1 (at 0 -0.5 180) (layer B.SilkS))
    (fp_text value DRV8871 (at 0 0.5 180) (layer B.Fab))
    (fp_text user * (at -1.9304 -1.7653 180) (layer B.SilkS))
    (pad 9 thru_hole circle (at -1.3 0.65 180) (size 0.45 0.45) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -1.3 -0.65 180) (size 0.45 0.45) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 1.3 -0.65 180) (size 0.45 0.45) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 1.3 0.65 180) (size 0.45 0.45) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0 0.65 180) (size 0.45 0.45) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0 -0.65 180) (size 0.45 0.45) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 smd trapezoid (at 0 0 180) (size 3.1 2.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd trapezoid (at -1.905 2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 6 /OUT2))
    (pad 7 smd trapezoid (at -0.635 2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd trapezoid (at 0.635 2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 5 /OUT1))
    (pad 5 smd trapezoid (at 1.905 2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd trapezoid (at 1.905 -2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(R1-Pad1)"))
    (pad 3 smd trapezoid (at 0.635 -2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 3 /IN1))
    (pad 2 smd trapezoid (at -0.635 -2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 4 /IN2))
    (pad 1 smd trapezoid (at -1.905 -2.875 180) (size 0.45 2.15) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 589027DC)
    (at 13.97 -20.828 270)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF/50V (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 589027DC)
    (at 8.255 -23.749 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C3 (at 0.0127 -0.0381 180) (layer B.SilkS))
    (fp_text value 47uF/16V (at -0.09906 -3.59918 180) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 180) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_D:Diode-SMB_Standard (layer B.Cu) (tedit 589027DC)
    (at 6.35 -29.21)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D1 (at -0.762 0.127) (layer B.SilkS))
    (fp_text value STPS340U (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072) (layer B.SilkS))
    (pad 2 smd rect (at -2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 589027DC)
    (at 7.62 -18.796)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J1 (at -5.842 0 90) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 589027DC)
    (at 7.62 -13.716)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J2 (at -5.842 0 90) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 589027DC)
    (at 15.367 -5.08 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /IN1))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /IN1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 589027DC)
    (at 17.907 -5.08 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /IN2))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /IN2))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 589027DC)
    (at 12.827 -5.08 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 589027DC)
    (at 13.335 -32.893 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J6 (at -5.842 0) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 /OUT1))
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 /OUT1))
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 589027DC)
    (at 18.415 -32.893 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J7 (at -5.842 0) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 /OUT2))
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 /OUT2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 589027DC)
    (at 13.97 -16.3195 270)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 33k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(R1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 589027DC)
    (at 8.128 -25.781 180)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -0.127 1.651 180) (layer F.SilkS))
    (fp_text value 47uF/63V (at 1.25 4.4 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 589027DC)
    (at 25.273 -25.781)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /OUT1))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /OUT1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 589027DC)
    (at 25.273 -28.321)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /OUT2))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /OUT2))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 589027DC)
    (at 15.367 -10.033 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /IN1))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 589027DC)
    (at 19.431 -10.033)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /IN2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MLAB.CZ\n2017" (at 26.035 -13.462 90) (layer B.Cu))
  (gr_text OUT1 (at 25.273 -23.368) (layer F.SilkS))
  (gr_text + (at 8.636 -24.384) (layer F.SilkS))
  (gr_text 2017 (at 25.273 -9.525) (layer F.SilkS))
  (gr_text HBRIDGE03A (at 27.432 -16.129 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 25.146 -16.256 90) (layer F.SilkS))
  (gr_text - (at 1.778 -10.287) (layer F.SilkS))
  (gr_text OUT1 (at 9.779 -35.179 90) (layer F.SilkS))
  (gr_text OUT2 (at 25.273 -30.734) (layer F.SilkS))
  (gr_text "MAX 0.5A" (at 28.956 -26.924 90) (layer F.SilkS))
  (gr_text "POWER\nIN" (at 20.447 -15.748 90) (layer F.SilkS))
  (gr_text + (at 1.524 -22.606) (layer F.SilkS))
  (gr_text GND (at 10.414 -5.08 90) (layer F.SilkS))
  (gr_text IN2 (at 20.32 -5.08 90) (layer F.SilkS))
  (gr_text IN1 (at 15.494 -8.89) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30.226 -40.386) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name /OUT2) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.685 -21.717) (xy 19.685 -27.051) (xy 18.161 -28.575) (xy 16.51 -30.226) (xy 16.51 -37.338)
        (xy 20.701 -37.338) (xy 20.701 -21.717)
      )
    )
  )
  (zone (net 5) (net_name /OUT1) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.653 -21.717) (xy 17.653 -26.035) (xy 15.494 -28.321) (xy 15.494 -37.465) (xy 11.303 -37.465)
        (xy 11.303 -28.321) (xy 12.192 -27.432) (xy 13.716 -27.432) (xy 14.859 -26.289) (xy 16.891 -24.257)
        (xy 16.891 -21.717)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 3.175 -16.891) (xy 3.175 -20.701) (xy 7.747 -20.701) (xy 8.001 -20.955) (xy 8.255 -21.209)
        (xy 8.255 -24.384) (xy 7.493 -25.146) (xy 7.493 -30.48) (xy 10.16 -30.48) (xy 10.16 -27.94)
        (xy 11.684 -26.416) (xy 13.843 -26.416) (xy 16.383 -23.876) (xy 16.383 -21.717) (xy 15.875 -21.717)
        (xy 15.367 -21.209) (xy 13.081 -21.209) (xy 12.319 -20.447) (xy 12.319 -16.764) (xy 8.255 -16.764)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.016 -41.148) (xy 32.131 -41.91) (xy 31.623 0.762) (xy -1.905 2.159)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.433 4.318) (xy -7.493 8.001) (xy -2.159 -42.291) (xy 37.465 -43.688)
      )
    )
  )
)
