(kicad_pcb (version 4) (host pcbnew 0.201601041403+6416~40~ubuntu15.10.1-stable)
  (general
    (links 115)
    (no_connects 0)
    (area -7.874 -47.046 60.673429 7.620001)
    (thickness 1.6)
    (drawings 36)
    (tracks 361)
    (zones 0)
    (modules 56)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.254)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.0988 2.89814)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x011e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VSS)
  (net 2 GND)
  (net 3 VDD)
  (net 4 "Net-(C10-Pad2)")
  (net 5 "Net-(J25-Pad1)")
  (net 6 /STBY)
  (net 7 /FLAG)
  (net 8 /SYNC)
  (net 9 "Net-(C11-Pad2)")
  (net 10 /STCK)
  (net 11 /ADCIN)
  (net 12 /CS)
  (net 13 /CK)
  (net 14 /SDO)
  (net 15 /SDI)
  (net 16 /OSCI)
  (net 17 /OSCO)
  (net 18 "Net-(C11-Pad1)")
  (net 19 /1A)
  (net 20 /2A)
  (net 21 /1B)
  (net 22 /2B)
  (net 23 "Net-(C14-Pad1)")
  (net 24 "Net-(C15-Pad1)")
  (net 25 "Net-(R6-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /1A)
    (add_net /1B)
    (add_net /2A)
    (add_net /2B)
    (add_net /ADCIN)
    (add_net /CK)
    (add_net /CS)
    (add_net /FLAG)
    (add_net /OSCI)
    (add_net /OSCO)
    (add_net /SDI)
    (add_net /SDO)
    (add_net /STBY)
    (add_net /STCK)
    (add_net /SYNC)
    (add_net GND)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(J25-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net VDD)
    (add_net VSS)
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55119582)
    (at 13.716 -32.766 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J5 (at -4.826 -3.556 270) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55119586)
    (at 18.796 -32.766 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J4 (at -4.826 -3.556 270) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 VSS))
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 VSS))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 29.21 -2.54)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J25-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 25.146 -2.54)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 68k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J25-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.148 -29.21 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /SYNC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.116 -29.21 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /FLAG))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.052 -2.54)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /STBY))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 551198FB)
    (at 45.72 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 551198EA)
    (at 45.72 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 551198F7)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 551198F4)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value sroub (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 55128FCE)
    (at 27.686 -5.334)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J25 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J25-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 55128FD6)
    (at 27.686 -7.874)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J24 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /ADCIN))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 55131494)
    (at 25.146 -7.874)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J19 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C15-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 55131498)
    (at 25.146 -5.334)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J18 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F70)
    (at 11.938 -5.08 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J15 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /OSCO))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /OSCO))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F75)
    (at 14.478 -5.08 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J14 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /OSCI))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /OSCI))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F9C)
    (at 35.56 -31.242)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J13 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SDI))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SDI))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F95)
    (at 35.56 -33.782)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /CK))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /CK))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F86)
    (at 35.56 -28.702)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /CS))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /CS))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128FB1)
    (at 30.226 -6.604 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /STBY))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /STBY))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F7F)
    (at 45.72 -27.178)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /STCK))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /STCK))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128FA0)
    (at 45.72 -29.718)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SYNC))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SYNC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128FA4)
    (at 35.56 -26.162)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /FLAG))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /FLAG))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F61)
    (at 3.81 -29.972)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F65)
    (at 3.81 -27.432)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 VDD))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 55128F69)
    (at 3.81 -24.892)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 56667F12)
    (at 40.132 -6.858 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D4 (at 0.254 -2.54 270) (layer B.SilkS))
    (fp_text value BZV55C-3,6V (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 11 /ADCIN))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 5511C478)
    (at 8.89 -27.178 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 -0.254 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 5511C45E)
    (at 23.368 -33.528 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 37.719 -7.747 90)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /ADCIN))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 20.574 -6.35 90)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 19.558 -9.144)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 220nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.148 -25.654 270)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /SYNC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.116 -25.146 270)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /FLAG))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 39.116 -2.54)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100pF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /STBY))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 5511C465)
    (at 28.448 -32.258 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C6 (at 0 0 90) (layer B.SilkS))
    (fp_text value 22-47uF/20V (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 15.748 -9.144 180)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 5511C47E)
    (at 19.558 -2.794 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -3.556 180) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 32.639 -10.922 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 24.384 -28.702)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 18.0975 -26.924 180)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:POWERSO36 (layer B.Cu) (tedit 5511C301)
    (at 23.876 -18.288 180)
    (descr "36 LEADS POWER SMALL OUTLINE PACKAGE")
    (tags "36 LEADS POWER SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference U1 (at -1.905 3.175 180) (layer B.SilkS))
    (fp_text value L6470 (at -1.27 -3.175 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -5.5245 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.87426 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 19 /1A))
    (pad 3 smd rect (at -4.22402 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 19 /1A))
    (pad 4 smd rect (at -3.57378 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 5 smd rect (at -2.92354 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 6 smd rect (at -2.2733 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 6 /STBY))
    (pad 7 smd rect (at -1.62306 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R6-Pad1)"))
    (pad 8 smd rect (at -0.97282 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 11 /ADCIN))
    (pad 9 smd rect (at -0.32258 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(C15-Pad1)"))
    (pad 10 smd rect (at 0.32258 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 16 /OSCI))
    (pad 11 smd rect (at 0.97282 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 17 /OSCO))
    (pad 12 smd rect (at 1.62306 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2.2733 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad2)"))
    (pad 14 smd rect (at 2.92354 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C10-Pad2)"))
    (pad 15 smd rect (at 3.57378 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 16 smd rect (at 4.22402 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 17 smd rect (at 4.87426 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 21 /1B))
    (pad 18 smd rect (at 5.5245 -6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 21 /1B))
    (pad 19 smd rect (at 5.5245 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.87426 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 22 /2B))
    (pad 21 smd rect (at 4.22402 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 22 /2B))
    (pad 22 smd rect (at 3.57378 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 23 smd rect (at 2.92354 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 24 smd rect (at 2.2733 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (pad 25 smd rect (at 1.62306 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 14 /SDO))
    (pad 26 smd rect (at 0.97282 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 13 /CK))
    (pad 27 smd rect (at 0.32258 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 15 /SDI))
    (pad 28 smd rect (at -0.32258 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 29 smd rect (at -0.97282 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 8 /SYNC))
    (pad 30 smd rect (at -1.62306 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 12 /CS))
    (pad 31 smd rect (at -2.2733 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 7 /FLAG))
    (pad 32 smd rect (at -2.92354 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 10 /STCK))
    (pad 33 smd rect (at -3.57378 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 34 smd rect (at -4.22402 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (pad 35 smd rect (at -4.87426 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 20 /2A))
    (pad 36 smd rect (at -5.5245 6.69798 180) (size 0.39878 1.39954) (layers B.Cu B.Paste B.Mask)
      (net 20 /2A))
    (pad 51 smd rect (at 0 0 180) (size 9.79932 6.1976) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 50 smd rect (at -6.44906 0 180) (size 3.0988 2.89814) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 52 smd rect (at 6.44906 0 180) (size 3.0988 2.89814) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Mlab_IO:SOT-23 (layer B.Cu) (tedit 5665593B)
    (at 17.907 -6.096)
    (tags SOT23)
    (fp_text reference D3 (at 0.127 -1.016) (layer B.SilkS))
    (fp_text value BAS70-04 (at 0.0635 0) (layer B.SilkS) hide)
    (pad 3 smd rect (at 0 1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 VSS))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Elko_ThroughHole:Elko_vert_11x5mm_RM2_CopperClear (layer F.Cu) (tedit 553F1B29)
    (at 26.67 -31.369 90)
    (descr "Electrolytic Capacitor, vertical, diameter 5mm, radial, RM 2mm, Copper Clear")
    (tags "Electrolytic Capacitor, vertical, diameter 5mm, radial, RM 2mm, Elko, Electrolytkondensator, Kondensator gepolt, Copper clear,")
    (fp_text reference C13 (at 0.889 1.651 270) (layer F.SilkS))
    (fp_text value 100uF/50V (at 1.016 5.08 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.01524 0 90) (size 1.48082 1.48082) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 VSS))
    (pad 2 thru_hole circle (at 2.01676 0 90) (size 1.48082 1.48082) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_Elko_ThroughHole.3dshapes/Elko_vert_11x5mm_RM2_CopperClear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 553F1BFE)
    (at 35.56 -36.322)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J12 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SDO))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SDO))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256_2 (layer F.Cu) (tedit 553F1DC0)
    (at 7.874 -18.288 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J23 (at -4.826 -3.556 180) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 /2B))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 /2B))
  )
  (module Mlab_Con:WAGO256_2 (layer F.Cu) (tedit 553F1DC0)
    (at 7.874 -13.288 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J22 (at -4.826 -3.556 180) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 21 /1B))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 21 /1B))
  )
  (module Mlab_Con:WAGO256_2 (layer F.Cu) (tedit 553F1DC0)
    (at 42.926 -20.066)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J21 (at -4.826 -3.556) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /2A))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /2A))
  )
  (module Mlab_Con:WAGO256_2 (layer F.Cu) (tedit 553F1DC0)
    (at 42.926 -15.066)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J20 (at -4.826 -3.556) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 19 /1A))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 19 /1A))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 40.894 -11.176)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56667C4F)
    (at 32.766 -5.334)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J27 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 36.83 -11.176)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(C14-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56667D69)
    (at 32.766 -7.874)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J26 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C14-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.433 -6.604 270)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 VDD))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 22.733 -6.35 270)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 34.417 -5.715) (layer F.SilkS))
  (gr_text SW (at 34.417 -8.255) (layer F.SilkS))
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 v" (at 55.452 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 50.546 -40.386) (xy 56.802 -40.386)))
    (feature2 (pts (xy 50.546 -0.254) (xy 56.802 -0.254)))
    (crossbar (pts (xy 54.102 -0.254) (xy 54.102 -40.386)))
    (arrow1a (pts (xy 54.102 -40.386) (xy 54.688421 -39.259496)))
    (arrow1b (pts (xy 54.102 -40.386) (xy 53.515579 -39.259496)))
    (arrow2a (pts (xy 54.102 -0.254) (xy 54.688421 -1.380504)))
    (arrow2b (pts (xy 54.102 -0.254) (xy 53.515579 -1.380504)))
  )
  (dimension 50.292 (width 0.3) (layer Dwgs.User)
    (gr_text "1,9800 v" (at 25.4 -45.546) (layer Dwgs.User))
    (feature1 (pts (xy 50.546 -40.386) (xy 50.546 -46.896)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -46.896)))
    (crossbar (pts (xy 0.254 -44.196) (xy 50.546 -44.196)))
    (arrow1a (pts (xy 50.546 -44.196) (xy 49.419496 -43.609579)))
    (arrow1b (pts (xy 50.546 -44.196) (xy 49.419496 -44.782421)))
    (arrow2a (pts (xy 0.254 -44.196) (xy 1.380504 -43.609579)))
    (arrow2b (pts (xy 0.254 -44.196) (xy 1.380504 -44.782421)))
  )
  (gr_text CK (at 32.512 -33.782) (layer F.SilkS))
  (gr_text OSC1 (at 17.018 -5.08 90) (layer F.SilkS))
  (gr_text OSC0 (at 9.652 -5.08 90) (layer F.SilkS))
  (gr_text MLAB (at 41.656 -35.306 90) (layer B.Cu))
  (gr_text JACHO (at 38.608 -3.556) (layer F.SilkS))
  (gr_text 2016 (at 38.608 -1.524) (layer F.SilkS))
  (gr_text HBSTEP01B (at 17.653 -15.494 90) (layer F.SilkS))
  (gr_text MLAB.cz (at 20.066 -15.875 90) (layer F.SilkS))
  (gr_text STBY (at 29.718 -12.065 90) (layer F.SilkS))
  (gr_text ADCIN (at 25.4 -9.652 90) (layer F.SilkS))
  (gr_text VREG (at 23.749 -7.62) (layer F.SilkS))
  (gr_text VDD (at 23.749 -5.334) (layer F.SilkS))
  (gr_text "#FLAG" (at 32.512 -25.908) (layer F.SilkS))
  (gr_text SYNC (at 41.529 -34.163 90) (layer F.SilkS))
  (gr_text SDI (at 32.893 -31.242) (layer F.SilkS))
  (gr_text SDO (at 32.512 -36.322) (layer F.SilkS))
  (gr_text STCK (at 49.53 -29.718 90) (layer F.SilkS))
  (gr_text "#CS" (at 32.512 -28.702) (layer F.SilkS))
  (gr_text MOTOR (at 23.114 -35.433 90) (layer F.SilkS))
  (gr_text POWER (at 9.525 -35.56 90) (layer F.SilkS))
  (gr_text "POWER\nIO\n" (at 8.636 -27.432 90) (layer F.SilkS))
  (gr_text + (at 21.9964 -24.8412) (layer F.SilkS))
  (gr_text OUT1B (at 7.112 -9.144) (layer F.SilkS))
  (gr_text OUT2B (at 6.858 -22.098) (layer F.SilkS))
  (gr_text OUT2A (at 42.926 -23.876) (layer F.SilkS))
  (gr_text OUT1A (at 45.974 -10.922) (layer F.SilkS))
  (gr_line (start 50.546 -40.386) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.546 -0.254) (end 50.546 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 50.546 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 20) (net_name /2A) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.26 -18.034) (xy 36.83 -18.034) (xy 28.448 -23.368) (xy 28.448 -25.908) (xy 29.972 -25.908)
        (xy 30.226 -25.908) (xy 30.226 -24.13) (xy 36.068 -24.13) (xy 38.354 -22.606) (xy 48.26 -22.606)
      )
    )
  )
  (zone (net 19) (net_name /1A) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.26 -17.018) (xy 36.83 -17.018) (xy 27.686 -13.208) (xy 27.686 -10.414) (xy 28.956 -10.414)
        (xy 29.21 -10.414) (xy 29.21 -12.7) (xy 48.26 -12.7)
      )
    )
  )
  (zone (net 22) (net_name /2B) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.54 -20.828) (xy 12.7 -20.828) (xy 18.542 -24.384) (xy 18.542 -25.908) (xy 20.066 -25.908)
        (xy 20.066 -22.86) (xy 20.066 -22.352) (xy 18.542 -22.352) (xy 12.446 -16.256) (xy 2.54 -16.256)
      )
    )
  )
  (zone (net 21) (net_name /1B) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.54 -15.24) (xy 12.7 -15.24) (xy 19.304 -12.7) (xy 19.304 -10.414) (xy 17.78 -10.414)
        (xy 17.272 -10.414) (xy 2.54 -10.414)
      )
    )
  )
  (zone (net 1) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.718 -26.67) (xy 28.448 -26.162) (xy 28.194 -26.162) (xy 28.194 -23.876) (xy 27.178 -23.876)
        (xy 27.178 -25.908) (xy 26.162 -26.924) (xy 26.162 -29.972) (xy 21.336 -29.972) (xy 21.336 -24.13)
        (xy 20.32 -24.13) (xy 20.32 -26.162) (xy 16.764 -28.194) (xy 16.764 -37.592) (xy 21.082 -37.592)
        (xy 21.082 -33.274) (xy 24.638 -33.274) (xy 26.924 -31.75) (xy 29.718 -31.75)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.30117 3.810293) (xy -4.318 4.318) (xy -4.318 3.81)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.102 4.826) (xy -4.30117 3.810293) (xy -2.794 -41.656) (xy 53.086 -41.148)
      )
    )
  )
  (zone (net 1) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.558 -10.668) (xy 20.574 -10.668) (xy 20.574 -13.716) (xy 19.558 -13.716)
      )
    )
  )
  (zone (net 1) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.416 -10.668) (xy 27.432 -10.668) (xy 27.432 -13.716) (xy 26.416 -13.716)
      )
    )
  )
  (zone (net 1) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.51 -37.592) (xy 21.082 -37.592) (xy 21.082 -14.732) (xy 21.082 -13.97) (xy 27.686 -13.97)
        (xy 27.686 -12.7) (xy 19.304 -12.7) (xy 16.51 -12.7)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -6.096 -45.466) (xy 57.404 -43.434) (xy 57.15 7.62) (xy -7.112 7.366) (xy -7.874 6.858)
      )
    )
  )
)
