(kicad_pcb (version 4) (host pcbnew 0.201603091917+6614~43~ubuntu15.10.1-product)
  (general
    (links 171)
    (no_connects 0)
    (area 96.468499 83.002 167.309715 150.3902)
    (thickness 1.6)
    (drawings 18)
    (tracks 430)
    (zones 0)
    (modules 80)
    (nets 43)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.2)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VCOM)
  (net 2 GNDA)
  (net 3 VSS)
  (net 4 +5V)
  (net 5 "Net-(C8-Pad1)")
  (net 6 "Net-(C9-Pad1)")
  (net 7 "Net-(C10-Pad1)")
  (net 8 "Net-(C10-Pad2)")
  (net 9 "Net-(C11-Pad1)")
  (net 10 "Net-(C12-Pad1)")
  (net 11 "Net-(C13-Pad1)")
  (net 12 "Net-(C14-Pad1)")
  (net 13 "Net-(C15-Pad2)")
  (net 14 "Net-(C16-Pad1)")
  (net 15 "Net-(C17-Pad2)")
  (net 16 "Net-(C18-Pad2)")
  (net 17 "Net-(C19-Pad1)")
  (net 18 "Net-(C20-Pad2)")
  (net 19 "Net-(D2-Pad1)")
  (net 20 "Net-(D3-Pad1)")
  (net 21 "Net-(D4-Pad1)")
  (net 22 "Net-(D5-Pad1)")
  (net 23 "Net-(J4-Pad1)")
  (net 24 "Net-(J7-Pad1)")
  (net 25 "Net-(J8-Pad1)")
  (net 26 "Net-(J9-Pad1)")
  (net 27 "Net-(J10-Pad1)")
  (net 28 "Net-(J11-Pad1)")
  (net 29 "Net-(J12-Pad1)")
  (net 30 "Net-(J13-Pad1)")
  (net 31 "Net-(J14-Pad1)")
  (net 32 "Net-(J15-Pad1)")
  (net 33 VCC)
  (net 34 "Net-(J19-Pad2)")
  (net 35 "Net-(J20-Pad1)")
  (net 36 "Net-(J21-Pad1)")
  (net 37 "Net-(J22-Pad2)")
  (net 38 "Net-(J23-Pad1)")
  (net 39 "Net-(R5-Pad1)")
  (net 40 "Net-(R6-Pad1)")
  (net 41 "Net-(C21-Pad2)")
  (net 42 "Net-(C22-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GNDA)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J19-Pad2)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J22-Pad2)")
    (add_net "Net-(J23-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net VCC)
    (add_net VCOM)
    (add_net VSS)
  )
  (module HBSTEP02A:Inductor_4.5_4.1 (layer B.Cu) (tedit 56E57FE2)
    (at 125.73 130.81 90)
    (fp_text reference L1 (at 4.064 0 90) (layer B.SilkS))
    (fp_text value 100nH (at 0 0.5 90) (layer B.Fab))
    (pad 1 smd rect (at 2.2 0 90) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -2.2 0 90) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C15-Pad2)"))
  )
  (module HBSTEP02A:SCHOT_D_MSS1P6 (layer B.Cu) (tedit 56E57F4F)
    (at 130.175 129.945 90)
    (fp_text reference D3 (at 2.183 0 90) (layer B.SilkS))
    (fp_text value MSS1P6 (at 0 0.5 90) (layer B.Fab))
    (pad 1 smd rect (at 0.4 0 90) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1.5 0 90) (size 2 1.1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57E93)
    (at 109.6645 102.8065 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.6195 0 90) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57E9C)
    (at 112.395 102.854 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.572 0 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57F0D)
    (at 100.584 122.428 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.937 0.0635 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57E8B)
    (at 106.9975 102.87 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -3.556 -0.0635 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57F06)
    (at 107.696 122.428)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.937 0.0635) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57E7B)
    (at 141.08241 125.73 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.0635 -1.905 270) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D10_L13_P5 (layer F.Cu) (tedit 56E58468)
    (at 105.41 132.08 270)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 13mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C7 (at 1.143 2.794 270) (layer F.SilkS))
    (fp_text value 100uF/50V (at 2.5 6.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 VSS))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L13_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57F43)
    (at 121.92 125.095)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.683 0.127) (layer B.SilkS))
    (fp_text value 1nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57F2C)
    (at 121.92 117.475)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.683 0) (layer B.SilkS))
    (fp_text value 1nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57FD5)
    (at 142.24 130.175 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.651 270) (layer B.SilkS))
    (fp_text value 22n (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57FD1)
    (at 145.415 130.175 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -2.032 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57FB3)
    (at 143.256 125.73 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -0.762 -1.905 90) (layer B.SilkS))
    (fp_text value 470nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57FF1)
    (at 143.891 138.684 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 3.937 0 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57EF2)
    (at 143.8275 100.0285 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 3.7625 0.0635 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E58029)
    (at 123.825 135.255)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -3.683 0) (layer B.SilkS))
    (fp_text value 470pF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57FEE)
    (at 142.875 135.255)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -2.032) (layer B.SilkS))
    (fp_text value 470pF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 123.825 103.886)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 2.1) (layer B.SilkS))
    (fp_text value 470pF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57EDE)
    (at 142.0495 104.0765 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 470pF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57FF6)
    (at 140.335 138.43 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 4.191 0 270) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57EBC)
    (at 126.365 100.0125 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0.127 1.905 270) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E5801B)
    (at 125.73 138.43 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at -3.683 0 90) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(C21-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E57EF7)
    (at 140.2715 100.0125 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at -3.7465 -0.0635 270) (layer B.SilkS))
    (fp_text value 4n7 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(C22-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Handsoldering (layer B.Cu) (tedit 56E57EAE)
    (at 116.1415 105.4735 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 2.85 90) (layer B.SilkS))
    (fp_text value M4 (at 0.05 -4.4 90) (layer B.Fab))
    (fp_text user K (at -3.2385 2.8575 90) (layer B.SilkS))
    (fp_text user A (at 3.175 2.667 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.49936 0 90) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 2.49936 0 90) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Diodes_SMD.3dshapes/SMA_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module HBSTEP02A:SCHOT_D_MSS1P6 (layer B.Cu) (tedit 56E57F59)
    (at 132.715 129.945 90)
    (fp_text reference D2 (at 2.183 0 90) (layer B.SilkS))
    (fp_text value MSS1P6 (at 0 0.5 90) (layer B.Fab))
    (pad 1 smd rect (at 0.4 0 90) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1.5 0 90) (size 2 1.1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
  )
  (module HBSTEP02A:SCHOT_D_MSS1P6 (layer B.Cu) (tedit 56E58039)
    (at 132.715 112.014 270)
    (fp_text reference D4 (at 1.905 0 270) (layer B.SilkS))
    (fp_text value MSS1P6 (at 0 0.5 270) (layer B.Fab))
    (pad 1 smd rect (at 0.4 0 270) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -1.5 0 270) (size 2 1.1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C14-Pad1)"))
  )
  (module HBSTEP02A:SCHOT_D_MSS1P6 (layer B.Cu) (tedit 56E5803B)
    (at 130.175 112.014 270)
    (fp_text reference D5 (at 1.778 0 270) (layer B.SilkS))
    (fp_text value MSS1P6 (at 0 0.5 270) (layer B.Fab))
    (pad 1 smd rect (at 0.4 0 270) (size 0.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -1.5 0 270) (size 2 1.1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C14-Pad1)"))
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 56E683D6)
    (at 102.5525 104.3305)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value "VIO 3.3-5V" (at -4.2545 -0.1905 270) (layer F.SilkS))
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCOM))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCOM))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E682D5)
    (at 102.4255 127.25079 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value REFL/STEP (at 0 9.0805 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E682E6)
    (at 102.4255 124.714 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value REFR/DIR (at 0 8.3185 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C9-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C9-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E682A7)
    (at 121.793 144.272 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value CLK (at -0.127 5.08 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J4-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J4-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 56E580D1)
    (at 104.2035 118.999)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J5 (at -5.842 0 90) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 VSS))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 VSS))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 56E580CE)
    (at 104.2035 113.919)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J6 (at -5.842 0 90) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E682C3)
    (at 119.253 144.272)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at 0 0.254 90) (layer F.SilkS) hide)
    (fp_text value CSN/CFG3 (at 0.127 -8.636 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J7-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J7-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E6829B)
    (at 116.713 144.272 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value SCK/CFG2 (at 0 8.636 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J8-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J8-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E6826F)
    (at 114.173 144.272 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value SID/CFG1 (at 0 8.382 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J9-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J9-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68250)
    (at 111.633 144.272 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at -8.509 0.889 180) (layer F.SilkS) hide)
    (fp_text value SDO/CFG0 (at -0.127 8.636 270) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J10-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J10-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68BE9)
    (at 153.035 114.808 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ENCN/DCO (at 0 -9.017 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J11-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J11-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68BD5)
    (at 153.035 117.348 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value ENCB/CFG4 (at 0 -9.525 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J12-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J12-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68BFC)
    (at 153.035 119.888 270)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J13 (at 0 -0.127 360) (layer F.SilkS) hide)
    (fp_text value ENCA/CFG5 (at 0 9.525 360) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J13-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J13-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68B70)
    (at 153.035 124.968 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SWP/DIAG1 (at 0 -9.017 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J14-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J14-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68BBE)
    (at 153.035 122.428 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J15 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SWN/DIAG0 (at 0 -9.271 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J15-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J15-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 56E580A5)
    (at 130.556 142.32 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J16 (at -5.842 0 180) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C15-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C15-Pad2)"))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 56E580A7)
    (at 135.5725 142.32 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J17 (at -5.842 0 180) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C16-Pad1)"))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C16-Pad1)"))
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 56E681B1)
    (at 112.5855 94.9325 90)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J18 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value "POW. SEL." (at 2.4765 -0.0635 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -2.54 90) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 0 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCOM))
    (pad 2 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 VCC))
    (pad 1 thru_hole rect (at 0 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68330)
    (at 120.2055 96.2025)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J19 (at 0 -5.2705) (layer F.SilkS) hide)
    (fp_text value SDMODE (at 0 7.4295 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J19-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68CF4)
    (at 153.035 130.048 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J20 (at 0 0.127 180) (layer F.SilkS) hide)
    (fp_text value DRV/CFG6 (at 0 -8.509 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J20-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J20-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68BAA)
    (at 153.035 127.508 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J21 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value SWSEL (at 0 -6.477 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J21-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J21-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E6834D)
    (at 122.7455 96.2025)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J22 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SPIMODE (at 0.1905 7.6835 90) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J22-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GNDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 56E68B58)
    (at 153.035 132.588 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J23 (at 0 -0.127 180) (layer F.SilkS) hide)
    (fp_text value AIN (at 0 -4.699 180) (layer F.SilkS))
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J23-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J23-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 56E580AE)
    (at 130.556 96.52 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J24 (at -5.842 0 360) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C17-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C17-Pad2)"))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 56E580B0)
    (at 135.5725 96.52 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J25 (at -5.842 0 360) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C18-Pad2)"))
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C18-Pad2)"))
  )
  (module HBSTEP02A:Inductor_4.5_4.1 (layer B.Cu) (tedit 56E57FDD)
    (at 136.525 130.81 90)
    (fp_text reference L2 (at 4.064 0.254 90) (layer B.SilkS))
    (fp_text value 100nH (at 0 0.5 90) (layer B.Fab))
    (pad 1 smd rect (at 2.2 0 90) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -2.2 0 90) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C16-Pad1)"))
  )
  (module HBSTEP02A:Inductor_4.5_4.1 (layer B.Cu) (tedit 56E58059)
    (at 125.73 109.982 270)
    (fp_text reference L3 (at 4.318 0 270) (layer B.SilkS))
    (fp_text value 100nH (at 0 0.5 270) (layer B.Fab))
    (pad 1 smd rect (at 2.2 0 270) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -2.2 0 270) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad2)"))
  )
  (module HBSTEP02A:Inductor_4.5_4.1 (layer B.Cu) (tedit 56E58052)
    (at 136.525 109.982 270)
    (fp_text reference L4 (at 4.318 0 270) (layer B.SilkS))
    (fp_text value 100nH (at 0 0.5 270) (layer B.Fab))
    (pad 1 smd rect (at 2.2 0 270) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -2.2 0 270) (size 1.5 2.2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C18-Pad2)"))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 101.6 144.78)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 152.4 93.98)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 152.4 144.78)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 101.6 93.98)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GNDA) (clearance 1) (zone_connect 2))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E58020)
    (at 123.19 138.43 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.286 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5418A20D)
    (at 147.1295 137.128 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 2.3 90) (layer B.SilkS))
    (fp_text value 0R27 (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57F3D)
    (at 121.92 127.635 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.683 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57F1C)
    (at 121.92 114.935 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.683 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57F38)
    (at 121.92 122.555 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.683 0 180) (layer B.SilkS))
    (fp_text value 22k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57F21)
    (at 121.92 120.015 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.683 0 180) (layer B.SilkS))
    (fp_text value 22k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57FC3)
    (at 145.415 125.73 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.032 270) (layer B.SilkS))
    (fp_text value 3.3 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 33 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56E57F91)
    (at 142.113 122.3645)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.2225) (layer B.SilkS))
    (fp_text value _R (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J23-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57F94)
    (at 147.066 118.745 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.302 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 56E57EE4)
    (at 146.939 101.6 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -2.921 270) (layer B.SilkS))
    (fp_text value 0R27 (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57F7F)
    (at 147.066 116.459 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 3.81 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J15-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E5800B)
    (at 137.795 135.255)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.778) (layer B.SilkS))
    (fp_text value 27 (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(C19-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5415CDEB)
    (at 128.778 103.886)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 2.1) (layer B.SilkS))
    (fp_text value 27 (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C20-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E58014)
    (at 128.905 135.255)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.778) (layer B.SilkS))
    (fp_text value 27 (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(C21-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C15-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 56E57ED2)
    (at 137.795 103.886 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -2.2225 180) (layer B.SilkS))
    (fp_text value 27 (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(C22-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 56E58010)
    (at 133.35 135.255)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference VR1 (at 0 1.778) (layer B.SilkS))
    (fp_text value VR (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C15-Pad2)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C16-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 133.35 103.886)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference VR2 (at 0 2.1) (layer B.SilkS))
    (fp_text value VR (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad2)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "be3D TSSOP:TQFP-48-1EP_7x7mm_Pitch0.5mm_TRINAMIC" (layer B.Cu) (tedit 56E57F4A)
    (at 132.715 120.65)
    (descr "48-Lead Thin Quad Flatpack (PT) - 7x7x1.0 mm Body [TQFP] With Exposed Pad (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at -4.953 4.445) (layer B.SilkS))
    (fp_text value TMC5130A (at 0 -5.95) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at -4.2 2.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J4-Pad1)"))
    (pad 3 smd rect (at -4.2 1.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J7-Pad1)"))
    (pad 4 smd rect (at -4.2 1.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J8-Pad1)"))
    (pad 5 smd rect (at -4.2 0.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J9-Pad1)"))
    (pad 6 smd rect (at -4.2 0.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -4.2 -0.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J10-Pad1)"))
    (pad 8 smd rect (at -4.2 -0.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R5-Pad1)"))
    (pad 9 smd rect (at -4.2 -1.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R6-Pad1)"))
    (pad 10 smd rect (at -4.2 -1.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCOM))
    (pad 11 smd rect (at -4.2 -2.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J19-Pad2)"))
    (pad 12 smd rect (at -4.2 -2.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J22-Pad2)"))
    (pad 13 smd rect (at -2.75 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 14 smd rect (at -2.25 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at -1.75 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D5-Pad1)"))
    (pad 16 smd rect (at -1.25 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at -0.75 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C14-Pad1)"))
    (pad 18 smd rect (at -0.25 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd rect (at 0.25 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D4-Pad1)"))
    (pad 20 smd rect (at 0.75 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at 1.25 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (pad 22 smd rect (at 1.75 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at 2.25 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(J11-Pad1)"))
    (pad 24 smd rect (at 2.75 -4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(J12-Pad1)"))
    (pad 25 smd rect (at 4.2 -2.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(J13-Pad1)"))
    (pad 26 smd rect (at 4.2 -2.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J15-Pad1)"))
    (pad 27 smd rect (at 4.2 -1.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(J14-Pad1)"))
    (pad 28 smd rect (at 4.2 -1.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J21-Pad1)"))
    (pad 29 smd rect (at 4.2 -0.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J20-Pad1)"))
    (pad 30 smd rect (at 4.2 -0.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J23-Pad1)"))
    (pad 31 smd rect (at 4.2 0.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 32 smd rect (at 4.2 0.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 33 smd rect (at 4.2 1.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 +5V))
    (pad 34 smd rect (at 4.2 1.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C12-Pad1)"))
    (pad 35 smd rect (at 4.2 2.25) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 36 smd rect (at 4.2 2.75) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 37 smd rect (at 2.75 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C10-Pad2)"))
    (pad 38 smd rect (at 2.25 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (pad 39 smd rect (at 1.75 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (pad 40 smd rect (at 1.25 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (pad 41 smd rect (at 0.75 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 42 smd rect (at 0.25 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D2-Pad1)"))
    (pad 43 smd rect (at -0.25 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 44 smd rect (at -0.75 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 45 smd rect (at -1.25 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 46 smd rect (at -1.75 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D3-Pad1)"))
    (pad 47 smd rect (at -2.25 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 48 smd rect (at -2.75 4.2 270) (size 1.5 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (pad 49 smd rect (at 0.875 -0.875) (size 1.75 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at 0.875 0.875) (size 1.75 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.875 -0.875) (size 1.75 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA) (solder_paste_margin_ratio -0.2))
    (pad 49 smd rect (at -0.875 0.875) (size 1.75 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA) (solder_paste_margin_ratio -0.2))
    (pad 49 thru_hole circle (at -1.4 1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -0.5 1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 0.5 1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 1.4 1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -1.4 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 1.4 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -1.4 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 1.4 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -1.4 -1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at -0.5 -1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 0.5 -1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (pad 49 thru_hole circle (at 1.4 -1.4) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GNDA))
    (model Housings_QFP.3dshapes/TQFP-48-1EP_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HBSTEP02A:QR_code (layer F.Cu) (tedit 0)
    (at 147.574 105.918)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Diodes_SMD:SMB_Handsoldering (layer B.Cu) (tedit 552FF2F0)
    (at 111.252 116.67998 90)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference D6 (at 0 3.1 90) (layer B.SilkS))
    (fp_text value M4 (at 0.1 -4.75 90) (layer B.Fab))
    (fp_text user K (at -3.5 -3.1 90) (layer B.SilkS))
    (fp_text user A (at 3 -3.05 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.70002 0 90) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 3 VSS))
    (pad 2 smd rect (at 2.70002 0 90) (size 3.50012 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDA))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "Nojby\n2016" (at 147.32 138.43) (layer F.SilkS))
  (gr_text "HBSTEP02A\nMLAB.cz" (at 124.46 119.126 90) (layer F.SilkS))
  (gr_text - (at 112.522 113.792) (layer F.SilkS))
  (gr_text + (at 112.522 119.126) (layer F.SilkS))
  (gr_text +5V (at 110.236 99.06 90) (layer F.SilkS))
  (dimension 60.452 (width 0.3) (layer Cmts.User)
    (gr_text "2,3800 in" (at 161.624 119.38 90) (layer Cmts.User))
    (feature1 (pts (xy 157.226 89.154) (xy 162.974 89.154)))
    (feature2 (pts (xy 157.226 149.606) (xy 162.974 149.606)))
    (crossbar (pts (xy 160.274 149.606) (xy 160.274 89.154)))
    (arrow1a (pts (xy 160.274 89.154) (xy 160.860421 90.280504)))
    (arrow1b (pts (xy 160.274 89.154) (xy 159.687579 90.280504)))
    (arrow2a (pts (xy 160.274 149.606) (xy 160.860421 148.479496)))
    (arrow2b (pts (xy 160.274 149.606) (xy 159.687579 148.479496)))
  )
  (dimension 60.452 (width 0.3) (layer Cmts.User)
    (gr_text "2,3800 in" (at 127 84.502) (layer Cmts.User))
    (feature1 (pts (xy 157.226 89.154) (xy 157.226 83.152)))
    (feature2 (pts (xy 96.774 89.154) (xy 96.774 83.152)))
    (crossbar (pts (xy 96.774 85.852) (xy 157.226 85.852)))
    (arrow1a (pts (xy 157.226 85.852) (xy 156.099496 86.438421)))
    (arrow1b (pts (xy 157.226 85.852) (xy 156.099496 85.265579)))
    (arrow2a (pts (xy 96.774 85.852) (xy 97.900504 86.438421)))
    (arrow2b (pts (xy 96.774 85.852) (xy 97.900504 85.265579)))
  )
  (gr_text "VIO IN" (at 115.316 99.822 90) (layer F.SilkS))
  (gr_text "MOT. POWER\n" (at 107.95 109.982) (layer F.SilkS))
  (gr_text "POWER\nIO" (at 107.696 104.394 90) (layer F.SilkS))
  (gr_text "OUT2A\n" (at 139.446 142.494 90) (layer F.SilkS))
  (gr_text "OUT1A\n\n" (at 127.889 142.24 90) (layer F.SilkS))
  (gr_text "OUT1B\n" (at 126.746 97.028 90) (layer F.SilkS))
  (gr_text "OUT2B\n\n" (at 140.716 97.028 90) (layer F.SilkS))
  (gr_line (start 96.774 89.154) (end 96.774 149.606) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.226 89.154) (end 96.774 89.154) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.226 149.606) (end 157.226 89.154) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.774 149.606) (end 157.226 149.606) (layer Edge.Cuts) (width 0.15))
  (zone (net 19) (net_name "Net-(D2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.0165 123.952) (xy 132.0165 131.572) (xy 139.446 131.572) (xy 139.446 126.873) (xy 135.636 126.873)
        (xy 134.62 125.857) (xy 134.62 123.952)
      )
    )
  )
  (zone (net 20) (net_name "Net-(D3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.699 123.952) (xy 131.699 129.921) (xy 131.699 131.5085) (xy 124.46 131.5085) (xy 124.46 125.857)
        (xy 124.46 125.349) (xy 130.556 125.349) (xy 130.556 123.952)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C13-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.413 130.302) (xy 129.413 132.588) (xy 133.731 132.588) (xy 133.731 130.302)
      )
    )
  )
  (zone (net 21) (net_name "Net-(D4-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.953 117.348) (xy 134.9375 117.348) (xy 134.9375 114.8715) (xy 136.144 113.665) (xy 137.8585 113.665)
        (xy 137.8585 111.1885) (xy 133.731 111.1885) (xy 133.731 111.76) (xy 131.953 111.76)
      )
    )
  )
  (zone (net 12) (net_name "Net-(C14-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 111.5695) (xy 133.35 109.4105) (xy 129.54 109.4105) (xy 129.54 111.5695)
      )
    )
  )
  (zone (net 22) (net_name "Net-(D5-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 117.348) (xy 131.572 111.76) (xy 129.159 111.76) (xy 129.161783 111.1885) (xy 124.3965 111.1885)
        (xy 124.3965 113.157) (xy 126.1745 114.9985) (xy 126.1745 115.697) (xy 130.2385 115.697) (xy 130.2385 117.348)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C15-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.5875 146.7485) (xy 132.5245 146.7485) (xy 133.096 146.7485) (xy 133.096 142.4305) (xy 133.096 132.842)
        (xy 129.159 132.842) (xy 129.159 131.572) (xy 124.333 131.572) (xy 124.333 137.033) (xy 128.5875 137.033)
      )
    )
  )
  (zone (net 14) (net_name "Net-(C16-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.096 132.842) (xy 134.0485 132.842) (xy 134.0485 131.572) (xy 142.4305 131.572) (xy 142.4305 136.5885)
        (xy 142.4305 136.8425) (xy 137.6045 136.8425) (xy 137.6045 146.7485) (xy 133.096 146.7485)
      )
    )
  )
  (zone (net 1) (net_name VCOM) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.33 102.87) (xy 114.173 102.87) (xy 114.173 106.172) (xy 117.729 106.172) (xy 117.729 109.982)
        (xy 113.03 109.982) (xy 113.03 105.283) (xy 100.33 105.283)
      )
    )
  )
  (zone (net 15) (net_name "Net-(C17-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.524 103.1875) (xy 128.524 92.075) (xy 133.096 92.075) (xy 133.096 105.664) (xy 133.096 109.1565)
        (xy 129.159 109.1565) (xy 129.159 110.871) (xy 123.825 110.871) (xy 123.825 103.1875)
      )
    )
  )
  (zone (net 4) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.319 122.301) (xy 139.319 123.825) (xy 139.319 124.079) (xy 141.605 124.079) (xy 141.605 121.666)
        (xy 139.319 121.666) (xy 139.319 122.174)
      )
    )
  )
  (zone (net 3) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.648 116.967) (xy 104.648 121.539) (xy 109.474 121.539) (xy 109.474 116.967)
      )
    )
  )
  (zone (net 16) (net_name "Net-(C18-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 92.075) (xy 137.6045 92.075) (xy 137.6045 103.1875) (xy 141.9225 103.1875) (xy 141.9225 110.871)
        (xy 133.731 110.871) (xy 133.731 109.1565) (xy 133.35 109.1565)
      )
    )
  )
  (zone (net 3) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.601 130.81) (xy 109.601 134.239) (xy 104.267 134.239) (xy 104.267 130.81)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 149.86) (xy 96.52 149.86) (xy 96.52 88.9) (xy 157.48 88.9) (xy 157.48 149.86)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.48 149.86) (xy 96.52 149.86) (xy 96.52 88.9) (xy 157.48 88.9) (xy 157.48 149.86)
      )
    )
  )
)
