(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 151)
    (no_connects 0)
    (area -5.4864 -146.2532 99.669601 6.146801)
    (thickness 1.6)
    (drawings 51)
    (tracks 346)
    (zones 0)
    (modules 90)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.4)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x01060_80000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 /G)
  (net 3 /F)
  (net 4 /B)
  (net 5 /A)
  (net 6 /E)
  (net 7 /DP)
  (net 8 /C)
  (net 9 /D)
  (net 10 VDD)
  (net 11 GND)
  (net 12 /SDA)
  (net 13 /SCL)
  (net 14 /#OE)
  (net 15 /LED00)
  (net 16 /LED01)
  (net 17 /LED02)
  (net 18 /LED03)
  (net 19 /LED04)
  (net 20 /LED05)
  (net 21 /LED06)
  (net 22 /LED07)
  (net 23 /A2)
  (net 24 /A3)
  (net 25 /A4)
  (net 26 "Net-(J29-Pad1)")
  (net 27 "Net-(AFF1-Pad2)")
  (net 28 /A1)
  (net 29 /A0)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 1.4)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /#OE)
    (add_net /A)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /B)
    (add_net /C)
    (add_net /D)
    (add_net /DP)
    (add_net /E)
    (add_net /F)
    (add_net /G)
    (add_net /LED00)
    (add_net /LED01)
    (add_net /LED02)
    (add_net /LED03)
    (add_net /LED04)
    (add_net /LED05)
    (add_net /LED06)
    (add_net /LED07)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(AFF1-Pad2)")
    (add_net "Net-(J29-Pad1)")
    (add_net VDD)
  )
  (module Mlab_DISPLAY:FYS-40011DS-11 (layer F.Cu) (tedit 5751252B)
    (at 45.6184 -71.6768)
    (fp_text reference AFF1 (at 0.0762 3.8862) (layer F.SilkS) hide)
    (fp_text value FYS-40011DS-11 (at 0.254 -2.0447) (layer F.Fab))
    (pad 8 thru_hole circle (at 0 -54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 10 thru_hole circle (at -10.16 -54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 /G))
    (pad 9 thru_hole circle (at -5.08 -54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /F))
    (pad 6 thru_hole circle (at 10.16 -54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /B))
    (pad 7 thru_hole circle (at 5.08 -54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A))
    (pad 2 thru_hole circle (at -5.08 54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(AFF1-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 /DP))
    (pad 4 thru_hole circle (at 5.08 54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 /C))
    (pad 1 thru_hole circle (at -10.16 54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 3 thru_hole circle (at 0 54.1) (size 2 2) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D))
  )
  (module Mlab_D:LED-10MM (layer F.Cu) (tedit 57512673)
    (at 44.45 -38.1)
    (descr "LED 10mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 10mm 10MM 100mil 2.54mm")
    (fp_text reference D3 (at 1.1684 3.0988) (layer F.SilkS))
    (fp_text value L-813ID (at 1.5 6.1) (layer F.Fab))
    (fp_text user + (at 2.4511 -2.1971) (layer F.SilkS))
    (fp_text user - (at -0.1016 -2.1717) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /E))
    (model LEDs.3dshapes/LED-10MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 41.1988 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J13 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /LED02))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.9852 -57.0992 90)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 29.04236 -52.7304 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0.0127 -0.0381 180) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 180) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 180) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 32.3596 -97.6884 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C3 (at 0.0127 -0.0381 90) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.9664 -57.0992 90)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 54BBE081)
    (at 33.2232 -10.0584)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 2.54) (layer B.SilkS))
    (fp_text value BZV55C-5,6V (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 1.75006 0) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 56BDB339)
    (at 14.6812 -10.8204 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 1 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 16.3068 -4.8768 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 33.5788 -4.8768 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 VDD))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 VDD))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 36.9824 -44.958 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SDA))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SDA))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 36.068 -4.8768 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 38.608 -4.8768 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 28.4988 -4.8768 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -137.16)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 27.5268 -106.704)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 86.36 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M5 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 27.5268 -45.744)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M6 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 58.0068 -106.704 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M7 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 86.36 -137.16)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M8 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 58.0068 -45.744)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M9 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M10 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 11 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 29.4259 -62.23 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /A2))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 29.3751 -66.294 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /A3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 29.4132 -70.3072 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /A4))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 37.9984 -49.2252 180)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 45.8343 -50.8)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /#OE))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.5036 -50.7492)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 34.1376 -76.5683 270)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 /G))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /LED00))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 37.8968 -76.5556 270)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /F))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /LED01))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 41.5544 -76.5556 270)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /A))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /LED02))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 52.6288 -76.5556 270)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /C))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 /LED05))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 45.2628 -76.5556 270)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /B))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 /LED03))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 56.134 -76.5556 270)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 /D))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 /LED06))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 48.9204 -76.5556 270)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /DP))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 /LED04))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 59.7408 -76.5556 270)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /E))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 /LED07))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:TSSOP28 (layer B.Cu) (tedit 57453D9F)
    (at 42.7736 -59.0296)
    (fp_text reference U1 (at 3.302 -1.1684) (layer B.SilkS))
    (fp_text value PCA9635PW (at -1.3335 0.7112) (layer B.SilkS))
    (fp_text user * (at -3.8354 -1.7399) (layer B.SilkS))
    (pad 1 smd rect (at -4.22402 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /A0))
    (pad 2 smd rect (at -3.57378 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /A1))
    (pad 3 smd rect (at -2.92354 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 23 /A2))
    (pad 4 smd rect (at -2.2733 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 24 /A3))
    (pad 5 smd rect (at -1.62306 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 25 /A4))
    (pad 6 smd rect (at -0.97282 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 15 /LED00))
    (pad 7 smd rect (at -0.32258 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 16 /LED01))
    (pad 8 smd rect (at 0.32258 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 17 /LED02))
    (pad 9 smd rect (at 0.97282 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 18 /LED03))
    (pad 10 smd rect (at 1.62306 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /LED04))
    (pad 11 smd rect (at 2.2733 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 20 /LED05))
    (pad 12 smd rect (at 2.92354 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 21 /LED06))
    (pad 13 smd rect (at 3.57378 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 22 /LED07))
    (pad 14 smd rect (at 4.22402 -2.79908 180) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 15 smd rect (at 4.22402 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 3.57378 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at 2.92354 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 2.2733 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd rect (at 1.62306 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 0.97282 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at 0.32258 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 22 smd rect (at -0.32258 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at -0.97282 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 14 /#OE))
    (pad 24 smd rect (at -1.62306 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 25 smd rect (at -2.2733 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 26 smd rect (at -2.92354 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SCL))
    (pad 27 smd rect (at -3.57378 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 12 /SDA))
    (pad 28 smd rect (at -4.22402 2.79908) (size 0.45 1.6) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 36.1188 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J11 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /LED00))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 38.6588 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J12 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /LED01))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 43.7388 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J14 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LED03))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 46.2788 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J15 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /LED04))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 48.8188 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J16 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LED05))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 51.3588 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J17 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LED06))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 53.8988 -69.6976)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J18 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LED07))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 36.1696 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J19 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /G))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 38.7096 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J20 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /F))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 41.2496 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J21 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 48.8696 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J22 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /C))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 43.7896 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J23 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /B))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 51.4096 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J24 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 46.3296 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J25 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /DP))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 53.9496 -86.1568)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J26 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /E))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 27.178 -96.3168)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J27 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 39.5224 -44.958 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J28 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 VDD))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 VDD))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 31.0388 -4.8768 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J29 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J29-Pad1)"))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J29-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 42.0624 -44.958 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J30 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 44.6024 -44.958 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J31 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 48.6664 -44.958 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J36 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /#OE))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /#OE))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -87.3252)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J37 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -79.7052)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J38 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -84.7852)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J39 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -82.2452)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J40 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -74.6252)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J41 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -77.1652)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J42 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -72.0852)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J43 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56EBDE01)
    (at 25.2984 -69.5452)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J44 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:LED-10MM (layer F.Cu) (tedit 5751267F)
    (at 44.45 -104.14)
    (descr "LED 10mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 10mm 10MM 100mil 2.54mm")
    (fp_text reference D4 (at 1.2192 3.1496) (layer F.SilkS))
    (fp_text value L-813ID (at 1.5 6.1) (layer F.Fab))
    (fp_text user + (at 2.4511 -2.1971) (layer F.SilkS))
    (fp_text user - (at -0.1016 -2.1717) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /B))
    (model LEDs.3dshapes/LED-10MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.8648 -38.5572 270)
    (attr smd)
    (fp_text reference R23 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /SDA))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J29-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.3784 -64.262)
    (attr smd)
    (fp_text reference R25 (at 0 0.3175) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /A2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.4292 -68.326)
    (attr smd)
    (fp_text reference R26 (at 0 0.3175) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /A3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.3276 -72.2884)
    (attr smd)
    (fp_text reference R27 (at 0 0.3175) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /A4))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.3784 -60.198)
    (attr smd)
    (fp_text reference R28 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 /A1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 29.464 -58.2168 180)
    (attr smd)
    (fp_text reference R29 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 /A1))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.4292 -56.1848)
    (attr smd)
    (fp_text reference R30 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /A0))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.9664 -60.5536 270)
    (attr smd)
    (fp_text reference R31 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /A0))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 24.2316 -4.9276 270)
    (attr smd)
    (fp_text reference R32 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 VDD))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 34.1376 -76.5048 270)
    (attr smd)
    (fp_text reference R15 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 /G))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 15 /LED00))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 37.8968 -76.5048 270)
    (attr smd)
    (fp_text reference R16 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 /F))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 16 /LED01))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 41.5544 -76.5048 270)
    (attr smd)
    (fp_text reference R17 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 5 /A))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 17 /LED02))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 52.6288 -76.4032 270)
    (attr smd)
    (fp_text reference R18 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 8 /C))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 20 /LED05))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 45.2628 -76.5048 270)
    (attr smd)
    (fp_text reference R19 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 4 /B))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 18 /LED03))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 56.134 -76.4032 270)
    (attr smd)
    (fp_text reference R20 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 9 /D))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 21 /LED06))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 48.9204 -76.4032 270)
    (attr smd)
    (fp_text reference R21 (at 0 0 270) (layer B.SilkS))
    (fp_text value 300R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 7 /DP))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 19 /LED04))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 59.7408 -76.4032 270)
    (attr smd)
    (fp_text reference R22 (at 0 0 270) (layer B.SilkS))
    (fp_text value 150R (at 0 0.127 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 6 /E))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 22 /LED07))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 41.7576 -22.098 90)
    (attr smd)
    (fp_text reference R24 (at 0 0 90) (layer B.SilkS))
    (fp_text value 0R (at 0 0.127 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(AFF1-Pad2)"))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 6 /E))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:0 (layer F.Cu) (tedit 57551423)
    (at 43.2816 -25.8572)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mlab_Mechanical:0 (layer F.Cu) (tedit 5755144C)
    (at 35.4584 -25.6032)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mlab_Mechanical:0 (layer F.Cu) (tedit 57554315)
    (at 24.638 -55.118)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Mlab_Mechanical:0 (layer F.Cu) (tedit 5755431E)
    (at 34.3916 -59.1312)
    (fp_text reference J3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (gr_text 2016 (at 8.4836 -125.0188) (layer B.Cu))
  (gr_text JACHO (at 8.5852 -127.508) (layer B.Cu))
  (gr_text LED7SEG01A (at 78.8416 -124.2568) (layer B.Cu))
  (gr_text MLAB.CZ (at 78.6384 -126.5936) (layer B.Cu))
  (gr_text MLAB.CZ (at 55.2196 -59.5376) (layer F.SilkS))
  (gr_text LED7SEG01A (at 55.2196 -56.8452) (layer F.SilkS))
  (gr_text JACHO (at 58.0136 -99.568) (layer F.SilkS))
  (gr_text 2016 (at 58.0136 -96.8756) (layer F.SilkS))
  (gr_text "VDD MAX 5V" (at 42.418 -53.6448) (layer F.SilkS))
  (gr_text E (at 53.9496 -87.5284 90) (layer F.SilkS))
  (gr_text D (at 51.4096 -87.5284 90) (layer F.SilkS))
  (gr_text C (at 48.8696 -87.5284 90) (layer F.SilkS))
  (gr_text DP (at 46.2788 -87.5284 90) (layer F.SilkS))
  (gr_text B (at 43.7896 -87.5284 90) (layer F.SilkS))
  (gr_text A (at 41.2496 -87.5792 90) (layer F.SilkS))
  (gr_text F (at 38.7096 -87.5284 90) (layer F.SilkS))
  (gr_text G (at 36.1696 -87.5284 90) (layer F.SilkS))
  (gr_text +12V (at 31.1404 -96.4184 90) (layer F.SilkS))
  (gr_text +12V (at 28.0416 -78.3336 90) (layer F.SilkS))
  (gr_text LED07 (at 53.8988 -68.3768 90) (layer F.SilkS))
  (gr_text LED06 (at 51.3588 -68.3768 90) (layer F.SilkS))
  (gr_text LED05 (at 48.8188 -68.3768 90) (layer F.SilkS))
  (gr_text LED04 (at 46.2788 -68.3768 90) (layer F.SilkS))
  (gr_text LED03 (at 43.7388 -68.3768 90) (layer F.SilkS))
  (gr_text LED02 (at 41.1988 -68.3768 90) (layer F.SilkS))
  (gr_text LED01 (at 38.6588 -68.3768 90) (layer F.SilkS))
  (gr_text LED00 (at 36.1188 -68.3768 90) (layer F.SilkS))
  (gr_text "#OE" (at 48.6664 -47.9044 90) (layer F.SilkS))
  (gr_text GND (at 44.5008 -47.8536 90) (layer F.SilkS))
  (gr_text SDA (at 36.9824 -47.8536 90) (layer F.SilkS))
  (gr_text VDD (at 39.4716 -47.8536 90) (layer F.SilkS))
  (gr_text SCL (at 42.0116 -47.8028 90) (layer F.SilkS))
  (gr_text LED7SEG01A (at 64.2112 -4.318) (layer F.SilkS))
  (gr_text 2016 (at 76.8096 -4.318) (layer F.SilkS))
  (gr_text JACHO (at 76.8096 -7.0104) (layer F.SilkS))
  (gr_text MLAB.CZ (at 64.2112 -7.0104) (layer F.SilkS))
  (gr_text "VDD MAX 5V" (at 49.276 -8.9916) (layer F.SilkS))
  (gr_text GND (at 25.908 -4.9276 90) (layer F.SilkS))
  (gr_text GND (at 41.402 -4.9784 90) (layer F.SilkS))
  (gr_text VDD (at 33.4772 -1.2192) (layer F.SilkS))
  (gr_text SCL (at 36.1188 -8.9408) (layer F.SilkS))
  (gr_text SDA (at 30.988 -8.9408) (layer F.SilkS))
  (gr_text +12V (at 16.256 -8.9408) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -141.986) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.186 -0.254) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.186 -141.986) (end 91.186 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -141.986) (end 91.186 -141.986) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.2004 -146.2532) (xy 99.6696 -146.2532) (xy 99.6696 6.1468) (xy -5.4864 6.1468) (xy -5.4864 -146.2532)
        (xy -3.302 -146.2532)
      )
    )
  )
)
