(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 145)
    (no_connects 0)
    (area 95.25 88.9 178.054001 141.478001)
    (thickness 1.6)
    (drawings 42)
    (tracks 798)
    (zones 0)
    (modules 74)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 1.3)
    (trace_clearance 0.25)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /OUT1)
  (net 4 /OUT2)
  (net 5 /OUT3)
  (net 6 /OUT4)
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(J4-Pad2)")
  (net 9 "Net-(J6-Pad2)")
  (net 10 "Net-(J8-Pad2)")
  (net 11 /SDA)
  (net 12 /SCL)
  (net 13 /A0)
  (net 14 /A1)
  (net 15 /IN1-)
  (net 16 /IN1+)
  (net 17 /IN2+)
  (net 18 /IN3+)
  (net 19 /IN4+)
  (net 20 /IN2-)
  (net 21 /IN3-)
  (net 22 /IN4-)
  (net 23 /IN1_2+)
  (net 24 /IN2_2+)
  (net 25 /IN1_2-)
  (net 26 /IN2_2-)
  (net 27 /IN3_2+)
  (net 28 /IN4_2+)
  (net 29 /IN3_2-)
  (net 30 /IN4_2-)
  (net 31 "Net-(C2-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.25)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.3)
    (add_net /A0)
    (add_net /A1)
    (add_net /IN1+)
    (add_net /IN1-)
    (add_net /IN1_2+)
    (add_net /IN1_2-)
    (add_net /IN2+)
    (add_net /IN2-)
    (add_net /IN2_2+)
    (add_net /IN2_2-)
    (add_net /IN3+)
    (add_net /IN3-)
    (add_net /IN3_2+)
    (add_net /IN3_2-)
    (add_net /IN4+)
    (add_net /IN4-)
    (add_net /IN4_2+)
    (add_net /IN4_2-)
    (add_net /OUT1)
    (add_net /OUT2)
    (add_net /OUT3)
    (add_net /OUT4)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J8-Pad2)")
    (add_net VCC)
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 6.5405 -25.654 180)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /IN1_2+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 38.354 -25.4)
    (attr smd)
    (fp_text reference R17 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 /IN3_2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 38.354 -22.86 180)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 /IN3_2+))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 41.8719 -24.8412)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /IN3_2-))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /OUT3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57F34C16)
    (at 45.466 -28.702)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 0) (layer B.SilkS))
    (fp_text value TLC27L2ID (at 0 -3.5) (layer B.SilkS))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /OUT3))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /IN3_2-))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 27 /IN3_2+))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /IN4_2+))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /IN4_2-))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /OUT4))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Housings_SOIC/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 40.5384 -35.9283 90)
    (attr smd)
    (fp_text reference R22 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /A0))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 10.6299 -22.86 180)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT1))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /IN1_2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34BDE)
    (at 4.8768 -19.1516 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D4 (at 4.1656 0.0508 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 23 /IN1_2+))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 24.892 -27.4955 270)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 24.892 -31.1785 90)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 20.066 -26.67)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /IN2_2+))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 13.5636 -24.4856 270)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 16.51 -22.86)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT2))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /IN2_2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 53.086 -24.384)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 /IN4_2+))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 41.91 -22.606 180)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /OUT3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /IN3_2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 49.022 -24.7904)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /OUT4))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /IN4_2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-MiniMELF_Standard (layer B.Cu) (tedit 57F342D4)
    (at 21.59 -36.322 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value BZV55C (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34BD9)
    (at 12.3444 -19.23034 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 3.99034 -0.1016 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 25 /IN1_2-))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34BA0)
    (at 14.986 -19.304 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 4.064 -0.254 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 26 /IN2_2-))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34BEF)
    (at 24.2316 -19.28114 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D5 (at 4.04114 -0.1524 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 24 /IN2_2+))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard locked (layer B.Cu) (tedit 57F34BFA)
    (at 45.0596 -19.17954 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D6 (at 4.19354 -0.1524 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 29 /IN3_2-))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34C00)
    (at 47.498 -19.2532 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D7 (at 4.2672 -0.254 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 30 /IN4_2-))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34BF4)
    (at 35.814 -18.288 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D8 (at 0 2.286 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 27 /IN3_2+))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 57F34C0F)
    (at 54.864 -19.304 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D9 (at 4.318 0 270) (layer B.SilkS))
    (fp_text value BAS85 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 270) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 270) (layer B.SilkS))
    (pad 1 smd rect (at 1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -1.75006 0 270) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 28 /IN4_2+))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 13.462 -15.24 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /IN1-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 20.066 -15.24 270)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 270) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /IN2-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 42.418 -15.494 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /IN3-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 48.514 -15.494 270)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at 0 -3.81 270) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J8-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /IN4-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57F342D4)
    (at 43.18 -35.814 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A0))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57F342D4)
    (at 45.72 -35.814 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A1))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 57F342D4)
    (at 30.988 -35.814 90)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J13 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value JUMP_5X2 (at 0 7.62 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SDA))
    (pad 4 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SDA))
    (pad 5 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 6 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 7 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SCL))
    (pad 8 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /SCL))
    (pad 9 thru_hole rect (at -1.27 5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole rect (at 1.27 5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57F342D4)
    (at 55.88 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57F342D4)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57F342D4)
    (at 55.88 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57F342D4)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 10.2108 -20.066 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /IN1_2-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /IN1-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 7.6708 -20.066 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /IN1_2+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /IN1+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 17.526 -20.066 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /IN2_2-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 /IN2-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 20.066 -20.066 270)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /IN2_2+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 /IN2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 6.5405 -23.114)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 /IN1_2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 20.066 -24.13 180)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 /IN2_2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 10.6299 -24.892)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 /IN1_2-))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 16.51 -25.146 180)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 /IN2_2-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 42.926 -19.558 270)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 /IN3_2-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 /IN3-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 40.386 -19.558 270)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 /IN3_2+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 /IN3+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 49.784 -19.304 270)
    (attr smd)
    (fp_text reference R15 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /IN4_2-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 /IN4-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 52.07 -19.304 270)
    (attr smd)
    (fp_text reference R16 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 180K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 /IN4_2+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 /IN4+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 53.086 -26.67 180)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 /IN4_2+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 49.022 -22.86 180)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 33K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /IN4_2-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /OUT4))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 48.514 -35.814 90)
    (attr smd)
    (fp_text reference R21 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /A1))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 28.702 -32.004 180)
    (attr smd)
    (fp_text reference R23 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 32.258 -32.004)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57F34BE3)
    (at 13.208 -29.21)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -0.254) (layer B.SilkS))
    (fp_text value TLC27L2ID (at 0 -3.5) (layer B.SilkS))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT1))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 25 /IN1_2-))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 23 /IN1_2+))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 /IN2_2+))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 /IN2_2-))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT2))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Housings_SOIC/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOIC-14 (layer B.Cu) (tedit 57F342D4)
    (at 31.242 -25.654 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value MCP3424 (at 0 -1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -3.81 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT1))
    (pad 2 smd rect (at -2.54 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 4 /OUT2))
    (pad 4 smd rect (at 0 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.27 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.54 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at 3.81 -3.302 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 11 /SDA))
    (pad 8 smd rect (at 3.81 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 12 /SCL))
    (pad 9 smd rect (at 2.54 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 13 /A0))
    (pad 11 smd rect (at 0 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 5 /OUT3))
    (pad 12 smd rect (at -1.27 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -2.54 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 6 /OUT4))
    (pad 14 smd rect (at -3.81 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.27 3.048 90) (size 0.6 1.143) (layers B.Cu B.Paste B.Mask)
      (net 14 /A1))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 45.466 -24.13 270)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 27.94 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 22.86 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J15 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /IN2-))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /IN2-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 25.4 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J16 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /IN2+))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /IN2+))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 20.32 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J17 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 38.608 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J18 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /IN3-))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /IN3-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 36.068 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J19 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /IN3+))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /IN3+))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 48.768 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J20 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 43.688 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J21 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /IN4-))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 22 /IN4-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 46.228 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J22 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /IN4+))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /IN4+))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 33.528 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J23 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57F342D4)
    (at 41.148 -5.08 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 12.7 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 17.78 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /IN1-))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /IN1-))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57F342D4)
    (at 15.24 -5.08)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /IN1+))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /IN1+))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57F342D4)
    (at 22.606 -31.9405 270)
    (attr smd)
    (fp_text reference L1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value BLM21PG300SN1D (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 57F342D4)
    (at 11.938 -11.684)
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer B.SilkS))
    (fp_text value 249R (at 0 0.127) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 16 /IN1+))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 57F342D4)
    (at 23.368 -11.684 180)
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer B.SilkS))
    (fp_text value 249R (at 0 0.127 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 17 /IN2+))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J4-Pad2)"))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 57F342D4)
    (at 37.846 -11.938)
    (attr smd)
    (fp_text reference R11 (at 0 0) (layer B.SilkS))
    (fp_text value 249R (at 0 0.127) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J6-Pad2)"))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 18 /IN3+))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 57F342D4)
    (at 49.784 -11.684 180)
    (attr smd)
    (fp_text reference R12 (at 0 0 180) (layer B.SilkS))
    (fp_text value 249R (at 0 0.127 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 19 /IN4+))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J8-Pad2)"))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text IN3+ (at 36.068 -8.128 90) (layer F.SilkS))
  (gr_text "SET CUR\nMEASUR" (at 5.588 -15.24) (layer F.SilkS))
  (gr_text VCAI2C01A (at 8.89 -28.702) (layer F.SilkS))
  (gr_text MLAB.CZ (at 58.928 -12.7 90) (layer B.Cu))
  (gr_text 2016 (at 56.134 -12.7 90) (layer B.Cu))
  (gr_text JACHO (at 55.626 -12.446 90) (layer F.SilkS))
  (gr_text 2016 (at 57.912 -12.446 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 8.89 -30.988) (layer F.SilkS))
  (gr_text "X: 0x8C" (at 35.052 -19.304) (layer F.SilkS))
  (gr_text "XY 0x6E" (at 35.052 -17.018) (layer F.SilkS))
  (gr_text ":Y 0x6A" (at 35.052 -21.59) (layer F.SilkS))
  (gr_text ":: 0x68" (at 35.052 -23.876) (layer F.SilkS))
  (gr_text ADDRESS (at 26.924 -26.416) (layer F.SilkS))
  (gr_text Y (at 45.72 -31.242 90) (layer F.SilkS))
  (gr_text X (at 43.18 -31.242 90) (layer F.SilkS))
  (gr_text "SET ADR" (at 40.132 -35.052 90) (layer F.SilkS))
  (gr_text GND (at 36.068 -33.02 90) (layer F.SilkS))
  (gr_text SCL (at 33.528 -33.02 90) (layer F.SilkS))
  (gr_text VCC (at 30.988 -33.02 90) (layer F.SilkS))
  (gr_text SDA (at 28.448 -33.02 90) (layer F.SilkS))
  (gr_text GND (at 25.908 -33.02 90) (layer F.SilkS))
  (gr_text I4 (at 48.514 -18.034) (layer F.SilkS))
  (gr_text I3 (at 42.418 -18.288) (layer F.SilkS))
  (gr_text I2 (at 20.066 -18.034) (layer F.SilkS))
  (gr_text I1 (at 13.462 -18.034) (layer F.SilkS))
  (gr_text GND (at 48.768 -8.128 90) (layer F.SilkS))
  (gr_text IN4+ (at 46.228 -8.128 90) (layer F.SilkS))
  (gr_text IN4- (at 43.688 -8.128 90) (layer F.SilkS))
  (gr_text GND (at 41.148 -8.128 90) (layer F.SilkS))
  (gr_text IN3- (at 38.608 -8.128 90) (layer F.SilkS))
  (gr_text GND (at 33.528 -8.128 90) (layer F.SilkS))
  (gr_text GND (at 27.94 -8.128 90) (layer F.SilkS))
  (gr_text IN2+ (at 25.4 -8.128 90) (layer F.SilkS))
  (gr_text IN2- (at 22.86 -8.128 90) (layer F.SilkS))
  (gr_text GND (at 20.32 -8.128 90) (layer F.SilkS))
  (gr_text IN1- (at 17.78 -8.128 90) (layer F.SilkS))
  (gr_text GND (at 12.7 -8.128 90) (layer F.SilkS))
  (gr_text IN1+ (at 15.24 -8.128 90) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 60.706 -0.254) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.706 -0.254) (end 60.706 -40.386) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 60.706 -40.386) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy -2.032 -42.418) (xy 64.008 -42.672) (xy 63.5 2.032) (xy -8.636 4.064)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 67.31 -44.196) (xy 65.786 6.35) (xy -13.97 7.874) (xy -15.494 -44.704)
      )
    )
  )
)
