(kicad_pcb (version 20170123) (host pcbnew "(2017-02-05 revision 431abcf)-makepkg")
  (general
    (links 59)
    (no_connects 0)
    (area 0.178999 -40.461001 20.141001 -0.178999)
    (thickness 1.6)
    (drawings 23)
    (tracks 252)
    (zones 0)
    (modules 26)
    (nets 9)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /SDA)
  (net 4 /SCL)
  (net 5 /A0)
  (net 6 /A1)
  (net 7 /A2)
  (net 8 /WP)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.25)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /WP)
    (add_net GND)
    (add_net VCC)
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 58C13C26)
    (at 15.748 -11.176 270)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J9 (at 0 -5.08 270) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0 5.08 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54 270) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /WP))
    (pad 1 thru_hole rect (at 0 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:TSSOP-8_4.4x3mm_Pitch0.65mm placed (layer B.Cu) (tedit 586A28E5)
    (at 15.6972 -14.8844 180)
    (descr "8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 0 180) (layer B.SilkS))
    (fp_text value EEPROM_TSSOP8 (at 0 -2.55 180) (layer B.Fab) hide)
    (fp_text user * (at -1.8669 0.8509 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.95 0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /A0))
    (pad 2 smd rect (at -2.95 0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 /A1))
    (pad 3 smd rect (at -2.95 -0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 /A2))
    (pad 4 smd rect (at -2.95 -0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.95 -0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 /SDA))
    (pad 6 smd rect (at 2.95 -0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 /SCL))
    (pad 7 smd rect (at 2.95 0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /WP))
    (pad 8 smd rect (at 2.95 0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Housings_SSOP.3dshapes/TSSOP-8_4.4x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:MSOP-8_3x3mm_Pitch0.65mm (layer B.Cu) (tedit 586A28E5)
    (at 16.51 -20.9804 180)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0.127 0 180) (layer B.SilkS))
    (fp_text value EEPROM_MSOP8 (at 0 -2.6 180) (layer B.SilkS) hide)
    (fp_text user * (at -1.1049 0.7747 180) (layer B.SilkS))
    (pad 1 smd rect (at -2.2 0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /A0))
    (pad 2 smd rect (at -2.2 0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 /A1))
    (pad 3 smd rect (at -2.2 -0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 /A2))
    (pad 4 smd rect (at -2.2 -0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.2 -0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 /SDA))
    (pad 6 smd rect (at 2.2 -0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 /SCL))
    (pad 7 smd rect (at 2.2 0.325 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /WP))
    (pad 8 smd rect (at 2.2 0.975 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/MSOP_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A28E5)
    (at 15.24 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A28E5)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A28E5)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 586A28E5)
    (at 15.24 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 15.6464 -24.13)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 14.2875 -17.8816)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.9568 -31.0896 90)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.9187 -17.8308 180)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -29.337)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -26.797)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SDA))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SDA))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -24.257)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -21.717)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SCL))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SCL))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -19.177)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -15.748 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -13.208 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 586A28E5)
    (at 4.953 -10.668 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A2))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.7155 -12.4968 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /A0))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.7409 -10.5664 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /A1))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.144 -25.6032 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /SDA))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.7155 -8.5344 180)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /A2))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 586A28E5)
    (at 9.144 -22.1488 90)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SO-8 (layer B.Cu) (tedit 586A28E5)
    (at 15.3924 -28.2956 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 270) (layer B.SilkS))
    (fp_text value EEPROM_SO8 (at 0 0 270) (layer B.SilkS) hide)
    (pad 8 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 7 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 8 /WP))
    (pad 6 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 4 /SCL))
    (pad 5 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 /SDA))
    (pad 4 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 7 /A2))
    (pad 2 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 6 /A1))
    (pad 1 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 5 /A0))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-MiniMELF_Standard (layer B.Cu) (tedit 586A28E5)
    (at 11.684 -21.59 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value BZV55C-5,6V (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 18.288 -12.7 90) (layer F.SilkS))
  (gr_text VCC (at 13.208 -12.7 90) (layer F.SilkS))
  (dimension 19.812 (width 0.3) (layer Dwgs.User)
    (gr_text "0,7800 in" (at 10.16 -43.1076) (layer Dwgs.User))
    (feature1 (pts (xy 20.066 -40.386) (xy 20.066 -44.4576)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.254 -44.4576)))
    (crossbar (pts (xy 0.254 -41.7576) (xy 20.066 -41.7576)))
    (arrow1a (pts (xy 20.066 -41.7576) (xy 18.939496 -41.171179)))
    (arrow1b (pts (xy 20.066 -41.7576) (xy 18.939496 -42.344021)))
    (arrow2a (pts (xy 0.254 -41.7576) (xy 1.380504 -41.171179)))
    (arrow2b (pts (xy 0.254 -41.7576) (xy 1.380504 -42.344021)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 25.3784 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 20.066 -40.386) (xy 26.7284 -40.386)))
    (feature2 (pts (xy 20.066 -0.254) (xy 26.7284 -0.254)))
    (crossbar (pts (xy 24.0284 -0.254) (xy 24.0284 -40.386)))
    (arrow1a (pts (xy 24.0284 -40.386) (xy 24.614821 -39.259496)))
    (arrow1b (pts (xy 24.0284 -40.386) (xy 23.441979 -39.259496)))
    (arrow2a (pts (xy 24.0284 -0.254) (xy 24.614821 -1.380504)))
    (arrow2b (pts (xy 24.0284 -0.254) (xy 23.441979 -1.380504)))
  )
  (gr_text JACHO (at 10.033 -35.687 90) (layer F.SilkS))
  (gr_text "MLAB.CZ\nEEPROM02A" (at 14.732 -24.511 90) (layer F.SilkS))
  (gr_text WP (at 15.748 -12.7 90) (layer F.SilkS))
  (gr_text A2 (at 7.62 -10.668) (layer F.SilkS))
  (gr_text A1 (at 7.62 -13.208) (layer F.SilkS))
  (gr_text A0 (at 7.62 -15.748) (layer F.SilkS))
  (gr_text VCC (at 1.397 -13.335 90) (layer F.SilkS))
  (gr_text SCL (at 7.62 -21.717) (layer F.SilkS))
  (gr_text VCC (at 7.62 -24.257) (layer F.SilkS))
  (gr_text GND (at 7.62 -29.337) (layer F.SilkS))
  (gr_text SDA (at 7.62 -26.797) (layer F.SilkS))
  (gr_text 2017 (at 10.16 -5.08 90) (layer F.SilkS))
  (gr_text 2017 (at 10.16 -3.683 90) (layer B.Cu))
  (gr_text MLAB (at 10.033 -36.322 90) (layer B.Cu))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 20.066 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.066 -40.386) (end 20.066 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 20.066 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.876 -43.942) (xy 23.876 2.54) (xy -7.239 3.556) (xy -4.572 -44.831)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.676 -42.545) (xy 73.66 1.524) (xy -2.921 1.524) (xy -1.651 -43.434)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.9464 -24.9936) (xy 7.0612 -24.9936) (xy 9.906 -24.9936) (xy 10.8204 -23.9776) (xy 12.5476 -23.9776)
        (xy 13.3604 -24.7904) (xy 15.1384 -24.7904) (xy 15.1384 -21.7424) (xy 13.5636 -21.7424) (xy 12.6492 -22.6568)
        (xy 7.5184 -22.6568) (xy 6.858 -23.3172) (xy 2.9464 -23.3172)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.414 -18.542) (xy 13.7668 -18.542) (xy 13.7668 -15.6464) (xy 11.9888 -15.6464) (xy 10.414 -17.1704)
      )
    )
  )
)
