(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu15.10.1-stable)
  (general
    (links 126)
    (no_connects 0)
    (area 126.165 69.667 180.212 118.320714)
    (thickness 1.6)
    (drawings 48)
    (tracks 367)
    (zones 0)
    (modules 55)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.7)
    (via_min_drill 0.3)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x011f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 /INA+)
  (net 2 /OUTA)
  (net 3 /INA-)
  (net 4 /VIN+)
  (net 5 GNDA)
  (net 6 VCC)
  (net 7 /VIN-)
  (net 8 VSS)
  (net 9 /INB+)
  (net 10 /OUTB)
  (net 11 /INB-)
  (net 12 GND)
  (net 13 /VREFA)
  (net 14 /VREFB)
  (net 15 "Net-(U1-Pad3)")
  (net 16 "Net-(U1-Pad1)")
  (net 17 "Net-(U1-Pad2)")
  (net 18 "Net-(U1-Pad6)")
  (net 19 "Net-(U1-Pad7)")
  (net 20 "Net-(U1-Pad5)")
  (net 21 "Net-(b0-Pad2)")
  (net 22 "Net-(b8-Pad2)")
  (net 23 "Net-(c1-Pad2)")
  (net 24 "Net-(c7-Pad2)")
  (net 25 /1)
  (net 26 /5)
  (net 27 /3)
  (net 28 /6)
  (net 29 /4)
  (net 30 /2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /1)
    (add_net /2)
    (add_net /3)
    (add_net /4)
    (add_net /5)
    (add_net /6)
    (add_net /INA+)
    (add_net /INA-)
    (add_net /INB+)
    (add_net /INB-)
    (add_net /OUTA)
    (add_net /OUTB)
    (add_net /VIN+)
    (add_net /VIN-)
    (add_net /VREFA)
    (add_net /VREFB)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(b0-Pad2)")
    (add_net "Net-(b8-Pad2)")
    (add_net "Net-(c1-Pad2)")
    (add_net "Net-(c7-Pad2)")
    (add_net VCC)
    (add_net VSS)
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 5798E7D0)
    (at 162.56 96.52 180)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J4 (at 0 -7.62 180) (layer F.SilkS) hide)
    (fp_text value OPAMPB (at -3.683 0.127 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /INB+))
    (pad 2 thru_hole rect (at 1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /INB+))
    (pad 3 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /VREFB))
    (pad 4 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /VREFB))
    (pad 5 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /INB-))
    (pad 6 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /INB-))
    (pad 7 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /OUTB))
    (pad 8 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /OUTB))
    (pad 9 thru_hole rect (at -1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 10 thru_hole rect (at 1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6BD)
    (at 158.75 96.52 90)
    (attr smd)
    (fp_text reference b9 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 11 /INB-))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(b8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SO-8 (layer F.Cu) (tedit 5479A0C5)
    (at 147.32 96.52 270)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 270) (layer F.SilkS))
    (fp_text value OZ (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd oval (at -1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
    (pad 2 smd oval (at -0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 3 smd oval (at 0.635 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 4 smd oval (at 1.905 2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 8 VSS))
    (pad 5 smd oval (at 1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (pad 6 smd oval (at 0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (pad 7 smd oval (at -0.635 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (pad 8 smd oval (at -1.905 -2.794 270) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6D8)
    (at 138.43 100.965 270)
    (attr smd)
    (fp_text reference c1 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 /INA+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(c1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E619)
    (at 140.97 92.075 270)
    (attr smd)
    (fp_text reference a2 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E5FD)
    (at 135.89 92.075 90)
    (attr smd)
    (fp_text reference a0 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 /OUTA))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E68C)
    (at 135.89 96.52 270)
    (attr smd)
    (fp_text reference b0 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 /INA-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(b0-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E62D)
    (at 146.05 92.075 90)
    (attr smd)
    (fp_text reference a4 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E635)
    (at 148.59 92.075 90)
    (attr smd)
    (fp_text reference a5 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6F2)
    (at 143.51 100.965 90)
    (attr smd)
    (fp_text reference c3 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 8 VSS))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E730)
    (at 146.05 100.965 90)
    (attr smd)
    (fp_text reference c4 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 25 /1))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 26 /5))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E738)
    (at 148.59 100.965 90)
    (attr smd)
    (fp_text reference c5 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 27 /3))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 26 /5))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E63F)
    (at 151.13 92.075 270)
    (attr smd)
    (fp_text reference a6 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E749)
    (at 153.67 100.965 270)
    (attr smd)
    (fp_text reference c7 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 9 /INB+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(c7-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E660)
    (at 158.75 92.075 90)
    (attr smd)
    (fp_text reference a9 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 10 /OUTB))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6A9)
    (at 153.67 96.52 90)
    (attr smd)
    (fp_text reference b7 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 157.48 111.76 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J1 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 5798E35A)
    (at 147.32 81.28 270)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J2 (at 0 -7.62 270) (layer F.SilkS) hide)
    (fp_text value POWER (at -3.556 0 360) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 2 thru_hole rect (at 1.27 -5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 3 thru_hole rect (at -1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /VIN-))
    (pad 4 thru_hole rect (at 1.27 -2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /VIN-))
    (pad 5 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VIN+))
    (pad 6 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VIN+))
    (pad 7 thru_hole rect (at -1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /VIN-))
    (pad 8 thru_hole rect (at 1.27 2.54 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /VIN-))
    (pad 9 thru_hole rect (at -1.27 5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 10 thru_hole rect (at 1.27 5.08 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 5798E2F6)
    (at 132.08 96.52 180)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J3 (at 0 -7.62 180) (layer F.SilkS) hide)
    (fp_text value OPAMPA (at 3.81 5.207 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /INA+))
    (pad 2 thru_hole rect (at 1.27 -5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /INA+))
    (pad 3 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /VREFA))
    (pad 4 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /VREFA))
    (pad 5 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /INA-))
    (pad 6 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /INA-))
    (pad 7 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /OUTA))
    (pad 8 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 /OUTA))
    (pad 9 thru_hole rect (at -1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 10 thru_hole rect (at 1.27 5.08 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 132.08 111.76 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 12 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 132.08 81.28 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 12 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 162.56 111.76 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 12 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 162.56 81.28 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 12 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6E0)
    (at 140.97 100.965 90)
    (attr smd)
    (fp_text reference c2 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /VREFA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E69D)
    (at 140.97 96.52 270)
    (attr smd)
    (fp_text reference b2 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /VREFA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E76F)
    (at 135.89 105.41 90)
    (attr smd)
    (fp_text reference d0 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(c1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E777)
    (at 138.43 105.41 270)
    (attr smd)
    (fp_text reference d1 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E623)
    (at 143.51 92.075 90)
    (attr smd)
    (fp_text reference a3 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E780)
    (at 140.97 105.41 270)
    (attr smd)
    (fp_text reference d2 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E695)
    (at 138.43 96.52 270)
    (attr smd)
    (fp_text reference b1 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(b0-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E60D)
    (at 138.43 92.075 270)
    (attr smd)
    (fp_text reference a1 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E34D)
    (at 149.225 85.344 180)
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value R (at 0.127 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 /VIN+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E33F)
    (at 145.415 85.344 180)
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer F.SilkS))
    (fp_text value R (at 0.127 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 8 VSS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 7 /VIN-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E7AF)
    (at 156.21 105.41 90)
    (attr smd)
    (fp_text reference d8 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(c7-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E64A)
    (at 153.67 92.075 90)
    (attr smd)
    (fp_text reference a7 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E7A8)
    (at 153.67 105.41 90)
    (attr smd)
    (fp_text reference d7 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E740)
    (at 151.13 100.965 90)
    (attr smd)
    (fp_text reference c6 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 /VREFB))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E754)
    (at 156.21 100.965 90)
    (attr smd)
    (fp_text reference c8 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 /VREFB))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E7B6)
    (at 158.75 105.41 90)
    (attr smd)
    (fp_text reference d9 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6B3)
    (at 156.21 96.52 270)
    (attr smd)
    (fp_text reference b8 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(b8-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E655)
    (at 156.21 92.075 270)
    (attr smd)
    (fp_text reference a8 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer F.Cu) (tedit 5798E3B9)
    (at 138.43 82.423 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 4.826 0.127 90) (layer F.SilkS))
    (fp_text value M4 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user A (at -3.29946 1.6002 90) (layer F.SilkS))
    (fp_text user K (at 2.99974 1.69926 90) (layer F.SilkS))
    (pad 2 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 /VIN-))
    (pad 1 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer F.Cu) (tedit 5798E3A5)
    (at 156.21 82.55 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at -4.826 0 270) (layer F.SilkS))
    (fp_text value M4 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text user A (at -3.29946 1.6002 270) (layer F.SilkS))
    (fp_text user K (at 2.99974 1.69926 270) (layer F.SilkS))
    (pad 2 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 1 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 /VIN+))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E6C7)
    (at 135.89 100.965 270)
    (attr smd)
    (fp_text reference c0 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /VREFA))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5798E760)
    (at 158.75 100.965 270)
    (attr smd)
    (fp_text reference c9 (at 0 -0.3175 270) (layer F.SilkS) hide)
    (fp_text value C (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 /VREFB))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sot23-6:TantalC_SizeC_Reflow (layer F.Cu) (tedit 5798E50E)
    (at 161.544 87.884)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C1 (at 0.0127 0.0381) (layer F.SilkS))
    (fp_text value 47u (at -0.09906 3.59918) (layer F.SilkS) hide)
    (fp_text user + (at -4.572 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 4 /VIN+))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module sot23-6:TantalC_SizeC_Reflow (layer F.Cu) (tedit 5798E50E)
    (at 133.604 87.884)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0.0127 0.0381) (layer F.SilkS))
    (fp_text value 47u (at -0.09906 3.59918) (layer F.SilkS) hide)
    (fp_text user + (at -4.572 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 7 /VIN-))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module sot23-6:TantalC_SizeC_Reflow (layer F.Cu) (tedit 5798E50E)
    (at 152.4 87.884)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C3 (at 0.0127 0.0381) (layer F.SilkS))
    (fp_text value 47u (at -0.09906 3.59918) (layer F.SilkS) hide)
    (fp_text user + (at -4.572 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module sot23-6:TantalC_SizeC_Reflow (layer F.Cu) (tedit 5798E50E)
    (at 143.256 87.884)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C4 (at 0.0127 0.0381) (layer F.SilkS))
    (fp_text value 47u (at -0.09906 3.59918) (layer F.SilkS) hide)
    (fp_text user + (at -4.572 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 8 VSS))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x08 (layer F.Cu) (tedit 57A77AF5)
    (at 146.05 111.76 270)
    (descr "pin header straight 2x08")
    (tags "pin header straight 2x08")
    (fp_text reference J5 (at 0 -11.43 270) (layer F.SilkS) hide)
    (fp_text value SOT23-6 (at 0 11.43 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -8.89 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -8.89 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 2 thru_hole rect (at 1.27 -8.89 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 GNDA))
    (pad 3 thru_hole rect (at -1.27 -6.35 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /6))
    (pad 4 thru_hole rect (at 1.27 -6.35 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 28 /6))
    (pad 5 thru_hole rect (at -1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /5))
    (pad 6 thru_hole rect (at 1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 26 /5))
    (pad 7 thru_hole rect (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 /4))
    (pad 8 thru_hole rect (at 1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 29 /4))
    (pad 9 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /3))
    (pad 10 thru_hole rect (at 1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /3))
    (pad 11 thru_hole rect (at -1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /2))
    (pad 12 thru_hole rect (at 1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /2))
    (pad 13 thru_hole rect (at -1.27 6.35 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /1))
    (pad 14 thru_hole rect (at 1.27 6.35 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 25 /1))
    (pad 15 thru_hole rect (at -1.27 8.89 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (pad 16 thru_hole rect (at 1.27 8.89 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 57A77DB5)
    (at 143.51 105.41 90)
    (attr smd)
    (fp_text reference d3 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 VCC))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 30 /2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 57A77DBF)
    (at 151.13 105.41 90)
    (attr smd)
    (fp_text reference d6 (at 0 -0.3175 90) (layer F.SilkS) hide)
    (fp_text value R (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 28 /6))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOT-23-6 (layer F.Cu) (tedit 57A77B32)
    (at 147.193 105.664 270)
    (fp_text reference U3 (at 1.99898 0 360) (layer F.SilkS) hide)
    (fp_text value "ANALOG SWITCH" (at 0.0635 0 270) (layer F.SilkS) hide)
    (pad 6 smd rect (at -0.9525 -1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 28 /6))
    (pad 5 smd rect (at 0 -1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 /5))
    (pad 4 smd rect (at 0.9525 -1.27 270) (size 0.50104 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 29 /4))
    (pad 3 smd rect (at 0.9525 1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 27 /3))
    (pad 2 smd rect (at 0 1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 /2))
    (pad 1 smd rect (at -0.9525 1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 /1))
    (model MLAB_3D/IO/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module sot23-6:SOT-23-3 (layer F.Cu) (tedit 57A77B2E)
    (at 147.193 105.664 90)
    (fp_text reference Q1 (at 1.99898 0 180) (layer F.SilkS) hide)
    (fp_text value BC846 (at 0.0635 0 90) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 -1.27 90) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 /2))
    (pad 2 smd rect (at 0.9525 1.27 90) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 28 /6))
    (pad 1 smd rect (at -0.9525 1.27 90) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 29 /4))
    (model MLAB_3D/IO/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (module sot23-6:SOT-23-3 (layer F.Cu) (tedit 57A77B36)
    (at 147.193 105.664 270)
    (fp_text reference U2 (at 1.99898 0 360) (layer F.SilkS) hide)
    (fp_text value MAX6066 (at 0.0635 0 270) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 -1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 /5))
    (pad 2 smd rect (at 0.9525 1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 27 /3))
    (pad 1 smd rect (at -0.9525 1.27 270) (size 0.5 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 /1))
    (model MLAB_3D/IO/SOT23_6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.11 0.11 0.11))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 139.7 107.95) (layer B.SilkS))
  (gr_text MLAB.CZ (at 147.32 92.71) (layer B.SilkS))
  (gr_text 6 (at 152.4 107.95) (layer B.SilkS))
  (gr_text 5 (at 149.86 107.95) (layer B.SilkS))
  (gr_text 4 (at 147.32 107.95) (layer B.SilkS))
  (gr_text 3 (at 144.78 107.95) (layer B.SilkS))
  (gr_text 2 (at 142.24 107.95) (layer B.SilkS))
  (gr_text "POWER IN" (at 147.32 77.724) (layer B.SilkS))
  (gr_text gnda (at 152.146 86.233 90) (layer B.SilkS))
  (gr_text vin- (at 149.733 86.106 90) (layer B.SilkS))
  (gr_text vin+ (at 147.193 86.106 90) (layer B.SilkS))
  (gr_text vin- (at 144.653 86.106 90) (layer B.SilkS))
  (gr_text gnda (at 141.986 86.233 90) (layer B.SilkS))
  (gr_text gnd (at 157.48 114.935) (layer B.SilkS))
  (gr_text gnda (at 157.48 107.95 90) (layer B.SilkS))
  (gr_text d (at 128.27 105.283) (layer F.SilkS))
  (gr_text c (at 128.27 100.711) (layer F.SilkS))
  (gr_text b (at 128.27 96.266) (layer F.SilkS))
  (gr_text a (at 128.27 91.821) (layer F.SilkS))
  (gr_text 9 (at 158.75 108.204) (layer F.SilkS))
  (gr_text 8 (at 156.21 108.204) (layer F.SilkS))
  (gr_text 7 (at 153.67 108.204) (layer F.SilkS))
  (gr_text 6 (at 151.13 108.204) (layer F.SilkS))
  (gr_text 5 (at 148.59 108.204) (layer F.SilkS))
  (gr_text 4 (at 146.05 108.204) (layer F.SilkS))
  (gr_text 3 (at 143.51 108.204) (layer F.SilkS))
  (gr_text 2 (at 140.97 108.204) (layer F.SilkS))
  (gr_text 1 (at 138.43 108.204) (layer F.SilkS))
  (gr_text 0 (at 135.89 108.204) (layer F.SilkS))
  (dimension 40.386 (width 0.3) (layer Dwgs.User)
    (gr_text "40.386 mm" (at 173.562 96.52 270) (layer Dwgs.User))
    (feature1 (pts (xy 167.513 116.713) (xy 174.912 116.713)))
    (feature2 (pts (xy 167.513 76.327) (xy 174.912 76.327)))
    (crossbar (pts (xy 172.212 76.327) (xy 172.212 116.713)))
    (arrow1a (pts (xy 172.212 116.713) (xy 171.625579 115.586496)))
    (arrow1b (pts (xy 172.212 116.713) (xy 172.798421 115.586496)))
    (arrow2a (pts (xy 172.212 76.327) (xy 171.625579 77.453504)))
    (arrow2b (pts (xy 172.212 76.327) (xy 172.798421 77.453504)))
  )
  (dimension 40.386 (width 0.3) (layer Dwgs.User)
    (gr_text "40.386 mm" (at 147.32 71.167) (layer Dwgs.User))
    (feature1 (pts (xy 167.513 76.327) (xy 167.513 69.817)))
    (feature2 (pts (xy 127.127 76.327) (xy 127.127 69.817)))
    (crossbar (pts (xy 127.127 72.517) (xy 167.513 72.517)))
    (arrow1a (pts (xy 167.513 72.517) (xy 166.386496 73.103421)))
    (arrow1b (pts (xy 167.513 72.517) (xy 166.386496 71.930579)))
    (arrow2a (pts (xy 127.127 72.517) (xy 128.253504 73.103421)))
    (arrow2b (pts (xy 127.127 72.517) (xy 128.253504 71.930579)))
  )
  (gr_line (start 127.254 116.586) (end 127.254 76.454) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.386 116.586) (end 127.254 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.386 76.454) (end 167.386 116.586) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.254 76.454) (end 167.386 76.454) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text OZDUAL03A (at 147.574 89.535) (layer B.SilkS))
  (gr_text vcc (at 137.16 107.95 90) (layer B.SilkS))
  (gr_text gnda (at 154.94 107.315 90) (layer B.SilkS))
  (gr_text inb+ (at 157.48 101.6) (layer B.SilkS))
  (gr_text Vrefb (at 157.48 99.06) (layer B.SilkS))
  (gr_text inb- (at 157.48 96.52) (layer B.SilkS))
  (gr_text outb (at 157.48 93.98) (layer B.SilkS))
  (gr_text gnda (at 157.48 91.44) (layer B.SilkS))
  (gr_text ina+ (at 137.414 101.854) (layer B.SilkS))
  (gr_text Vrefa (at 137.16 99.06) (layer B.SilkS))
  (gr_text ina- (at 137.16 96.52) (layer B.SilkS))
  (gr_text outa (at 137.16 93.98) (layer B.SilkS))
  (gr_text gnda (at 136.906 91.44) (layer B.SilkS))
  (zone (net 12) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 116.84) (xy 127 116.84) (xy 127 76.2) (xy 167.64 76.2) (xy 167.64 116.84)
      )
    )
    (polygon
      (pts        (xy 135.89 77.47) (xy 128.27 85.09) (xy 128.27 107.95) (xy 135.89 115.57) (xy 157.0355 115.57)
        (xy 157.0355 112.395) (xy 157.861 112.395) (xy 157.861 115.57) (xy 158.75 115.57) (xy 166.37 107.95)
        (xy 166.37 85.09) (xy 158.75 77.47) (xy 135.89 77.47)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 116.84) (xy 127 116.84) (xy 127 76.2) (xy 167.64 76.2) (xy 167.64 116.84)
      )
    )
    (polygon
      (pts        (xy 135.89 77.47) (xy 128.27 85.09) (xy 128.27 107.95) (xy 135.89 115.57) (xy 157.0355 115.57)
        (xy 157.0355 112.395) (xy 157.861 112.395) (xy 157.861 115.57) (xy 158.75 115.57) (xy 166.37 107.95)
        (xy 166.37 85.09) (xy 158.75 77.47) (xy 135.89 77.47)
      )
    )
  )
  (zone (net 5) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.905 87.3125) (xy 128.905 107.6325) (xy 136.2075 114.935) (xy 156.2735 114.935) (xy 156.2735 111.76)
        (xy 157.7975 111.76) (xy 158.369 111.76) (xy 158.369 114.935) (xy 158.4325 114.935) (xy 165.735 107.6325)
        (xy 165.735 85.4075) (xy 158.4325 78.105) (xy 136.2075 78.105) (xy 128.905 85.4075) (xy 128.905 87.3125)
      )
    )
  )
  (zone (net 5) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.905 87.3125) (xy 128.905 107.6325) (xy 136.2075 114.935) (xy 156.2735 114.935) (xy 156.2735 111.76)
        (xy 157.7975 111.76) (xy 158.369 111.76) (xy 158.369 114.935) (xy 158.4325 114.935) (xy 165.735 107.6325)
        (xy 165.735 85.4075) (xy 158.4325 78.105) (xy 136.2075 78.105) (xy 128.905 85.4075) (xy 128.905 87.3125)
      )
    )
  )
)
