(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 47)
    (no_connects 0)
    (area 0.205999 -40.434001 40.434001 -0.205999)
    (thickness 1.6)
    (drawings 25)
    (tracks 185)
    (zones 0)
    (modules 31)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.81 3.81)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /Vin)
  (net 3 /Vout)
  (net 4 /FB)
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(Q1-Pad4)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.15)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /FB)
    (add_net /Vin)
    (add_net /Vout)
    (add_net GND)
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(Q1-Pad4)")
  )
  (module Hrebinky:Pin_Header_Straight_2x04 placed (layer F.Cu) (tedit 5478C15F)
    (at 14.605 -35.687)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 5.0165 -11.7475) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 1.27 0) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Vin))
    (pad 6 thru_hole rect (at 1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Vin))
    (pad 1 thru_hole rect (at -3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at -1.27 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Vin))
    (pad 4 thru_hole rect (at 3.81 1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole rect (at 3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Vin))
    (pad 8 thru_hole rect (at -3.81 -1.27) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5478C1A4)
    (at 22.1615 -7.3025 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J4 (at -13.7795 1.016 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole rect (at 1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /FB))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5478C1A2)
    (at 19.6215 -7.3025 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J5 (at -13.462 0.4445 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole rect (at 1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /FB))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5478C19F)
    (at 17.0815 -7.3025 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J6 (at -13.462 0.1905 90) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole rect (at 1.27 0.127 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 /FB))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Hrebinky:Pin_Header_Straight_2x04 placed (layer F.Cu) (tedit 5478C16E)
    (at 26.035 -36.187 180)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J9 (at -0.8255 9.652 180) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 1.27 0 180) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 1.27 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /Vout))
    (pad 6 thru_hole rect (at 1.27 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /Vout))
    (pad 1 thru_hole rect (at -3.81 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at -1.27 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /Vout))
    (pad 4 thru_hole rect (at 3.81 1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole rect (at 3.81 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 /Vout))
    (pad 8 thru_hole rect (at -3.81 -1.27 180) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Dira:MountingHole_3mm placed (layer F.Cu) (tedit 54345FDC)
    (at 35.56 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0.1778 -0.0762) (layer F.SilkS))
    (fp_text value _ (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module MLAB_L:DE1205-10 (layer B.Cu) (tedit 54785DDA)
    (at 30.988 -16.121 180)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (fp_text reference L1 (at 0 5.842 180) (layer B.SilkS))
    (fp_text value "22uH DE1207-22" (at 0 -5.842 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 5 0 180) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -5 0 180) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /Vout))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_CON:WAGO256 (layer F.Cu) (tedit 5478C184)
    (at 32.766 -29.591 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J3 (at -17.4625 -9.906 180) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at -3.1115 18.0975 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module MLAB_CON:WAGO256 (layer F.Cu) (tedit 5478C187)
    (at 32.766 -24.5745 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J7 (at -18.7325 -8.3185 180) (layer F.SilkS) hide)
    (fp_text value Vout+ (at -15.875 24.511 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 /Vout))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 /Vout))
  )
  (module MLAB_CON:WAGO256 (layer F.Cu) (tedit 5478C155)
    (at 7.8105 -28.0035)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J2 (at -12.827 -3.556) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at -24.9555 -1.016) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Vin))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Vin))
  )
  (module MLAB_CON:WAGO256 (layer F.Cu) (tedit 5478C158)
    (at 7.8105 -22.987)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J8 (at -17.653 -5.6515) (layer F.SilkS) hide)
    (fp_text value Vout- (at -24.1935 -2.667) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module MLAB_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 550A6CC3)
    (at 13.97 -15.875 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C1 (at -0.127 0 90) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vin))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 12.7 -9.652 270)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 6.35 -17.272)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 25.781 -6.5452 180)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100pF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.9855 -5.6515 270)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 470pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 54799D12)
    (at 25.654 -27.813 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C6 (at 0.1016 -0.1016 90) (layer B.SilkS))
    (fp_text value 100uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908 90) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0 90) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.175 0 90) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 3 /Vout))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 550A6CBC)
    (at 20.701 -27.94 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C7 (at 0 -0.127 90) (layer B.SilkS))
    (fp_text value 100uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908 90) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0 90) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.175 0 90) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 3 /Vout))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_D:Diode-SMA_Standard (layer B.Cu) (tedit 54799A7E)
    (at 15.621 -28.956 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0.0762 90) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vin))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_D:Diode-SMA_Standard (layer B.Cu) (tedit 54799A7E)
    (at 19.812 -20.701)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0.2794 -0.127 270) (layer B.SilkS))
    (fp_text value 15MQ040N (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SO-8 (layer B.Cu) (tedit 5479A0C5)
    (at 20.066 -15.748 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference Q1 (at -0.2032 -0.127 90) (layer B.SilkS))
    (fp_text value IRF7416 (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.905 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vin))
    (pad 2 smd oval (at -0.635 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vin))
    (pad 3 smd oval (at 0.635 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vin))
    (pad 4 smd oval (at 1.905 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q1-Pad4)"))
    (pad 5 smd oval (at 1.905 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 6 smd oval (at 0.635 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 7 smd oval (at -0.635 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 8 smd oval (at -1.905 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 6.35 -19.431)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 22k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 19.685 -2.921 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 20k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.145 -2.921 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 11k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 22.352 -2.921 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:MSOP-8_3x3mm_Pitch0.65mm (layer B.Cu) (tedit 5493B8D8)
    (at 9.398 -12.827 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0.127 0 90) (layer B.SilkS))
    (fp_text value LM3485 (at 0 -2.6 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 /FB))
    (pad 5 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q1-Pad4)"))
    (pad 8 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 /Vin))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/MSOP_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module graphics:QR_code (layer F.Cu) (tedit 55007D9E)
    (at 31.9024 -15.4686 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 550A6D9D)
    (at 25.7302 -8.1534 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -0.0508 -0.0254 180) (layer B.SilkS))
    (fp_text value 33k (at 0 -2.1 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask))
    (model Resistors_SMD/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 47.7812 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -40.386) (xy 49.1312 -40.386)))
    (feature2 (pts (xy 40.386 -0.254) (xy 49.1312 -0.254)))
    (crossbar (pts (xy 46.4312 -0.254) (xy 46.4312 -40.386)))
    (arrow1a (pts (xy 46.4312 -40.386) (xy 47.017621 -39.259496)))
    (arrow1b (pts (xy 46.4312 -40.386) (xy 45.844779 -39.259496)))
    (arrow2a (pts (xy 46.4312 -0.254) (xy 47.017621 -1.380504)))
    (arrow2b (pts (xy 46.4312 -0.254) (xy 45.844779 -1.380504)))
  )
  (dimension 40.132008 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 20.325098 -48.428157 359.9637369) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -40.3606) (xy 40.391953 -49.765457)))
    (feature2 (pts (xy 0.254 -40.386) (xy 0.259953 -49.790857)))
    (crossbar (pts (xy 0.258244 -47.090858) (xy 40.390244 -47.065458)))
    (arrow1a (pts (xy 40.390244 -47.065458) (xy 39.263369 -46.47975)))
    (arrow1b (pts (xy 40.390244 -47.065458) (xy 39.264112 -47.652592)))
    (arrow2a (pts (xy 0.258244 -47.090858) (xy 1.384376 -46.503724)))
    (arrow2b (pts (xy 0.258244 -47.090858) (xy 1.385119 -47.676566)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 44.5808 -20.32 90) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -40.386) (xy 45.9308 -40.386)))
    (feature2 (pts (xy 40.386 -0.254) (xy 45.9308 -0.254)))
    (crossbar (pts (xy 43.2308 -0.254) (xy 43.2308 -40.386)))
    (arrow1a (pts (xy 43.2308 -40.386) (xy 43.817221 -39.259496)))
    (arrow1b (pts (xy 43.2308 -40.386) (xy 42.644379 -39.259496)))
    (arrow2a (pts (xy 43.2308 -0.254) (xy 43.817221 -1.380504)))
    (arrow2b (pts (xy 43.2308 -0.254) (xy 42.644379 -1.380504)))
  )
  (dimension 40.132032 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 20.314111 -45.012818 0.07252626444) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -40.386) (xy 40.378402 -46.388217)))
    (feature2 (pts (xy 0.254 -40.3352) (xy 0.246402 -46.337417)))
    (crossbar (pts (xy 0.24982 -43.637419) (xy 40.38182 -43.688219)))
    (arrow1a (pts (xy 40.38182 -43.688219) (xy 39.256059 -43.100373)))
    (arrow1b (pts (xy 40.38182 -43.688219) (xy 39.254575 -44.273213)))
    (arrow2a (pts (xy 0.24982 -43.637419) (xy 1.377065 -43.052425)))
    (arrow2b (pts (xy 0.24982 -43.637419) (xy 1.375581 -44.225265)))
  )
  (gr_text - (at 38.9382 -33.1978 90) (layer F.SilkS))
  (gr_text - (at 1.5748 -19.0754 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 30.2895 -5.5245 90) (layer B.Cu))
  (gr_text BATPOWER04C (at 1.6002 -14.0208 270) (layer B.Cu))
  (gr_text 2015 (at 28.0035 -4.7625) (layer F.SilkS))
  (gr_text JACHO (at 27.94 -6.6675) (layer F.SilkS))
  (gr_text BATPOWER04C (at 7.7978 -11.684) (layer F.SilkS))
  (gr_text MLAB.cz (at 7.6962 -13.8684) (layer F.SilkS))
  (gr_text 5V-16V (at 11.684 -31.75) (layer F.SilkS))
  (gr_text "VAR\n" (at 22.225 -4.445 90) (layer F.SilkS))
  (gr_text 3.3V (at 19.685 -4.445 90) (layer F.SilkS))
  (gr_text 5V (at 17.145 -4.318 90) (layer F.SilkS))
  (gr_text "SET OUTPUT" (at 19.7485 -10.922) (layer F.SilkS))
  (gr_text + (at 38.8112 -21.0058) (layer F.SilkS))
  (gr_text + (at 1.7018 -31.6738) (layer F.SilkS))
  (gr_text "POWER OUT" (at 25.9334 -39.5224) (layer F.SilkS))
  (gr_text "POWER IN" (at 14.6685 -39.1795) (layer F.SilkS))
  (gr_line (start 0.256 -0.256) (end 0.256 -40.384) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -0.256) (end 40.384 -0.256) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.384 -40.384) (end 40.384 -0.256) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.256 -40.384) (end 40.384 -40.384) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name "Net-(D2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.32 -21.844) (xy 20.32 -18.288) (xy 21.971 -18.288) (xy 21.971 -12.573) (xy 27.813 -12.573)
        (xy 27.813 -18.796) (xy 24.384 -21.844)
      )
    )
  )
  (zone (net 3) (net_name /Vout) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37.846 -12.446) (xy 30.607 -12.446) (xy 28.067 -12.446) (xy 28.067 -18.796) (xy 23.622 -22.86)
        (xy 19.05 -22.86) (xy 19.05 -26.67) (xy 27.432 -26.67) (xy 37.592 -26.67) (xy 37.846 -26.67)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.762 -41.402) (xy 42.545 -41.402) (xy 42.672 1.27) (xy -0.762 1.143)
      )
    )
  )
  (zone (net 2) (net_name /Vin) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.034 -12.065) (xy 15.748 -12.065) (xy 13.843 -10.033) (xy 0.762 -10.033) (xy 0.762 -30.48)
        (xy 4.953 -30.48) (xy 4.953 -32.004) (xy 12.446 -32.004) (xy 12.446 -37.973) (xy 17.018 -37.973)
        (xy 17.018 -29.718) (xy 12.5095 -29.718) (xy 12.5095 -25.781) (xy 3.048 -25.781) (xy 3.048 -20.447)
        (xy 6.731 -20.447) (xy 6.731 -14.224) (xy 10.033 -14.224) (xy 10.033 -16.002) (xy 16.129 -16.002)
        (xy 16.129 -18.288) (xy 18.034 -18.288)
      )
    )
  )
  (zone (net 3) (net_name /Vout) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37.4015 -26.9748) (xy 37.3888 -22.5044) (xy 24.3586 -22.5044) (xy 23.749 -23.233) (xy 23.749 -38.346)
        (xy 28.2956 -38.354) (xy 28.2956 -26.9748)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.2225 -42.799) (xy -2.2225 2.0955) (xy 47.371 2.54) (xy 47.371 -42.799)
      )
    )
  )
)
