(kicad_pcb (version 20170123) (host pcbnew "(2017-02-05 revision 431abcf)-makepkg")
  (general
    (links 49)
    (no_connects 0)
    (area -8.913285 -44.323 56.007001 6.858001)
    (thickness 1.6)
    (drawings 10)
    (tracks 291)
    (zones 0)
    (modules 22)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /OUT)
  (net 4 /ADJ)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ADJ)
    (add_net /OUT)
    (add_net GND)
    (add_net VCC)
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54BBE393)
    (at 5.334 -29.21 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C1 (at 0 3.556 180) (layer B.SilkS))
    (fp_text value CP (at 0 -3.556 180) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936 180) (layer B.SilkS))
    (pad 2 smd rect (at 1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5494 0 180) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 4.826 -29.21 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0.0127 -0.0381 180) (layer B.SilkS))
    (fp_text value CP (at -0.09906 -3.59918 180) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 180) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 6.858 -25.908 180)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.636 -13.716 270)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 22.098 -12.7 270)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 23.876 -29.972)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeB_Reflow (layer B.Cu) (tedit 54BBE393)
    (at 25.4 -22.86)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C7 (at 0 3.556) (layer B.SilkS))
    (fp_text value CP (at 0 -3.556) (layer B.SilkS) hide)
    (fp_text user + (at -3.59918 2.49936) (layer B.SilkS))
    (pad 1 smd rect (at -1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (pad 2 smd rect (at 1.5494 0) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 25.654 -26.67)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C8 (at 0.0127 -0.0381) (layer B.SilkS))
    (fp_text value CP (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016) (layer B.SilkS))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 56BDB339)
    (at 5.08 -22.606)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 56BDB339)
    (at 13.462 -19.812 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (pad 1 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 4.826 -15.24)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value HEADER_2x04_PARALLEL (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 25.908 -14.986)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J2 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value HEADER_2x04_PARALLEL (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /OUT))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /OUT))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /OUT))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /OUT))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 19.304 -19.812)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value R (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /ADJ))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 20.574 -22.606 90)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /ADJ))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:D2PAK-TO-263-2Lead (layer B.Cu) (tedit 58B40229)
    (at 15.24 -10.414 270)
    (descr "D2PAK / TO-263 3-lead smd package")
    (tags "D2PAK D2PAK-3 TO-263AB TO-263")
    (attr smd)
    (fp_text reference U1 (at 0 6.4 90) (layer B.SilkS))
    (fp_text value L78_DPAK_D2PAK (at 0 -6.45 270) (layer B.Fab))
    (pad 4 smd rect (at 4.58 0 270) (size 9.4 10.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -4.58 -2.54 270) (size 4.6 1.39) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (pad 1 smd rect (at -4.58 2.54 270) (size 4.6 1.39) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/TO-263-3Lead.wrl
      (at (xyz -0.18 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:SOT-223 (layer B.Cu) (tedit 0)
    (at 14.986 -28.956 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0.762 180) (layer B.SilkS))
    (fp_text value LM1117_ADJ_SOT (at 0 -0.762 180) (layer B.Fab))
    (pad 4 smd rect (at 0 3.302 180) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (pad 2 smd rect (at 0 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (pad 3 smd rect (at 2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 4 /ADJ))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:D2PAK-TO-263-2Lead (layer B.Cu) (tedit 58B66603)
    (at 15.24 -28.956 90)
    (descr "D2PAK / TO-263 3-lead smd package")
    (tags "D2PAK D2PAK-3 TO-263AB TO-263")
    (attr smd)
    (fp_text reference U3 (at 0 6.4 -90) (layer B.SilkS))
    (fp_text value LM317M_LM217_DPAK_D2PAK (at 0 -6.45 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -4.58 2.54 90) (size 4.6 1.39) (layers B.Cu B.Paste B.Mask)
      (net 4 /ADJ))
    (pad 3 smd rect (at -4.58 -2.54 90) (size 4.6 1.39) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 4.58 0 90) (size 9.4 10.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (model TO_SOT_Packages_SMD.3dshapes/TO-263-3Lead.wrl
      (at (xyz -0.18 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:DPAK-TO-252-2Lead (layer B.Cu) (tedit 58B66606)
    (at 15.24 -28.702 90)
    (descr "TO-252-2Lead DPAK")
    (attr smd)
    (fp_text reference U4 (at 0.3 4.54 90) (layer B.SilkS))
    (fp_text value LM317M_LM217_DPAK_D2PAK (at 0.25 -4.81 90) (layer B.Fab) hide)
    (pad 4 smd rect (at 3.7 -0.01 180) (size 7 7) (layers B.Cu B.Paste B.Mask)
      (net 3 /OUT))
    (pad 3 smd rect (at -3.7 -2.29 180) (size 2 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -3.7 2.29 180) (size 2 3.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /ADJ))
    (model TO_SOT_Packages_SMD.3dshapes\TO-252-2Lead.wrl
      (at (xyz -0.1377952755905512 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "POWER OUT" (at 21.844 -16.51 90) (layer F.SilkS))
  (gr_text "MLAB.CZ\nLINREG01A" (at 14.986 -24.638) (layer F.SilkS))
  (gr_text 2017 (at 25.4 -29.718) (layer F.SilkS))
  (gr_text JACHO (at 5.08 -29.718) (layer F.SilkS))
  (gr_text "Vout\n3.3V\n5.0V\nADJ\n" (at 15.24 -16.51) (layer F.SilkS))
  (gr_text "POWER IN" (at 8.89 -15.748 90) (layer F.SilkS))
  (gr_line (start 0.254 -40.386) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30.226 -0.254) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.016 -41.148) (xy 54.102 -43.942) (xy 49.53 2.794) (xy -2.032 2.032)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.943 6.858) (xy -6.604 4.064) (xy -2.54 -42.672) (xy 56.007 -44.323)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.54 -12.954) (xy 7.366 -12.954) (xy 13.97 -12.954) (xy 13.97 -17.526) (xy 12.954 -18.796)
        (xy 12.954 -20.828) (xy 12.954 -26.924) (xy 8.89 -30.988) (xy 5.588 -30.988) (xy 5.588 -27.686)
        (xy 6.604 -27.686) (xy 7.112 -27.178) (xy 7.112 -17.526) (xy 2.54 -17.526)
      )
    )
  )
  (zone (net 3) (net_name /OUT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.224 -12.446) (xy 14.224 -27.432) (xy 12.954 -28.702) (xy 9.652 -28.702) (xy 9.652 -38.354)
        (xy 20.828 -38.354) (xy 20.828 -30.988) (xy 23.622 -30.988) (xy 23.622 -28.956) (xy 24.638 -28.956)
        (xy 25.146 -28.448) (xy 25.146 -21.082) (xy 25.146 -20.828) (xy 25.146 -17.272) (xy 28.194 -17.272)
        (xy 28.194 -12.446)
      )
    )
    (polygon
      (pts        (xy 22.352 -24.384) (xy 21.59 -25.146) (xy 21.59 -28.448) (xy 17.526 -28.448) (xy 16.002 -26.924)
        (xy 16.002 -22.098) (xy 17.272 -20.828) (xy 19.05 -20.828) (xy 19.05 -18.542) (xy 21.59 -18.542)
        (xy 21.59 -19.558) (xy 22.352 -20.32)
      )
    )
  )
  (zone (net 3) (net_name /OUT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9.906 -28.956) (xy 20.066 -28.956) (xy 20.066 -38.1) (xy 9.906 -38.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9.906 -28.956) (xy 20.066 -28.956) (xy 20.066 -38.1) (xy 9.906 -38.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9.906 -10.16) (xy 21.082 -10.16) (xy 21.082 -1.016) (xy 9.906 -1.016)
      )
    )
  )
)
