(kicad_pcb (version 4) (host pcbnew "(2015-01-07 BZR 5359)-product")
  (general
    (links 210)
    (no_connects 0)
    (area 94.818999 56.083999 175.691001 116.636001)
    (thickness 1.6)
    (drawings 31)
    (tracks 805)
    (zones 0)
    (modules 96)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.18)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.89)
    (trace_clearance 0.18)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.18)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.89)
    (via_drill 0.5)
    (via_min_size 0.89)
    (via_min_drill 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 /BAT+)
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 /CMODE)
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 /REGIN)
  (net 12 "Net-(C13-Pad1)")
  (net 13 "Net-(C13-Pad2)")
  (net 14 "Net-(C14-Pad1)")
  (net 15 "Net-(C17-Pad1)")
  (net 16 "Net-(D3-Pad1)")
  (net 17 /PG)
  (net 18 "Net-(D4-Pad1)")
  (net 19 "Net-(D4-Pad2)")
  (net 20 "Net-(D5-Pad1)")
  (net 21 /STAT1)
  (net 22 "Net-(D6-Pad2)")
  (net 23 "Net-(D7-Pad2)")
  (net 24 "Net-(D8-Pad2)")
  (net 25 "Net-(D9-Pad2)")
  (net 26 "Net-(D10-Pad2)")
  (net 27 "Net-(D11-Pad2)")
  (net 28 "Net-(D12-Pad2)")
  (net 29 "Net-(D13-Pad2)")
  (net 30 /CE)
  (net 31 /CELLS)
  (net 32 "Net-(L1-Pad1)")
  (net 33 "Net-(Q1-PadG)")
  (net 34 "Net-(Q3-PadD)")
  (net 35 "Net-(Q3-PadG)")
  (net 36 "Net-(Q4-PadD)")
  (net 37 "Net-(Q4-PadG)")
  (net 38 "Net-(R3-Pad1)")
  (net 39 "Net-(R10-Pad2)")
  (net 40 "Net-(R11-Pad1)")
  (net 41 "Net-(R12-Pad1)")
  (net 42 "Net-(R13-Pad1)")
  (net 43 "Net-(R17-Pad2)")
  (net 44 "Net-(R20-Pad1)")
  (net 45 "Net-(R27-Pad2)")
  (net 46 "Net-(R28-Pad2)")
  (net 47 "Net-(R29-Pad2)")
  (net 48 "Net-(R30-Pad2)")
  (net 49 "Net-(R31-Pad2)")
  (net 50 "Net-(R32-Pad2)")
  (net 51 "Net-(R33-Pad2)")
  (net 52 /P2)
  (net 53 /P1)
  (net 54 /BAT-MIDPOINT)
  (net 55 /BATTERY-)
  (net 56 /BATTERY+)
  (net 57 /SDA)
  (net 58 /SCL)
  (net 59 /HDQ)
  (net 60 "Net-(D14-Pad2)")
  (net 61 "Net-(R34-Pad2)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.18)
    (trace_width 0.18)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /BAT+)
    (add_net /BAT-MIDPOINT)
    (add_net /BATTERY+)
    (add_net /BATTERY-)
    (add_net /CE)
    (add_net /CELLS)
    (add_net /CMODE)
    (add_net /HDQ)
    (add_net /P1)
    (add_net /P2)
    (add_net /PG)
    (add_net /REGIN)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /STAT1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(Q1-PadG)")
    (add_net "Net-(Q3-PadD)")
    (add_net "Net-(Q3-PadG)")
    (add_net "Net-(Q4-PadD)")
    (add_net "Net-(Q4-PadG)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R30-Pad2)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R34-Pad2)")
  )
  (module Mlab_Batery:2LION (layer F.Cu) (tedit 553735D5)
    (at 135.255 86.106)
    (fp_text reference BT1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 2x18650_LION (at 0 0) (layer F.SilkS) hide)
    (fp_text user - (at 22.86 8.89) (layer F.SilkS))
    (fp_text user - (at 22.86 -10.16) (layer F.SilkS))
    (fp_text user + (at -22.86 8.89) (layer F.SilkS))
    (fp_text user + (at -22.86 -10.16) (layer F.SilkS))
    (pad 1 thru_hole rect (at -36.25 -9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 /BAT+))
    (pad 2 thru_hole rect (at 36.25 -9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 54 /BAT-MIDPOINT))
    (pad 3 thru_hole rect (at -36.25 9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 54 /BAT-MIDPOINT))
    (pad 4 thru_hole rect (at 36.25 9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 55 /BATTERY-))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 103.505 89.916 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 553736FB)
    (at 112.014 69.088 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0 0 270) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 270) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 270) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 114.808 73.66 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 103.505 86.233 270)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 107.061 85.344)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 116.332 67.691 90)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /CMODE))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 116.713 73.66 270)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 110.49 86.106 90)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 127.381 68.453 90)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 119.38 94.361 270)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 145.034 92.329 270)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 158.115 93.853 90)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 164.084 99.568 270)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 162.433 90.932 180)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 160.528 99.695 270)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 /BATTERY-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 138.811 83.947 270)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 3n3 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 141.478 96.647 270)
    (attr smd)
    (fp_text reference C18 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 55373700)
    (at 108.077 68.834 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0 90) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 5537370C)
    (at 113.157 78.74 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 0 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736E3)
    (at 119.38 60.96 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0 90) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 17 /PG))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736EB)
    (at 124.46 60.96 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D4 (at 0 0 90) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D4-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736EF)
    (at 129.54 60.96 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D5 (at 0 0 90) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 21 /STAT1))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 5537379A)
    (at 138.811 88.773 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D6 (at 0 0 90) (layer B.SilkS))
    (fp_text value BZV55C-5,6V (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736A0)
    (at 137.16 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D7 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D7-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736A7)
    (at 139.827 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D8 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736AE)
    (at 142.494 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D9 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D9-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736B9)
    (at 145.161 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D10 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D10-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736C9)
    (at 147.828 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D11 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D11-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736CF)
    (at 150.495 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D12 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D12-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553736D4)
    (at 153.162 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D13 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D13-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 55373713)
    (at 106.68 80.518)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F1 (at 0 0) (layer B.SilkS))
    (fp_text value FUSE (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 2 smd rect (at 2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 110.363 60.96 270)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35 270) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 143.637 61.214)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /STAT1))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /STAT1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 133.477 61.214 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PG))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PG))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 138.557 61.214)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /CMODE))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /CMODE))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 141.097 61.214)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CE))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CE))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 136.017 61.214)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CELLS))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CELLS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 130.175 111.76 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J7 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55372F24)
    (at 112.014 108.966)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J8 (at -5.969 0.127) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55372F27)
    (at 112.014 113.919)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J9 (at -5.334 0.127) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 157.48 63.119)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 /SDA))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 /SDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 160.02 63.119)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 /SCL))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 /SCL))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 162.56 63.119)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 /HDQ))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 /HDQ))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 150.495 61.214 270)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J13 (at 0 -6.35 270) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_L:DE1205-10 (layer B.Cu) (tedit 54BBE563)
    (at 122.174 82.931 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (fp_text reference L1 (at 0 5.842 90) (layer B.SilkS))
    (fp_text value DE1205-10 (at 0 -5.842 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 5 0 90) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -5 0 90) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 170.815 111.76)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 99.695 60.96)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 99.695 111.76)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 170.815 60.96)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373750)
    (at 113.538 85.725 180)
    (tags SOT23)
    (fp_text reference Q1 (at 0 0 180) (layer B.SilkS))
    (fp_text value IRLML6244 (at 0.0635 0 180) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad S smd rect (at 0.9525 -1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad G smd rect (at -0.9525 -1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q1-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 553737A9)
    (at 142.367 92.837)
    (tags SOT23)
    (fp_text reference Q2 (at 0 0) (layer B.SilkS))
    (fp_text value MMBF170LT1G (at 0.0635 0) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad S smd rect (at 0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad G smd rect (at -0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373790)
    (at 148.971 86.233 180)
    (tags SOT23)
    (fp_text reference Q3 (at 0 0 180) (layer B.SilkS))
    (fp_text value MMBF170LT1G (at 0.0635 0 180) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(Q3-PadD)"))
    (pad S smd rect (at 0.9525 -1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad G smd rect (at -0.9525 -1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(Q3-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373782)
    (at 144.907 83.82 270)
    (tags SOT23)
    (fp_text reference Q4 (at 0 -0.127 270) (layer B.SilkS))
    (fp_text value BSS83P (at 0.0635 0 270) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(Q4-PadD)"))
    (pad S smd rect (at 0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad G smd rect (at -0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q4-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 101.092 82.931 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 100.457 88.773 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 54 /BAT-MIDPOINT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 100.457 86.487 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 240R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 54 /BAT-MIDPOINT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 141.097 66.294 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /CE))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 131.572 65.532)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /CELLS))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 117.094 64.262 90)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 122.047 64.389 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 127 64.389 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D5-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 111.252 89.154)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 111.633 91.567 180)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q1-PadG)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 120.523 67.691 90)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 7K5 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 118.491 67.691 90)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 7K5 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 128.397 71.247)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 9K31 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 124.714 68.453 270)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 442K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5537367F)
    (at 107.442 76.454)
    (attr smd)
    (fp_text reference R15 (at 0 -2.286) (layer F.SilkS))
    (fp_text value NCP21XV103J03RA (at 0.127 0.381) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512 (layer B.Cu) (tedit 5537376D)
    (at 131.572 82.423 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R16 (at -0.254 1.016 270) (layer B.SilkS))
    (fp_text value 0R1 (at -0.254 -0.762 270) (layer B.Fab))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 55373690)
    (at 163.068 95.758 180)
    (attr smd)
    (fp_text reference R17 (at 0 2.286 180) (layer F.SilkS))
    (fp_text value "10K NTC" (at 0.127 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R17-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 158.115 97.536 90)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 /BATTERY-))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 158.496 90.932 180)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 166.116 102.489 90)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 142.621 89.408)
    (attr smd)
    (fp_text reference R21 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 166.751 93.599 90)
    (attr smd)
    (fp_text reference R22 (at 0 0 90) (layer B.SilkS))
    (fp_text value "0R01 75PPM" (at 0 0.127 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 90) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 55 /BATTERY-))
    (pad 2 smd rect (at 1.651 0 90) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 141.097 83.947 90)
    (attr smd)
    (fp_text reference R23 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value "16k5 25ppm" (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 142.748 80.645 180)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value "divider.1% 25ppm" (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(Q4-PadD)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 149.733 81.153)
    (attr smd)
    (fp_text reference R25 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 165K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q4-PadG)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(Q3-PadD)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 148.844 83.312)
    (attr smd)
    (fp_text reference R26 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q4-PadG)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 137.16 107.188 90)
    (attr smd)
    (fp_text reference R27 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 139.827 107.188 90)
    (attr smd)
    (fp_text reference R28 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 142.494 107.188 90)
    (attr smd)
    (fp_text reference R29 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(R29-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 145.161 107.188 90)
    (attr smd)
    (fp_text reference R30 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R30-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 147.828 107.188 90)
    (attr smd)
    (fp_text reference R31 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R31-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 150.495 107.188 90)
    (attr smd)
    (fp_text reference R32 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R32-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 153.162 107.188 90)
    (attr smd)
    (fp_text reference R33 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R33-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SO-14 (layer B.Cu) (tedit 5534C67E)
    (at 146.304 100.076 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U4 (at 0 0 90) (layer B.SilkS))
    (fp_text value SN74HC164D (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -3.81 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 53 /P1))
    (pad 2 smd oval (at -2.54 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 53 /P1))
    (pad 3 smd oval (at -1.27 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (pad 4 smd oval (at 0 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (pad 11 smd oval (at 0 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R32-Pad2)"))
    (pad 12 smd oval (at -1.27 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R33-Pad2)"))
    (pad 13 smd oval (at -2.54 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R34-Pad2)"))
    (pad 14 smd oval (at -3.81 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 5 smd oval (at 1.27 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(R29-Pad2)"))
    (pad 6 smd oval (at 2.54 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R30-Pad2)"))
    (pad 7 smd oval (at 3.81 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 10 smd oval (at 1.27 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R31-Pad2)"))
    (pad 9 smd oval (at 2.54 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 8 smd oval (at 3.81 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 52 /P2))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 55372ECF)
    (at 161.798 111.252)
    (fp_text reference SW1 (at 0 0.127) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R20-Pad1)"))
    (pad 2 thru_hole rect (at 3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(Q3-PadG)"))
    (pad 1 thru_hole rect (at -3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R20-Pad1)"))
    (pad 2 thru_hole rect (at -3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(Q3-PadG)"))
  )
  (module Mlab_IO:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 553737BB)
    (at 151.384 91.948)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -0.127) (layer B.SilkS))
    (fp_text value BQ34Z100 (at 0 -3.55) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 52 /P2))
    (pad 2 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(Q3-PadG)"))
    (pad 3 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 53 /P1))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (pad 5 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 6 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 7 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (pad 8 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 9 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (pad 10 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R17-Pad2)"))
    (pad 12 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 59 /HDQ))
    (pad 13 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 /SCL))
    (pad 14 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 57 /SDA))
    (model Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:VSON-8 (layer B.Cu) (tedit 55350D0D)
    (at 107.061 88.392 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 90) (layer B.SilkS))
    (fp_text value BQ29209 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user * (at -0.889 -1.524 90) (layer B.SilkS))
    (pad 2 smd rect (at -0.325 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at 0.325 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at 0.975 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 0.975 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0.325 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 7 smd rect (at -0.325 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 8 smd rect (at -0.975 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -0.975 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at 0 0 90) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 5537375C)
    (at 126.873 92.456)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C10 (at 0.127 0.127) (layer B.SilkS))
    (fp_text value 100uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 165.1 63.119)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:VQFN-20 (layer B.Cu) (tedit 553757B7)
    (at 121.666 73.152 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U2 (at 0 0 90) (layer B.SilkS))
    (fp_text value BQ24103 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user * (at -1.651 -1.778 90) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 21 /STAT1))
    (pad 21 smd rect (at 0 0 90) (size 3.05 2.05) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -0.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -0.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 17 /PG))
    (pad 6 smd rect (at 0.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at 0.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 7 /CMODE))
    (pad 8 smd rect (at 1.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R12-Pad1)"))
    (pad 9 smd rect (at 1.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R11-Pad1)"))
    (pad 10 smd rect (at 2.225 -0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 11 smd rect (at 2.225 0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 12 smd rect (at 1.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (pad 13 smd rect (at 1.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 31 /CELLS))
    (pad 14 smd rect (at 0.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad 15 smd rect (at 0.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 16 smd rect (at -0.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 30 /CE))
    (pad 17 smd rect (at -0.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 18 smd rect (at -1.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 19 smd rect (at -1.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D4-Pad2)"))
    (pad 20 smd rect (at -2.225 0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(L1-Pad1)"))
    (pad 1 smd rect (at -2.225 -0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(L1-Pad1)"))
    (pad 21 smd trapezoid (at -2.075 0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -2.075 -0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.075 -0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.075 0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -1.75 0 90) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 1.75 0 90) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.143 0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.143 0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.143 -0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.143 -0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 553517B5)
    (at 155.829 112.395 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D14 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(D14-Pad2)"))
    (pad "" thru_hole circle (at 0 0 90) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 155.829 107.188 90)
    (attr smd)
    (fp_text reference R34 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R34-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "60,452 mm" (at 186.6938 86.36 90) (layer Dwgs.User))
    (feature1 (pts (xy 175.641 56.134) (xy 188.0438 56.134)))
    (feature2 (pts (xy 175.641 116.586) (xy 188.0438 116.586)))
    (crossbar (pts (xy 185.3438 116.586) (xy 185.3438 56.134)))
    (arrow1a (pts (xy 185.3438 56.134) (xy 185.930221 57.260504)))
    (arrow1b (pts (xy 185.3438 56.134) (xy 184.757379 57.260504)))
    (arrow2a (pts (xy 185.3438 116.586) (xy 185.930221 115.459496)))
    (arrow2b (pts (xy 185.3438 116.586) (xy 184.757379 115.459496)))
  )
  (dimension 80.772 (width 0.3) (layer Dwgs.User)
    (gr_text "80,772 mm" (at 135.255 44.9796) (layer Dwgs.User))
    (feature1 (pts (xy 175.641 56.134) (xy 175.641 43.6296)))
    (feature2 (pts (xy 94.869 56.134) (xy 94.869 43.6296)))
    (crossbar (pts (xy 94.869 46.3296) (xy 175.641 46.3296)))
    (arrow1a (pts (xy 175.641 46.3296) (xy 174.514496 46.916021)))
    (arrow1b (pts (xy 175.641 46.3296) (xy 174.514496 45.743179)))
    (arrow2a (pts (xy 94.869 46.3296) (xy 95.995504 46.916021)))
    (arrow2b (pts (xy 94.869 46.3296) (xy 95.995504 45.743179)))
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "2,3800 v" (at 180.6486 86.36 90) (layer Dwgs.User))
    (feature1 (pts (xy 175.641 56.134) (xy 181.9986 56.134)))
    (feature2 (pts (xy 175.641 116.586) (xy 181.9986 116.586)))
    (crossbar (pts (xy 179.2986 116.586) (xy 179.2986 56.134)))
    (arrow1a (pts (xy 179.2986 56.134) (xy 179.885021 57.260504)))
    (arrow1b (pts (xy 179.2986 56.134) (xy 178.712179 57.260504)))
    (arrow2a (pts (xy 179.2986 116.586) (xy 179.885021 115.459496)))
    (arrow2b (pts (xy 179.2986 116.586) (xy 178.712179 115.459496)))
  )
  (dimension 80.772 (width 0.3) (layer Dwgs.User)
    (gr_text "3,1800 v" (at 135.255 50.0596) (layer Dwgs.User))
    (feature1 (pts (xy 175.641 56.134) (xy 175.641 48.7096)))
    (feature2 (pts (xy 94.869 56.134) (xy 94.869 48.7096)))
    (crossbar (pts (xy 94.869 51.4096) (xy 175.641 51.4096)))
    (arrow1a (pts (xy 175.641 51.4096) (xy 174.514496 51.996021)))
    (arrow1b (pts (xy 175.641 51.4096) (xy 174.514496 50.823179)))
    (arrow2a (pts (xy 94.869 51.4096) (xy 95.995504 51.996021)))
    (arrow2b (pts (xy 94.869 51.4096) (xy 95.995504 50.823179)))
  )
  (gr_text LION2CELL01B (at 164.338 85.598) (layer B.Cu))
  (gr_text MLAB.CZ (at 164.211 82.55) (layer B.Cu))
  (gr_text 2015 (at 101.346 103.759) (layer F.SilkS))
  (gr_text JACHO (at 101.346 101.473) (layer F.SilkS))
  (gr_text LION2CELL01B (at 135.255 88.138) (layer F.SilkS))
  (gr_text MLAB.CZ (at 135.255 83.947) (layer F.SilkS))
  (gr_text STAT1 (at 145.796 57.531) (layer F.SilkS))
  (gr_text CE (at 141.097 64.897) (layer F.SilkS))
  (gr_text CMODE (at 138.557 57.531) (layer F.SilkS))
  (gr_text CELLS (at 136.017 64.897) (layer F.SilkS))
  (gr_text PG (at 132.588 57.531) (layer F.SilkS))
  (gr_text "SW POWER" (at 150.495 64.897) (layer F.SilkS))
  (gr_text SDA (at 157.48 60.452 90) (layer F.SilkS))
  (gr_text GND (at 165.1 60.579 90) (layer F.SilkS))
  (gr_text HDQ (at 162.56 60.579 90) (layer F.SilkS))
  (gr_text SCL (at 160.02 60.452 90) (layer F.SilkS))
  (gr_text "POWER IN" (at 110.363 57.404) (layer F.SilkS))
  (gr_text "POWER OUT" (at 130.175 107.95) (layer F.SilkS))
  (gr_text + (at 120.269 108.839) (layer F.SilkS))
  (gr_text "0% ----100%" (at 146.431 108.712) (layer F.SilkS))
  (gr_text CHARGE (at 127 60.96 90) (layer F.SilkS))
  (gr_text DONE (at 122.047 60.833 90) (layer F.SilkS))
  (gr_text ON (at 117.221 60.96 90) (layer F.SilkS))
  (gr_line (start 94.869 116.586) (end 94.869 56.134) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.869 56.134) (end 175.641 56.134) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175.641 116.586) (end 175.641 56.134) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.869 116.586) (end 175.641 116.586) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name "Net-(C2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.823 58.42) (xy 112.903 58.42) (xy 112.903 64.897) (xy 114.808 64.897) (xy 114.808 69.723)
        (xy 115.824 69.723) (xy 118.745 72.39) (xy 120.396 72.39) (xy 120.396 73.152) (xy 120.396 74.676)
        (xy 117.856 74.676) (xy 116.967 73.787) (xy 113.919 73.787) (xy 113.538 73.787) (xy 113.538 70.104)
        (xy 106.553 70.104) (xy 106.553 65.024) (xy 107.696 65.024) (xy 107.696 58.42)
      )
    )
  )
  (zone (net 32) (net_name "Net-(L1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.968 79.629) (xy 119.253 79.629) (xy 119.253 74.676) (xy 120.269 74.676) (xy 120.65 74.93)
        (xy 120.65 74.676) (xy 124.968 74.676)
      )
    )
  )
  (zone (net 10) (net_name "Net-(C10-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.035 63.881) (xy 137.033 79.883) (xy 137.033 89.789) (xy 125.73 89.789) (xy 125.73 94.234)
        (xy 118.491 94.234) (xy 118.491 84.709) (xy 133.858 84.709) (xy 133.858 77.47) (xy 147.955 63.373)
        (xy 147.955 58.928) (xy 153.035 58.928)
      )
    )
  )
  (zone (net 56) (net_name /BATTERY+) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.731 78.232) (xy 133.731 84.328) (xy 112.395 84.328) (xy 111.506 82.55) (xy 107.696 82.55)
        (xy 107.696 78.486) (xy 107.696 78.232)
      )
    )
  )
  (zone (net 1) (net_name /BAT+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.647 74.168) (xy 101.346 74.168) (xy 101.346 76.2) (xy 103.759 78.613) (xy 105.537 78.613)
        (xy 105.537 82.55) (xy 99.949 82.55) (xy 98.679 79.248) (xy 96.647 79.248) (xy 96.647 78.74)
      )
    )
  )
  (zone (net 54) (net_name /BAT-MIDPOINT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.901 97.917) (xy 101.092 97.917) (xy 101.092 90.551) (xy 101.092 85.471) (xy 96.901 85.471)
      )
    )
  )
  (zone (net 56) (net_name /BATTERY+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 114.3) (xy 127.762 114.3) (xy 127.762 108.839) (xy 120.269 108.839) (xy 118.11 110.998)
        (xy 118.11 111.125) (xy 117.983 111.125) (xy 107.442 111.125) (xy 107.442 106.807) (xy 112.268 106.807)
        (xy 112.268 80.01) (xy 107.823 79.756) (xy 107.95 78.74) (xy 115.697 78.867) (xy 118.11 78.867)
        (xy 118.11 101.854) (xy 132.715 101.854) (xy 132.715 114.3)
      )
    )
  )
  (zone (net 11) (net_name /REGIN) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.161 90.424) (xy 149.225 90.424) (xy 149.225 91.567) (xy 147.447 91.567) (xy 146.939 92.075)
        (xy 144.653 92.075) (xy 144.653 90.424)
      )
    )
  )
  (zone (net 55) (net_name /BATTERY-) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.736 98.044) (xy 169.164 98.044) (xy 167.386 96.266) (xy 165.481 96.266) (xy 165.481 93.472)
        (xy 173.736 93.472)
      )
    )
  )
  (zone (net 54) (net_name /BAT-MIDPOINT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.901 98.298) (xy 110.617 98.298) (xy 117.221 91.694) (xy 137.033 91.694) (xy 137.033 78.486)
        (xy 173.863 78.486) (xy 173.863 73.66) (xy 132.207 73.66) (xy 132.207 86.741) (xy 116.459 86.741)
        (xy 109.601 93.599) (xy 96.901 93.599) (xy 96.901 93.98)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.948 54.229) (xy 183.769 54.229) (xy 181.991 120.65) (xy 87.63 122.809)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.106 52.451) (xy 187.96 51.943) (xy 187.071 123.952) (xy 84.074 125.603)
      )
    )
  )
)
