(kicad_pcb (version 4) (host pcbnew "(2015-05-13 BZR 5653)-product")
  (general
    (links 210)
    (no_connects 0)
    (area 106.655601 39.5172 193.929001 143.637001)
    (thickness 1.6)
    (drawings 31)
    (tracks 1083)
    (zones 0)
    (modules 98)
    (nets 64)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.18)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.89)
    (trace_clearance 0.18)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.18)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.89)
    (via_drill 0.5)
    (via_min_size 0.89)
    (via_min_drill 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 /BAT+)
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 /CMODE)
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 /REGIN)
  (net 12 "Net-(C13-Pad1)")
  (net 13 "Net-(C13-Pad2)")
  (net 14 "Net-(C14-Pad1)")
  (net 15 "Net-(C17-Pad1)")
  (net 16 "Net-(D3-Pad1)")
  (net 17 /PG)
  (net 18 "Net-(D4-Pad1)")
  (net 19 "Net-(D4-Pad2)")
  (net 20 "Net-(D5-Pad1)")
  (net 21 /STAT1)
  (net 22 "Net-(D6-Pad2)")
  (net 23 "Net-(D7-Pad2)")
  (net 24 "Net-(D8-Pad2)")
  (net 25 "Net-(D9-Pad2)")
  (net 26 "Net-(D10-Pad2)")
  (net 27 "Net-(D11-Pad2)")
  (net 28 "Net-(D12-Pad2)")
  (net 29 "Net-(D13-Pad2)")
  (net 30 /CE)
  (net 31 /CELLS)
  (net 32 "Net-(L1-Pad1)")
  (net 33 "Net-(Q1-PadG)")
  (net 34 "Net-(Q3-PadD)")
  (net 35 "Net-(Q3-PadG)")
  (net 36 "Net-(Q4-PadD)")
  (net 37 "Net-(Q4-PadG)")
  (net 38 "Net-(R3-Pad1)")
  (net 39 "Net-(R10-Pad2)")
  (net 40 "Net-(R11-Pad1)")
  (net 41 "Net-(R12-Pad1)")
  (net 42 "Net-(R13-Pad1)")
  (net 43 "Net-(R17-Pad2)")
  (net 44 "Net-(R20-Pad1)")
  (net 45 "Net-(R27-Pad2)")
  (net 46 "Net-(R28-Pad2)")
  (net 47 "Net-(R29-Pad2)")
  (net 48 "Net-(R30-Pad2)")
  (net 49 "Net-(R31-Pad2)")
  (net 50 "Net-(R32-Pad2)")
  (net 51 "Net-(R33-Pad2)")
  (net 52 /P2)
  (net 53 /P1)
  (net 54 /BAT-MIDPOINT)
  (net 55 /BATTERY-)
  (net 56 /BATTERY+)
  (net 57 /SDA)
  (net 58 /SCL)
  (net 59 /HDQ)
  (net 60 "Net-(D14-Pad2)")
  (net 61 "Net-(R34-Pad2)")
  (net 62 "Net-(F3-Pad1)")
  (net 63 "Net-(J15-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.18)
    (trace_width 0.18)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /BAT+)
    (add_net /BAT-MIDPOINT)
    (add_net /BATTERY+)
    (add_net /BATTERY-)
    (add_net /CE)
    (add_net /CELLS)
    (add_net /CMODE)
    (add_net /HDQ)
    (add_net /P1)
    (add_net /P2)
    (add_net /PG)
    (add_net /REGIN)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /STAT1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(F3-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(Q1-PadG)")
    (add_net "Net-(Q3-PadD)")
    (add_net "Net-(Q3-PadG)")
    (add_net "Net-(Q4-PadD)")
    (add_net "Net-(Q4-PadG)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R30-Pad2)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R34-Pad2)")
  )
  (module Mlab_Batery:2LION (layer F.Cu) (tedit 553735D5)
    (at 154.432 92.456 90)
    (fp_text reference BT1 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value 2x18650_LION-RESCUE-LION2CELL01C (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user - (at 22.86 8.89 90) (layer F.SilkS))
    (fp_text user - (at 22.86 -10.16 90) (layer F.SilkS))
    (fp_text user + (at -22.86 8.89 90) (layer F.SilkS))
    (fp_text user + (at -22.86 -10.16 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -36.25 -9.65 90) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 /BAT+))
    (pad 2 thru_hole rect (at 36.25 -9.65 90) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 54 /BAT-MIDPOINT))
    (pad 3 thru_hole rect (at -36.25 9.65 90) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 54 /BAT-MIDPOINT))
    (pad 4 thru_hole rect (at 36.25 9.65 90) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 55 /BATTERY-))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 158.242 124.206)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 553736FB)
    (at 138.92276 115.824)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0 0) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 141.986 112.903)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 154.559 124.206)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 153.67 120.65 90)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 330nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 136.017 111.379 180)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /CMODE))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 141.986 110.998)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 154.178 117.348 180)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 136.779 100.33 180)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 162.687 108.331)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 160.655 82.677)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 160.02 70.104)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 167.894 63.627)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 162.814 69.088 90)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 156.718 69.088 90)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 152.273 88.9)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 3n3 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 164.973 86.233)
    (attr smd)
    (fp_text reference C18 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 55373700)
    (at 135.89 121.37898 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0 90) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 5537370C)
    (at 147.066 114.554)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:MiniMELF_Standard (layer B.Cu) (tedit 5537379A)
    (at 157.099 88.9 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D6 (at 0 0 180) (layer B.SilkS))
    (fp_text value BZV55C-5,6V (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 180) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.75006 0 180) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 129.286 117.348)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 129.54 84.074 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /STAT1))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 /STAT1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 129.54 94.234 270)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 270) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 270) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PG))
    (pad 1 thru_hole rect (at 0 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /PG))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 129.54 89.154 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /CMODE))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /CMODE))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 129.54 86.614 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CE))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CE))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 129.54 91.694 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CELLS))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CELLS))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 180.086 97.536 180)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J7 (at 0 -6.35 180) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 4 thru_hole rect (at 1.27 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 5 thru_hole rect (at -1.27 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 6 thru_hole rect (at 1.27 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 7 thru_hole rect (at -1.27 3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55372F24)
    (at 177.292 115.697 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J8 (at -5.969 0.127 90) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BATTERY+))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55372F27)
    (at 182.245 115.697 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J9 (at -5.334 0.127 90) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 131.445 70.231 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 /SDA))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 57 /SDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 131.445 67.691 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 /SCL))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 58 /SCL))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 131.445 65.151 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 /HDQ))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 /HDQ))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 129.54 77.216)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J13 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_L:DE1205-10 (layer B.Cu) (tedit 54BBE563)
    (at 151.257 105.537 180)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (fp_text reference L1 (at 0 5.842 180) (layer B.SilkS))
    (fp_text value DE1205-10 (at 0 -5.842 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 5 0 180) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -5 0 180) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 180.086 56.896 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 129.286 128.016 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 180.086 128.016 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 129.286 56.896 90)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191 90) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373750)
    (at 154.051 114.173 270)
    (tags SOT23)
    (fp_text reference Q1 (at 0 0 270) (layer B.SilkS))
    (fp_text value IRLML6244 (at 0.0635 0 270) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (pad S smd rect (at 0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad G smd rect (at -0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q1-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 553737A9)
    (at 161.163 85.344 90)
    (tags SOT23)
    (fp_text reference Q2 (at 0 0 90) (layer B.SilkS))
    (fp_text value MMBF170LT1G (at 0.0635 0 90) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad S smd rect (at 0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad G smd rect (at -0.9525 -1.09982 90) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373790)
    (at 154.559 78.74 270)
    (tags SOT23)
    (fp_text reference Q3 (at 0 0 270) (layer B.SilkS))
    (fp_text value MMBF170LT1G (at 0.0635 0 270) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(Q3-PadD)"))
    (pad S smd rect (at 0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad G smd rect (at -0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(Q3-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373782)
    (at 152.146 82.804)
    (tags SOT23)
    (fp_text reference Q4 (at 0 -0.127) (layer B.SilkS))
    (fp_text value BSS83P (at 0.0635 0) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(Q4-PadD)"))
    (pad S smd rect (at 0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad G smd rect (at -0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q4-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 151.257 126.619 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 160R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 157.099 127.254 270)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 260R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 54 /BAT-MIDPOINT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 154.813 127.254 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 54 /BAT-MIDPOINT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 134.62 86.614)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0R (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 /CE))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 133.858 96.139 90)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 /CELLS))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 132.588 110.617 180)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 132.715 105.664 180)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 132.715 100.711 180)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D5-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 157.48 116.332 90)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 159.893 116.078 270)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q1-PadG)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 136.017 107.188 180)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 7K5 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 136.017 109.22 180)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 7K5 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 139.573 99.314 90)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 9K31 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 136.779 102.997)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 442K (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5537367F)
    (at 144.78 120.269 90)
    (attr smd)
    (fp_text reference R15 (at 0 -2.286 90) (layer F.SilkS))
    (fp_text value NCP21XV103J03RA (at 0.127 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512 (layer B.Cu) (tedit 5537376D)
    (at 150.749 96.139)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R16 (at -0.254 1.016) (layer B.SilkS))
    (fp_text value 0R1 (at -0.254 -0.762) (layer B.Fab))
    (pad 1 smd rect (at -3.1 0) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(F3-Pad1)"))
    (pad 2 smd rect (at 3.1 0) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 55373690)
    (at 164.084 64.643 270)
    (attr smd)
    (fp_text reference R17 (at 0 2.286 270) (layer F.SilkS))
    (fp_text value "10K NTC" (at 0.127 0.381 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R17-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 160.02 67.564 180)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 /BATTERY-))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 159.258 64.262 270)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 170.815 61.595 180)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 157.734 85.09 90)
    (attr smd)
    (fp_text reference R21 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 54799957)
    (at 161.925 60.96 180)
    (attr smd)
    (fp_text reference R22 (at 0 0 180) (layer B.SilkS))
    (fp_text value "0R01 75PPM" (at 0 0.127 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 55 /BATTERY-))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 152.273 86.614 180)
    (attr smd)
    (fp_text reference R23 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value "16k5 25ppm" (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 148.971 84.963 270)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value "140k .1% 25ppm" (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(Q4-PadD)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 149.479 77.978 90)
    (attr smd)
    (fp_text reference R25 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 165K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q4-PadG)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(Q3-PadD)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 151.638 78.867 90)
    (attr smd)
    (fp_text reference R26 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(Q4-PadG)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 90.551 180)
    (attr smd)
    (fp_text reference R27 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 87.884 180)
    (attr smd)
    (fp_text reference R28 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 85.217 180)
    (attr smd)
    (fp_text reference R29 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(R29-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 82.55 180)
    (attr smd)
    (fp_text reference R30 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R30-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 79.883 180)
    (attr smd)
    (fp_text reference R31 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R31-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 77.216 180)
    (attr smd)
    (fp_text reference R32 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R32-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 74.549 180)
    (attr smd)
    (fp_text reference R33 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R33-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SO-14 (layer B.Cu) (tedit 5534C67E)
    (at 168.402 81.407 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U4 (at 0 0 180) (layer B.SilkS))
    (fp_text value SN74HC164D (at 0 0 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -3.81 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 53 /P1))
    (pad 2 smd oval (at -2.54 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 53 /P1))
    (pad 3 smd oval (at -1.27 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R27-Pad2)"))
    (pad 4 smd oval (at 0 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R28-Pad2)"))
    (pad 11 smd oval (at 0 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(R32-Pad2)"))
    (pad 12 smd oval (at -1.27 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(R33-Pad2)"))
    (pad 13 smd oval (at -2.54 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R34-Pad2)"))
    (pad 14 smd oval (at -3.81 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 5 smd oval (at 1.27 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(R29-Pad2)"))
    (pad 6 smd oval (at 2.54 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(R30-Pad2)"))
    (pad 7 smd oval (at 3.81 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 10 smd oval (at 1.27 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(R31-Pad2)"))
    (pad 9 smd oval (at 2.54 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 8 smd oval (at 3.81 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 52 /P2))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 55372ECF)
    (at 179.578 65.913 90)
    (fp_text reference SW1 (at 0 0.127 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.15 -2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R20-Pad1)"))
    (pad 2 thru_hole rect (at 3.15 2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(Q3-PadG)"))
    (pad 1 thru_hole rect (at -3.15 -2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R20-Pad1)"))
    (pad 2 thru_hole rect (at -3.15 2.25 90) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(Q3-PadG)"))
  )
  (module Mlab_IO:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 553737BB)
    (at 160.274 76.327 90)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -0.127 90) (layer B.SilkS))
    (fp_text value BQ34Z100 (at 0 -3.55 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.95 1.95 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 52 /P2))
    (pad 2 smd rect (at -2.95 1.3 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(Q3-PadG)"))
    (pad 3 smd rect (at -2.95 0.65 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 53 /P1))
    (pad 4 smd rect (at -2.95 0 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.95 -0.65 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 6 smd rect (at -2.95 -1.3 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 7 smd rect (at -2.95 -1.95 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C14-Pad1)"))
    (pad 8 smd rect (at 2.95 -1.95 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 9 smd rect (at 2.95 -1.3 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad1)"))
    (pad 10 smd rect (at 2.95 -0.65 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C13-Pad2)"))
    (pad 11 smd rect (at 2.95 0 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R17-Pad2)"))
    (pad 12 smd rect (at 2.95 0.65 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 59 /HDQ))
    (pad 13 smd rect (at 2.95 1.3 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 58 /SCL))
    (pad 14 smd rect (at 2.95 1.95 90) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 57 /SDA))
    (model Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:VSON-8 (layer B.Cu) (tedit 55350D0D)
    (at 156.718 120.65 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 180) (layer B.SilkS))
    (fp_text value BQ29209 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user * (at -0.889 -1.524 180) (layer B.SilkS))
    (pad 2 smd rect (at -0.325 -1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at 0.325 -1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at 0.975 -1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 0.975 1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0.325 1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(J15-Pad1)"))
    (pad 7 smd rect (at -0.325 1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 8 smd rect (at -0.975 1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -0.975 -1.475 180) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at 0 0 180) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 5537375C)
    (at 160.782 100.838 90)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C10 (at 0.127 0.127 90) (layer B.SilkS))
    (fp_text value 100uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908 90) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0 90) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.175 0 90) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 131.445 62.611 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:VQFN-20 (layer B.Cu) (tedit 553757B7)
    (at 141.478 106.045 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U2 (at 0 0 180) (layer B.SilkS))
    (fp_text value BQ24103 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user * (at -1.651 -1.778 180) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 21 /STAT1))
    (pad 21 smd rect (at 0 0 180) (size 3.05 2.05) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.25 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -0.75 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -0.25 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 17 /PG))
    (pad 6 smd rect (at 0.25 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at 0.75 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 7 /CMODE))
    (pad 8 smd rect (at 1.25 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R12-Pad1)"))
    (pad 9 smd rect (at 1.75 -1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R11-Pad1)"))
    (pad 10 smd rect (at 2.225 -0.75 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 11 smd rect (at 2.225 0.75 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 1.75 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R13-Pad1)"))
    (pad 13 smd rect (at 1.25 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 31 /CELLS))
    (pad 14 smd rect (at 0.75 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(F3-Pad1)"))
    (pad 15 smd rect (at 0.25 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 16 smd rect (at -0.25 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 30 /CE))
    (pad 17 smd rect (at -0.75 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 18 smd rect (at -1.25 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 19 smd rect (at -1.75 1.725 180) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D4-Pad2)"))
    (pad 20 smd rect (at -2.225 0.75 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(L1-Pad1)"))
    (pad 1 smd rect (at -2.225 -0.75 180) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(L1-Pad1)"))
    (pad 21 smd trapezoid (at -2.075 0.3 180) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -2.075 -0.3 180) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.075 -0.3 180) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.075 0.3 180) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -1.75 0 180) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 1.75 0 180) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.143 0.635 180) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.143 0.635 180) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.143 -0.635 180) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.143 -0.635 180) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 175.514 71.882 180)
    (attr smd)
    (fp_text reference R34 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R34-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:Drzak_2410 (layer B.Cu) (tedit 564C162A)
    (at 148.844 120.904 90)
    (descr "F 2410 s držákem")
    (tags "F 2410 s držákem")
    (attr smd)
    (fp_text reference F1 (at 0.13462 3.15468 90) (layer B.SilkS))
    (fp_text value 5A (at 0 -3.81 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.91 0 90) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 2 smd rect (at 2.91 0 90) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:Drzak_2410 (layer B.Cu) (tedit 564C162A)
    (at 143.002 93.218 90)
    (descr "F 2410 s držákem")
    (tags "F 2410 s držákem")
    (attr smd)
    (fp_text reference F3 (at 0.13462 3.15468 90) (layer B.SilkS))
    (fp_text value 2A (at 0 -3.81 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.91 0 90) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(F3-Pad1)"))
    (pad 2 smd rect (at 2.91 0 90) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 56 /BATTERY+))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 90.551 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D7 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D7-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 87.884 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D8 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 85.217 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D9 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D9-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 82.55 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D10 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D10-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 79.883 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D11 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D11-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 77.216 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D12 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D12-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 74.549 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D13 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D13-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 180.721 71.882 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D14 (at 0 0 180) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /REGIN))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(D14-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 129.286 108.331 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0 180) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 17 /PG))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 129.286 103.251 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D4 (at 0 0 180) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D4-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 129.286 98.171 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D5 (at 0 0 180) (layer B.SilkS))
    (fp_text value LED (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 21 /STAT1))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:SMD_1_2x2 (layer B.Cu) (tedit 565FDD1E)
    (at 160.274 119.888 180)
    (fp_text reference J15 (at 0 -5.6007 180) (layer B.SilkS) hide)
    (fp_text value CONN_2 (at -0.2032 1.778 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 -2.54 180) (size 2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 180) (size 2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(J15-Pad1)"))
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "60,452 mm" (at 154.686 41.0172) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 52.07) (xy 124.46 39.6672)))
    (feature2 (pts (xy 184.912 52.07) (xy 184.912 39.6672)))
    (crossbar (pts (xy 184.912 42.3672) (xy 124.46 42.3672)))
    (arrow1a (pts (xy 124.46 42.3672) (xy 125.586504 41.780779)))
    (arrow1b (pts (xy 124.46 42.3672) (xy 125.586504 42.953621)))
    (arrow2a (pts (xy 184.912 42.3672) (xy 183.785496 41.780779)))
    (arrow2b (pts (xy 184.912 42.3672) (xy 183.785496 42.953621)))
  )
  (dimension 80.772 (width 0.3) (layer Dwgs.User)
    (gr_text "80,772 mm" (at 113.3056 92.456 90) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 52.07) (xy 111.9556 52.07)))
    (feature2 (pts (xy 124.46 132.842) (xy 111.9556 132.842)))
    (crossbar (pts (xy 114.6556 132.842) (xy 114.6556 52.07)))
    (arrow1a (pts (xy 114.6556 52.07) (xy 115.242021 53.196504)))
    (arrow1b (pts (xy 114.6556 52.07) (xy 114.069179 53.196504)))
    (arrow2a (pts (xy 114.6556 132.842) (xy 115.242021 131.715496)))
    (arrow2b (pts (xy 114.6556 132.842) (xy 114.069179 131.715496)))
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "2,3800 v" (at 154.686 47.0624) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 52.07) (xy 124.46 45.7124)))
    (feature2 (pts (xy 184.912 52.07) (xy 184.912 45.7124)))
    (crossbar (pts (xy 184.912 48.4124) (xy 124.46 48.4124)))
    (arrow1a (pts (xy 124.46 48.4124) (xy 125.586504 47.825979)))
    (arrow1b (pts (xy 124.46 48.4124) (xy 125.586504 48.998821)))
    (arrow2a (pts (xy 184.912 48.4124) (xy 183.785496 47.825979)))
    (arrow2b (pts (xy 184.912 48.4124) (xy 183.785496 48.998821)))
  )
  (dimension 80.772 (width 0.3) (layer Dwgs.User)
    (gr_text "3,1800 v" (at 118.3856 92.456 90) (layer Dwgs.User))
    (feature1 (pts (xy 124.46 52.07) (xy 117.0356 52.07)))
    (feature2 (pts (xy 124.46 132.842) (xy 117.0356 132.842)))
    (crossbar (pts (xy 119.7356 132.842) (xy 119.7356 52.07)))
    (arrow1a (pts (xy 119.7356 52.07) (xy 120.322021 53.196504)))
    (arrow1b (pts (xy 119.7356 52.07) (xy 119.149179 53.196504)))
    (arrow2a (pts (xy 119.7356 132.842) (xy 120.322021 131.715496)))
    (arrow2b (pts (xy 119.7356 132.842) (xy 119.149179 131.715496)))
  )
  (gr_text LION2CELL01C (at 153.924 63.373 90) (layer B.Cu))
  (gr_text MLAB.CZ (at 150.876 63.5 90) (layer B.Cu))
  (gr_text 2015 (at 172.085 126.365 90) (layer F.SilkS))
  (gr_text JACHO (at 169.799 126.365 90) (layer F.SilkS))
  (gr_text LION2CELL01C (at 156.464 92.456 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 152.273 92.456 90) (layer F.SilkS))
  (gr_text STAT1 (at 125.857 81.915 90) (layer F.SilkS))
  (gr_text CE (at 133.223 86.614 90) (layer F.SilkS))
  (gr_text CMODE (at 125.857 89.154 90) (layer F.SilkS))
  (gr_text CELLS (at 133.223 91.694 90) (layer F.SilkS))
  (gr_text PG (at 125.857 95.123 90) (layer F.SilkS))
  (gr_text "SW POWER" (at 133.223 77.216 90) (layer F.SilkS))
  (gr_text SDA (at 128.778 70.231 180) (layer F.SilkS))
  (gr_text GND (at 128.905 62.611 180) (layer F.SilkS))
  (gr_text HDQ (at 128.905 65.151 180) (layer F.SilkS))
  (gr_text SCL (at 128.778 67.691 180) (layer F.SilkS))
  (gr_text "POWER IN" (at 125.73 117.348 90) (layer F.SilkS))
  (gr_text "POWER OUT" (at 176.276 97.536 90) (layer F.SilkS))
  (gr_text + (at 177.165 107.442 90) (layer F.SilkS))
  (gr_text "0% ----100%" (at 177.038 81.28 90) (layer F.SilkS))
  (gr_text CHARGE (at 129.286 100.711 180) (layer F.SilkS))
  (gr_text DONE (at 129.159 105.664 180) (layer F.SilkS))
  (gr_text ON (at 129.286 110.49 180) (layer F.SilkS))
  (gr_line (start 184.912 132.842) (end 124.46 132.842) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 132.842) (end 124.46 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.912 52.07) (end 124.46 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.912 132.842) (end 184.912 52.07) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 32) (net_name "Net-(L1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.955 102.743) (xy 147.955 108.458) (xy 143.002 108.458) (xy 143.002 107.442) (xy 143.256 107.061)
        (xy 143.002 107.061) (xy 143.002 102.743)
      )
    )
  )
  (zone (net 56) (net_name /BATTERY+) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.796 88.646) (xy 145.796 91.186) (xy 152.654 91.186) (xy 152.654 91.694) (xy 152.654 91.948)
        (xy 152.654 99.314) (xy 152.654 102.108) (xy 152.654 115.316) (xy 150.876 116.205) (xy 150.876 120.015)
        (xy 146.812 120.015) (xy 146.558 120.015) (xy 146.558 99.314) (xy 148.59 99.314) (xy 148.59 93.98)
        (xy 140.97 93.98) (xy 140.97 88.646) (xy 145.542 88.646)
      )
    )
  )
  (zone (net 1) (net_name /BAT+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.494 131.064) (xy 142.494 126.365) (xy 144.526 126.365) (xy 146.939 123.952) (xy 146.939 122.174)
        (xy 150.876 122.174) (xy 150.876 127.762) (xy 147.574 129.032) (xy 147.574 131.064) (xy 147.066 131.064)
      )
    )
  )
  (zone (net 54) (net_name /BAT-MIDPOINT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.243 130.81) (xy 166.243 126.619) (xy 158.877 126.619) (xy 153.797 126.619) (xy 153.797 130.81)
      )
    )
  )
  (zone (net 56) (net_name /BATTERY+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.193 112.014) (xy 147.193 109.601) (xy 170.18 109.601) (xy 170.18 109.728) (xy 174.752 109.728)
        (xy 174.752 95.123) (xy 182.372 95.123) (xy 182.372 99.822) (xy 177.927 99.822) (xy 177.546 100.203)
        (xy 177.546 104.902) (xy 179.451 106.807) (xy 179.451 120.269) (xy 175.133 120.269) (xy 175.133 115.443)
        (xy 148.336 115.443) (xy 148.082 119.888) (xy 147.066 119.761) (xy 147.193 112.014)
      )
    )
  )
  (zone (net 11) (net_name /REGIN) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 82.55) (xy 158.75 78.486) (xy 159.893 78.486) (xy 159.893 80.264) (xy 160.401 80.772)
        (xy 160.401 83.058) (xy 158.75 83.058)
      )
    )
  )
  (zone (net 55) (net_name /BATTERY-) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 53.975) (xy 166.37 58.547) (xy 164.592 60.325) (xy 164.592 62.23) (xy 161.798 62.23)
        (xy 161.798 53.975)
      )
    )
  )
  (zone (net 54) (net_name /BAT-MIDPOINT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.624 130.81) (xy 166.624 117.094) (xy 160.02 110.49) (xy 160.02 90.678) (xy 146.812 90.678)
        (xy 146.812 53.848) (xy 141.986 53.848) (xy 141.986 95.504) (xy 155.067 95.504) (xy 155.067 111.252)
        (xy 161.925 118.11) (xy 161.925 130.81) (xy 162.306 130.81)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.555 135.763) (xy 122.555 43.942) (xy 188.976 45.72) (xy 191.135 140.081)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.777 141.605) (xy 120.269 39.751) (xy 192.278 40.64) (xy 193.929 143.637)
      )
    )
  )
  (zone (net 62) (net_name "Net-(F3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.336 97.79) (xy 148.336 94.234) (xy 142.748 94.234) (xy 142.748 97.536) (xy 142.748 97.79)
      )
    )
  )
  (zone (net 10) (net_name "Net-(C10-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.814 109.22) (xy 162.814 101.6) (xy 158.496 101.6) (xy 158.496 90.932) (xy 152.908 90.932)
        (xy 152.908 109.22)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.746 114.808) (xy 133.223 114.808) (xy 133.223 112.903) (xy 138.049 112.903) (xy 138.049 111.887)
        (xy 140.716 108.966) (xy 140.716 107.315) (xy 141.478 107.315) (xy 143.002 107.315) (xy 143.002 109.855)
        (xy 142.113 110.744) (xy 142.113 113.792) (xy 142.113 114.173) (xy 138.43 114.173) (xy 138.43 121.158)
        (xy 133.35 121.158) (xy 133.35 119.634) (xy 126.746 119.634)
      )
    )
  )
)
