(kicad_pcb (version 4) (host pcbnew 4.0.2-4+6225~38~ubuntu15.10.1-stable)
  (general
    (links 222)
    (no_connects 0)
    (area -10.541 -73.3604 98.7288 8.763001)
    (thickness 1.6)
    (drawings 34)
    (tracks 1276)
    (zones 0)
    (modules 100)
    (nets 61)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.89)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only yes)
    (trace_min 0.18)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.89)
    (via_drill 0.5)
    (via_min_size 0.7)
    (via_min_drill 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.7 2.7)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 /BAT+)
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 /CMODE)
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C13-Pad1)")
  (net 12 "Net-(C13-Pad2)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(C17-Pad1)")
  (net 15 "Net-(D3-Pad1)")
  (net 16 /PG)
  (net 17 "Net-(D4-Pad1)")
  (net 18 "Net-(D5-Pad1)")
  (net 19 /STAT1)
  (net 20 "Net-(D7-Pad2)")
  (net 21 "Net-(D8-Pad2)")
  (net 22 "Net-(D9-Pad2)")
  (net 23 "Net-(D10-Pad2)")
  (net 24 "Net-(D11-Pad2)")
  (net 25 "Net-(D12-Pad2)")
  (net 26 "Net-(D13-Pad2)")
  (net 27 /CE)
  (net 28 "Net-(L1-Pad1)")
  (net 29 "Net-(Q1-PadG)")
  (net 30 "Net-(R3-Pad1)")
  (net 31 "Net-(R10-Pad2)")
  (net 32 "Net-(R11-Pad1)")
  (net 33 "Net-(R12-Pad1)")
  (net 34 "Net-(R13-Pad1)")
  (net 35 "Net-(R17-Pad2)")
  (net 36 "Net-(R20-Pad1)")
  (net 37 "Net-(R27-Pad2)")
  (net 38 "Net-(R28-Pad2)")
  (net 39 "Net-(R29-Pad2)")
  (net 40 "Net-(R30-Pad2)")
  (net 41 "Net-(R31-Pad2)")
  (net 42 "Net-(R32-Pad2)")
  (net 43 "Net-(R33-Pad2)")
  (net 44 /P2)
  (net 45 /P1)
  (net 46 /BAT-MIDPOINT)
  (net 47 /BATTERY-)
  (net 48 /BATTERY+)
  (net 49 /SDA)
  (net 50 /SCL)
  (net 51 /HDQ)
  (net 52 "Net-(D14-Pad2)")
  (net 53 "Net-(R34-Pad2)")
  (net 54 "Net-(F3-Pad1)")
  (net 55 +3V3)
  (net 56 "Net-(R25-Pad1)")
  (net 57 "Net-(SW1-Pad2)")
  (net 58 /CB_EN)
  (net 59 /STAT2)
  (net 60 "Net-(R5-Pad2)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /BAT+)
    (add_net /BAT-MIDPOINT)
    (add_net /BATTERY+)
    (add_net /BATTERY-)
    (add_net /CB_EN)
    (add_net /CE)
    (add_net /CMODE)
    (add_net /HDQ)
    (add_net /P1)
    (add_net /P2)
    (add_net /PG)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /STAT1)
    (add_net /STAT2)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(F3-Pad1)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(Q1-PadG)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R30-Pad2)")
    (add_net "Net-(R31-Pad2)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R33-Pad2)")
    (add_net "Net-(R34-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(SW1-Pad2)")
  )
  (net_class Low_power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net GND)
  )
  (module Mlab_Batery:2LION (layer F.Cu) (tedit 56950FA6)
    (at 40.5765 -30.861)
    (fp_text reference BT1 (at -12.6365 -2.8575) (layer F.SilkS))
    (fp_text value 2x18650_LION-RESCUE-LION2CELL01C (at 0 0) (layer F.SilkS) hide)
    (fp_text user - (at 22.86 8.89) (layer F.SilkS))
    (fp_text user - (at 22.86 -10.16) (layer F.SilkS))
    (fp_text user + (at -22.86 8.89) (layer F.SilkS))
    (fp_text user + (at -22.86 -10.16) (layer F.SilkS))
    (pad 1 thru_hole rect (at -36.25 -9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 /BAT+))
    (pad 2 thru_hole rect (at 36.25 -9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 46 /BAT-MIDPOINT))
    (pad 3 thru_hole rect (at -36.25 9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 46 /BAT-MIDPOINT))
    (pad 4 thru_hole rect (at 36.25 9.65) (size 4 4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 47 /BATTERY-))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.89 -26.924 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 553736FB)
    (at 17.272 -46.24324 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C2 (at 0 0 270) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 270) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 270) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 20.193 -43.18 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.89 -30.607 270)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 12.446 -31.496)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 330nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.717 -49.149 90)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /CMODE))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.8694 -43.18 270)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 15.748 -30.988 90)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 32.766 -48.387 90)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 24.765 -22.479 270)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 50.419 -24.511 270)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 62.992 -25.146 270)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 69.469 -17.272 270)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 64.008 -22.352)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 64.008 -28.448)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 53.9115 -32.258 90)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 3n3 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 46.863 -20.193 270)
    (attr smd)
    (fp_text reference C18 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 55373700)
    (at 11.71702 -49.276)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 5537370C)
    (at 18.542 -38.1 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 0 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 48 /BATTERY+))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 15.748 -55.88 270)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35 270) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 49.022 -55.626)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /STAT1))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /STAT1))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 38.862 -55.626 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PG))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PG))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 43.942 -55.626 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /CMODE))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 46.482 -55.626)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CE))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CE))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 41.402 -55.626)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 /STAT2))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 59 /STAT2))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 35.56 -5.08 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J7 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 /BATTERY+))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 /BATTERY+))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 /BATTERY+))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 48 /BATTERY+))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55372F24)
    (at 17.399 -7.874)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J8 (at -5.969 0.127) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 48 /BATTERY+))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 48 /BATTERY+))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55372F27)
    (at 17.399 -2.921)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J9 (at -5.334 0.127) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 62.865 -53.721)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 /SDA))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 49 /SDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 65.405 -53.721)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 /SCL))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 50 /SCL))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 67.945 -53.721)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 /HDQ))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 51 /HDQ))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 55.88 -55.626 270)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J13 (at 0 -6.35 270) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C10-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_L:DE1205-10 (layer B.Cu) (tedit 54BBE563)
    (at 27.559 -33.909 90)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (fp_text reference L1 (at 0 5.842 90) (layer B.SilkS))
    (fp_text value DE1205-10 (at 0 -5.842 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 5 0 90) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -5 0 90) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 76.2 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -55.88)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 76.2 -55.88)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_T:SOT-23 (layer B.Cu) (tedit 55373750)
    (at 18.923 -31.115 180)
    (tags SOT23)
    (fp_text reference Q1 (at 0 0 180) (layer B.SilkS))
    (fp_text value IRLML6244 (at 0.0635 0 180) (layer B.SilkS) hide)
    (pad D smd rect (at 0 1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 48 /BATTERY+))
    (pad S smd rect (at 0.9525 -1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad G smd rect (at -0.9525 -1.09982 180) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(Q1-PadG)"))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 6.477 -33.909 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 160R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 5.842 -28.067 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 260R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 46 /BAT-MIDPOINT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 5.842 -30.353 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 46 /BAT-MIDPOINT))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 46.482 -50.546 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 27 /CE))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 35.052 -50.3555 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R5-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 22.479 -52.578 90)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.432 -52.451 90)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D4-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 32.385 -52.451 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D5-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 16.764 -27.686)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.0815 -25.0825 270)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(Q1-PadG)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(R10-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 25.908 -49.149 90)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 7K5 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 23.876 -49.149 90)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 7K5 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 33.782 -45.593)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 9K31 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.099 -48.387 270)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 442K (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 5537367F)
    (at 12.827 -40.386)
    (attr smd)
    (fp_text reference R15 (at 0 -2.286) (layer F.SilkS))
    (fp_text value NCP21XV103J03RA (at 0.127 0.381) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512 (layer B.Cu) (tedit 5537376D)
    (at 36.957 -34.417 270)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R16 (at -0.254 1.016 270) (layer B.SilkS))
    (fp_text value 0R1 (at -0.254 -0.762 270) (layer B.Fab))
    (pad 1 smd rect (at -3.1 0 270) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(F3-Pad1)"))
    (pad 2 smd rect (at 3.1 0 270) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 55373690)
    (at 68.453 -21.082 180)
    (attr smd)
    (fp_text reference R17 (at 0 2.286 180) (layer F.SilkS))
    (fp_text value "10K NTC" (at 0.127 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R17-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 65.532 -25.146 90)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 47 /BATTERY-))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 68.834 -25.908 180)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100R (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 71.501 -14.351 90)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1K (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 15.24 -25.0825 90)
    (attr smd)
    (fp_text reference R21 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 270k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 58 /CB_EN))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 55.9435 -32.258 270)
    (attr smd)
    (fp_text reference R23 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value "16k5 25ppm" (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 52.6415 -29.2735)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175) (layer B.SilkS))
    (fp_text value "140k .1% 25ppm" (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 51.308 -36.1315 90)
    (attr smd)
    (fp_text reference R25 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 270k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R25-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 51.308 -32.8295 90)
    (attr smd)
    (fp_text reference R26 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 165k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R25-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 42.545 -9.652 90)
    (attr smd)
    (fp_text reference R27 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R27-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 45.212 -9.652 90)
    (attr smd)
    (fp_text reference R28 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R28-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 47.879 -9.652 90)
    (attr smd)
    (fp_text reference R29 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R29-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 50.546 -9.652 90)
    (attr smd)
    (fp_text reference R30 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R30-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 53.213 -9.652 90)
    (attr smd)
    (fp_text reference R31 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R31-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 55.88 -9.652 90)
    (attr smd)
    (fp_text reference R32 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R32-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 58.547 -9.652 90)
    (attr smd)
    (fp_text reference R33 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R33-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SO-14 (layer B.Cu) (tedit 5534C67E)
    (at 51.689 -16.764 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U4 (at 0 0 90) (layer B.SilkS))
    (fp_text value SN74HC164D (at 0 0 90) (layer B.SilkS) hide)
    (pad 1 smd oval (at -3.81 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 45 /P1))
    (pad 2 smd oval (at -2.54 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 45 /P1))
    (pad 3 smd oval (at -1.27 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R27-Pad2)"))
    (pad 4 smd oval (at 0 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(R28-Pad2)"))
    (pad 11 smd oval (at 0 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(R32-Pad2)"))
    (pad 12 smd oval (at -1.27 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(R33-Pad2)"))
    (pad 13 smd oval (at -2.54 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R34-Pad2)"))
    (pad 14 smd oval (at -3.81 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 5 smd oval (at 1.27 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(R29-Pad2)"))
    (pad 6 smd oval (at 2.54 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(R30-Pad2)"))
    (pad 7 smd oval (at 3.81 -2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 10 smd oval (at 1.27 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(R31-Pad2)"))
    (pad 9 smd oval (at 2.54 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 8 smd oval (at 3.81 2.794 90) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 44 /P2))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_SW:SW_PUSH_SMALL placed (layer F.Cu) (tedit 55372ECF)
    (at 67.183 -5.588)
    (fp_text reference SW1 (at 0 0.127) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.0508 0.9652) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R20-Pad1)"))
    (pad 2 thru_hole rect (at 3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(SW1-Pad2)"))
    (pad 1 thru_hole rect (at -3.15 -2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R20-Pad1)"))
    (pad 2 thru_hole rect (at -3.15 2.25) (size 1.6764 1.6764) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(SW1-Pad2)"))
  )
  (module Mlab_IO:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 553737BB)
    (at 56.769 -24.892)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -0.127) (layer B.SilkS))
    (fp_text value BQ34Z100 (at 0 -3.55) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 44 /P2))
    (pad 2 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(SW1-Pad2)"))
    (pad 3 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 45 /P1))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C17-Pad1)"))
    (pad 5 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 6 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 7 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 8 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 9 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C13-Pad1)"))
    (pad 10 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C13-Pad2)"))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(R17-Pad2)"))
    (pad 12 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 51 /HDQ))
    (pad 13 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 50 /SCL))
    (pad 14 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 49 /SDA))
    (model Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:VSON-8 (layer B.Cu) (tedit 55350D0D)
    (at 12.446 -28.448 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0 90) (layer B.SilkS))
    (fp_text value BQ29209 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user * (at -0.889 -1.524 90) (layer B.SilkS))
    (pad 2 smd rect (at -0.325 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at 0.325 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(R3-Pad1)"))
    (pad 4 smd rect (at 0.975 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 0.975 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0.325 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 58 /CB_EN))
    (pad 7 smd rect (at -0.325 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 8 smd rect (at -0.975 1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -0.975 -1.475 90) (size 0.35 0.85) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at 0 0 90) (size 2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 5537375C)
    (at 32.258 -24.384)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C10 (at 0.127 0.127) (layer B.SilkS))
    (fp_text value 100uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 70.485 -53.721)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J14 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:VQFN-20 (layer B.Cu) (tedit 553757B7)
    (at 27.051 -43.688 90)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U2 (at 0 0 90) (layer B.SilkS))
    (fp_text value BQ24103 (at 0 0 90) (layer B.SilkS) hide)
    (fp_text user * (at -1.651 -1.778 90) (layer B.SilkS))
    (pad 2 smd rect (at -1.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 19 /STAT1))
    (pad 21 smd rect (at 0 0 90) (size 3.05 2.05) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -0.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -0.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 16 /PG))
    (pad 6 smd rect (at 0.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at 0.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 7 /CMODE))
    (pad 8 smd rect (at 1.25 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(R12-Pad1)"))
    (pad 9 smd rect (at 1.75 -1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(R11-Pad1)"))
    (pad 10 smd rect (at 2.225 -0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 11 smd rect (at 2.225 0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 12 smd rect (at 1.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R13-Pad1)"))
    (pad 13 smd rect (at 1.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R5-Pad2)"))
    (pad 14 smd rect (at 0.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(F3-Pad1)"))
    (pad 15 smd rect (at 0.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 16 smd rect (at -0.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 27 /CE))
    (pad 17 smd rect (at -0.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 18 smd rect (at -1.25 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 19 smd rect (at -1.75 1.725 90) (size 0.28 0.85) (layers B.Cu B.Paste B.Mask)
      (net 59 /STAT2))
    (pad 20 smd rect (at -2.225 0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(L1-Pad1)"))
    (pad 1 smd rect (at -2.225 -0.75 90) (size 0.85 0.28) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(L1-Pad1)"))
    (pad 21 smd trapezoid (at -2.075 0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -2.075 -0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.075 -0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 2.075 0.3 90) (size 1.125 0.28) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at -1.75 0 90) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 smd rect (at 1.75 0 90) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.143 0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.143 0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 1.143 -0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at -1.143 -0.635 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 61.214 -9.652 90)
    (attr smd)
    (fp_text reference R34 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2K2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(R34-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:Drzak_2410 (layer B.Cu) (tedit 564C162A)
    (at 12.192 -36.322)
    (descr "F 2410 s držákem")
    (tags "F 2410 s držákem")
    (attr smd)
    (fp_text reference F1 (at 0.13462 3.15468) (layer B.SilkS))
    (fp_text value 5A (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.91 0) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 2 smd rect (at 2.91 0) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 48 /BATTERY+))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:Drzak_2410 (layer B.Cu) (tedit 564C162A)
    (at 39.878 -42.164)
    (descr "F 2410 s držákem")
    (tags "F 2410 s držákem")
    (attr smd)
    (fp_text reference F3 (at 0.13462 3.15468) (layer B.SilkS))
    (fp_text value 2A (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.91 0) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(F3-Pad1)"))
    (pad 2 smd rect (at 2.91 0) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 48 /BATTERY+))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 42.545 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D7 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D7-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 45.212 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D8 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D8-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 47.879 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D9 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D9-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 50.546 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D10 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D10-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 53.213 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D11 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D11-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 55.88 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D12 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D12-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 58.547 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D13 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D13-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 61.214 -4.445 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D14 (at 0 0 90) (layer B.SilkS))
    (fp_text value ORAGE (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(D14-Pad2)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 56C24CAC)
    (at 24.765 -55.88 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0 90) (layer B.SilkS))
    (fp_text value Green (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 16 /PG))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS)
      (clearance 0.1))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 29.845 -55.88 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D4 (at 0 0 90) (layer B.SilkS))
    (fp_text value Green (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 59 /STAT2))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 565E87C9)
    (at 34.925 -55.88 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D5 (at 0 0 90) (layer B.SilkS))
    (fp_text value Red (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 19 /STAT1))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:SMD_1_2x2 (layer B.Cu) (tedit 565FDD1E)
    (at 13.208 -24.892 90)
    (fp_text reference J15 (at 0 -5.6007 90) (layer B.SilkS) hide)
    (fp_text value CONN_2 (at -0.2032 1.778 90) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 -2.54 90) (size 2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0 90) (size 2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 58 /CB_EN))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 46.99 -38.1 90)
    (attr smd)
    (fp_text reference C19 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 50.6095 -42.2275 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C20 (at 0.0127 -0.0381 90) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_IO:SO-8 (layer B.Cu) (tedit 5479A0C5)
    (at 47.3075 -32.5755 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U5 (at 0 0 180) (layer B.SilkS))
    (fp_text value TPS76601 (at 0 0 180) (layer B.SilkS) hide)
    (pad 1 smd oval (at -1.905 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(R25-Pad1)"))
    (pad 2 smd oval (at -0.635 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd oval (at 0.635 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 4 smd oval (at 1.905 -2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 5 smd oval (at 1.905 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 6 smd oval (at 0.635 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 1 /BAT+))
    (pad 7 smd oval (at -0.635 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (pad 8 smd oval (at -1.905 2.794 180) (size 0.6096 1.4732) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (model MLAB_3D/IO/cms_so8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.45))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 55.1815 -34.9885 180)
    (attr smd)
    (fp_text reference R35 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 49 /SDA))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 56.515 -36.8935 180)
    (attr smd)
    (fp_text reference R36 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 47k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 50 /SCL))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 55 +3V3))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOT-23 (layer B.Cu) (tedit 569E36E4)
    (at 15.6845 -20.8915)
    (tags SOT23)
    (fp_text reference U6 (at 1.99898 0.09906 270) (layer B.SilkS))
    (fp_text value APX810-31SAG-7 (at 0.0635 0) (layer B.SilkS))
    (pad 3 smd rect (at 0 1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 46 /BAT-MIDPOINT))
    (pad 2 smd rect (at 0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 58 /CB_EN))
    (pad 1 smd rect (at -0.9525 -1.09982) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model D:/Honza/library/KiCAD/MLAB_3D/IO/SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-2512 (layer B.Cu) (tedit 56BD8BA5)
    (at 72.517 -24.511 90)
    (descr "Resistor SMD 2512, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R22 (at 0 3.1 90) (layer B.SilkS))
    (fp_text value "0R01 75PPM" (at 0 -3.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -3.1 0 90) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 47 /BATTERY-))
    (pad 2 smd rect (at 3.1 0 90) (size 1 3.2) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 6 (at 43.942 -52.07) (layer F.SilkS))
  (gr_text 5 (at 49.022 -59.309) (layer F.SilkS))
  (gr_text 4 (at 46.482 -59.309) (layer F.SilkS))
  (gr_text 2 (at 41.402 -59.309) (layer F.SilkS))
  (gr_text 1 (at 38.862 -59.309) (layer F.SilkS))
  (gr_text 3 (at 43.942 -59.309) (layer F.SilkS))
  (gr_text 2 (at 68.3895 -40.5765 90) (layer F.SilkS))
  (gr_text 1 (at 12.7 -21.209 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 40.64 -32.893) (layer F.SilkS))
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "60,452 mm" (at 92.0788 -30.48 90) (layer Dwgs.User))
    (feature1 (pts (xy 81.026 -60.706) (xy 93.4288 -60.706)))
    (feature2 (pts (xy 81.026 -0.254) (xy 93.4288 -0.254)))
    (crossbar (pts (xy 90.7288 -0.254) (xy 90.7288 -60.706)))
    (arrow1a (pts (xy 90.7288 -60.706) (xy 91.315221 -59.579496)))
    (arrow1b (pts (xy 90.7288 -60.706) (xy 90.142379 -59.579496)))
    (arrow2a (pts (xy 90.7288 -0.254) (xy 91.315221 -1.380504)))
    (arrow2b (pts (xy 90.7288 -0.254) (xy 90.142379 -1.380504)))
  )
  (dimension 80.772 (width 0.3) (layer Dwgs.User)
    (gr_text "80,772 mm" (at 40.64 -71.8604) (layer Dwgs.User))
    (feature1 (pts (xy 81.026 -60.706) (xy 81.026 -73.2104)))
    (feature2 (pts (xy 0.254 -60.706) (xy 0.254 -73.2104)))
    (crossbar (pts (xy 0.254 -70.5104) (xy 81.026 -70.5104)))
    (arrow1a (pts (xy 81.026 -70.5104) (xy 79.899496 -69.923979)))
    (arrow1b (pts (xy 81.026 -70.5104) (xy 79.899496 -71.096821)))
    (arrow2a (pts (xy 0.254 -70.5104) (xy 1.380504 -69.923979)))
    (arrow2b (pts (xy 0.254 -70.5104) (xy 1.380504 -71.096821)))
  )
  (dimension 60.452 (width 0.3) (layer Dwgs.User)
    (gr_text "2,3800 v" (at 86.0336 -30.48 90) (layer Dwgs.User))
    (feature1 (pts (xy 81.026 -60.706) (xy 87.3836 -60.706)))
    (feature2 (pts (xy 81.026 -0.254) (xy 87.3836 -0.254)))
    (crossbar (pts (xy 84.6836 -0.254) (xy 84.6836 -60.706)))
    (arrow1a (pts (xy 84.6836 -60.706) (xy 85.270021 -59.579496)))
    (arrow1b (pts (xy 84.6836 -60.706) (xy 84.097179 -59.579496)))
    (arrow2a (pts (xy 84.6836 -0.254) (xy 85.270021 -1.380504)))
    (arrow2b (pts (xy 84.6836 -0.254) (xy 84.097179 -1.380504)))
  )
  (dimension 80.772 (width 0.3) (layer Dwgs.User)
    (gr_text "3,1800 v" (at 40.64 -66.7804) (layer Dwgs.User))
    (feature1 (pts (xy 81.026 -60.706) (xy 81.026 -68.1304)))
    (feature2 (pts (xy 0.254 -60.706) (xy 0.254 -68.1304)))
    (crossbar (pts (xy 0.254 -65.4304) (xy 81.026 -65.4304)))
    (arrow1a (pts (xy 81.026 -65.4304) (xy 79.899496 -64.843979)))
    (arrow1b (pts (xy 81.026 -65.4304) (xy 79.899496 -66.016821)))
    (arrow2a (pts (xy 0.254 -65.4304) (xy 1.380504 -64.843979)))
    (arrow2b (pts (xy 0.254 -65.4304) (xy 1.380504 -66.016821)))
  )
  (gr_text LION2CELL01D (at 69.723 -31.242) (layer B.Cu))
  (gr_text MLAB.CZ (at 69.596 -34.29) (layer B.Cu))
  (gr_text 2016 (at 6.731 -13.081) (layer F.SilkS))
  (gr_text JACHO (at 6.731 -15.367) (layer F.SilkS))
  (gr_text LION2CELL01D (at 40.64 -28.702) (layer F.SilkS))
  (gr_text "SW POWER" (at 55.88 -51.943) (layer F.SilkS))
  (gr_text SDA (at 62.865 -56.388 90) (layer F.SilkS))
  (gr_text GND (at 70.485 -56.261 90) (layer F.SilkS))
  (gr_text HDQ (at 67.945 -56.261 90) (layer F.SilkS))
  (gr_text SCL (at 65.405 -56.388 90) (layer F.SilkS))
  (gr_text "POWER IN" (at 15.748 -59.436) (layer F.SilkS))
  (gr_text "POWER OUT" (at 35.56 -8.89) (layer F.SilkS))
  (gr_text + (at 25.654 -8.001) (layer F.SilkS))
  (gr_text "0% ----100%" (at 51.816 -8.128) (layer F.SilkS))
  (gr_text CHARGE (at 32.385 -55.88 90) (layer F.SilkS))
  (gr_text DONE (at 27.432 -56.007 90) (layer F.SilkS))
  (gr_text ON (at 22.606 -55.88 90) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -60.706) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -60.706) (end 81.026 -60.706) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81.026 -0.254) (end 81.026 -60.706) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 81.026 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 28) (net_name "Net-(L1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.353 -37.211) (xy 24.638 -37.211) (xy 24.638 -42.164) (xy 25.654 -42.164) (xy 26.035 -41.91)
        (xy 26.035 -42.164) (xy 30.353 -42.164)
      )
    )
  )
  (zone (net 48) (net_name /BATTERY+) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.45 -39.37) (xy 41.91 -39.37) (xy 41.91 -32.512) (xy 41.402 -32.512) (xy 41.148 -32.512)
        (xy 33.782 -32.512) (xy 30.988 -32.512) (xy 17.78 -32.512) (xy 16.891 -34.29) (xy 13.081 -34.29)
        (xy 13.07084 -37.75456) (xy 13.078615 -38.315838) (xy 22.824477 -38.300164) (xy 23.124936 -38.00856) (xy 33.81248 -38.01872)
        (xy 33.782 -36.576) (xy 39.116 -36.576) (xy 39.116 -44.196) (xy 44.45 -44.196) (xy 44.45 -39.624)
      )
    )
  )
  (zone (net 1) (net_name /BAT+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.032 -42.672) (xy 6.731 -42.672) (xy 6.731 -40.64) (xy 9.144 -38.227) (xy 10.922 -38.227)
        (xy 10.922 -34.29) (xy 5.334 -34.29) (xy 4.064 -37.592) (xy 2.032 -37.592) (xy 2.032 -38.1)
      )
    )
  )
  (zone (net 46) (net_name /BAT-MIDPOINT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.286 -18.923) (xy 6.477 -18.923) (xy 6.477 -26.289) (xy 6.477 -31.369) (xy 2.286 -31.369)
      )
    )
  )
  (zone (net 48) (net_name /BATTERY+) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21.082 -37.973) (xy 23.495 -37.973) (xy 23.495 -14.986) (xy 23.368 -14.986) (xy 23.368 -10.414)
        (xy 37.973 -10.414) (xy 37.973 -2.794) (xy 33.274 -2.794) (xy 33.274 -7.239) (xy 32.893 -7.62)
        (xy 28.194 -7.62) (xy 26.289 -5.715) (xy 12.827 -5.715) (xy 12.827 -10.033) (xy 17.653 -10.033)
        (xy 17.653 -36.83) (xy 13.208 -37.084) (xy 13.335 -38.1) (xy 21.082 -37.973)
      )
    )
  )
  (zone (net 55) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.546 -26.416) (xy 54.61 -26.416) (xy 54.61 -25.273) (xy 52.832 -25.273) (xy 52.324 -24.765)
        (xy 50.038 -24.765) (xy 50.038 -26.416)
      )
    )
  )
  (zone (net 47) (net_name /BATTERY-) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.121 -18.796) (xy 74.549 -18.796) (xy 72.771 -20.574) (xy 70.866 -20.574) (xy 70.866 -23.368)
        (xy 79.121 -23.368)
      )
    )
  )
  (zone (net 46) (net_name /BAT-MIDPOINT) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 2.286 -18.542) (xy 16.002 -18.542) (xy 22.606 -25.146) (xy 42.418 -25.146) (xy 42.418 -38.354)
        (xy 79.248 -38.354) (xy 79.248 -43.18) (xy 37.592 -43.18) (xy 37.592 -30.099) (xy 21.844 -30.099)
        (xy 14.986 -23.241) (xy 2.286 -23.241) (xy 2.286 -22.86)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.667 -62.611) (xy 89.154 -62.611) (xy 87.376 3.81) (xy -6.985 5.969)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -8.509 -64.389) (xy 93.345 -64.897) (xy 92.456 7.112) (xy -10.541 8.763)
      )
    )
  )
  (zone (net 54) (net_name "Net-(F3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.306 -36.83) (xy 38.862 -36.83) (xy 38.862 -42.418) (xy 35.56 -42.418) (xy 35.306 -42.418)
      )
    )
  )
  (zone (net 10) (net_name "Net-(C10-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.876 -22.352) (xy 31.496 -22.352) (xy 31.496 -26.67) (xy 42.164 -26.67) (xy 42.164 -32.258)
        (xy 23.876 -32.258)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.288 -58.42) (xy 18.288 -51.943) (xy 20.193 -51.943) (xy 20.193 -47.117) (xy 21.844 -47.117)
        (xy 24.511 -44.45) (xy 25.781 -44.45) (xy 25.781 -43.688) (xy 25.781 -42.164) (xy 23.241 -42.164)
        (xy 22.352 -43.053) (xy 19.304 -43.053) (xy 18.923 -43.053) (xy 18.923 -46.736) (xy 11.938 -46.736)
        (xy 11.938 -51.816) (xy 13.462 -51.816) (xy 13.462 -58.42)
      )
    )
  )
)
