(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 62)
    (no_connects 0)
    (area -4.191 -41.783 42.291001 2.794001)
    (thickness 1.6)
    (drawings 24)
    (tracks 341)
    (zones 0)
    (modules 31)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1.3)
    (user_trace_width 2.6)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.7)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.12)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 /VIN)
  (net 2 GND)
  (net 3 "Net-(C2-Pad2)")
  (net 4 /EN)
  (net 5 /VSEL)
  (net 6 /#PFO)
  (net 7 /PG)
  (net 8 "Net-(L1-Pad1)")
  (net 9 "Net-(L2-Pad1)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 /OUT)
  (net 12 /Vpull-up)
  (net 13 "Net-(R3-Pad1)")
  (net 14 /OUT2)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /#PFO)
    (add_net /EN)
    (add_net /OUT)
    (add_net /OUT2)
    (add_net /PG)
    (add_net /VSEL)
    (add_net /Vpull-up)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad1)")
  )
  (net_class Vin ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /VIN)
  )
  (module Mlab_C:C_Radial_D16_L25_P7.5 (layer F.Cu) (tedit 57ECA00F)
    (at 13.3985 -31.1785)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 0.3175 -3.8735) (layer F.SilkS))
    (fp_text value 22F (at 3.75 9.3) (layer F.Fab))
    (fp_text user + (at -0.0381 -2.3114) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.5 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 /OUT))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L25_P7.5.wrl
      (at (xyz 0.1476378 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57EC99EE)
    (at 11.176 -5.842 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J14 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /Vpull-up))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /Vpull-up))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_C:C_Radial_D16_L25_P7.5 (layer F.Cu) (tedit 57ECA014)
    (at 28.194 -22.6695)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 0.254 -5.0165) (layer F.SilkS))
    (fp_text value 22F (at 3.75 9.3) (layer F.Fab))
    (fp_text user + (at -0.0381 -2.3114) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.5 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L25_P7.5.wrl
      (at (xyz 0.1476378 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 57EC99EE)
    (at 33.528 -13.335 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (pad 2 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 /VIN))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 57EC99EE)
    (at 7.62 -13.081)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J13 (at -5.842 0 90) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57EC99EE)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57EC99EE)
    (at 35.56 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57EC99EE)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57EC99EE)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_IO:DFN-12-1EP_3x4mm_Pitch0.5mm (layer B.Cu) (tedit 57EC99EE)
    (at 16.637 -18.542 90)
    (descr "DE/UE Package; 12-Lead Plastic DFN (4mm x 3mm) (see Linear Technology DFN_12_05-08-1695.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 3.05 90) (layer B.SilkS))
    (fp_text value LTC3625 (at 0 -3.05 90) (layer B.Fab))
    (fp_text user * (at -0.9652 1.1684 90) (layer B.SilkS))
    (pad 13 smd rect (at -0.425 1.2375 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.425 0.4125 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.425 -0.4125 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.425 -1.2375 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.425 1.2375 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.425 0.4125 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.425 -0.4125 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.425 -1.2375 90) (size 0.85 0.825) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 12 smd rect (at 1.45 1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(L1-Pad1)"))
    (pad 11 smd rect (at 1.45 0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 11 /OUT))
    (pad 10 smd rect (at 1.45 0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 9 smd rect (at 1.45 -0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /PG))
    (pad 8 smd rect (at 1.45 -0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 /#PFO))
    (pad 7 smd rect (at 1.45 -1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 6 smd rect (at -1.45 -1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 5 smd rect (at -1.45 -0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /EN))
    (pad 4 smd rect (at -1.45 -0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /VSEL))
    (pad 3 smd rect (at -1.45 0.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.45 0.75 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /VIN))
    (pad 1 smd rect (at -1.45 1.25 90) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(L2-Pad1)"))
    (model Housings_DFN_QFN.3dshapes/DFN-12-1EP_3x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57EC9C2C)
    (at 18.415 -13.462 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /VIN))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57EC99EE)
    (at 18.415 -10.414 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 200k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 /VIN))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57EC99EE)
    (at 14.605 -10.414 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 75k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57EC99EE)
    (at 14.605 -13.335 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 75k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57EC99EE)
    (at 16.256 -5.842 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /#PFO))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /#PFO))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 57EC99EE)
    (at 13.716 -5.842 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /PG))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /PG))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 57EC99EE)
    (at 7.62 -18.034)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J12 (at -5.842 0 90) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 /OUT))
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 /OUT))
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 57EC99EE)
    (at 18.796 -4.572)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /EN))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 57EC99EE)
    (at 18.796 -7.112)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J5 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VIN))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 57EC99EE)
    (at 21.336 -7.112)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VIN))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 57EC99EE)
    (at 21.336 -4.572)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J8 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /VSEL))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 57EC99EE)
    (at 29.21 -9.144 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VIN))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VIN))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 57EC99EE)
    (at 4.953 -26.67 180)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J11 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 180) (layer F.SilkS))
    (pad 6 thru_hole rect (at 1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole rect (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /OUT2))
    (pad 3 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /OUT2))
    (pad 2 thru_hole rect (at 1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -1.27 -2.54 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 57EC99EE)
    (at 28.448 -33.02 90)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0.127 0 90) (layer B.SilkS))
    (fp_text value 15MQ040N (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.69926 90) (layer B.SilkS))
    (fp_text user A (at -3.29946 -1.6002 90) (layer B.SilkS))
    (pad 1 smd rect (at 1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 14 /OUT2))
    (pad 2 smd rect (at -1.99898 0 90) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 /VIN))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 57EC99EE)
    (at 11.176 -26.67 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D3 (at 0 3.81 180) (layer B.SilkS))
    (fp_text value 15MQ040N (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (pad 1 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 14 /OUT2))
    (pad 2 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 11 /OUT))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57EC99EE)
    (at 14.986 -2.032)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /#PFO))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vpull-up))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57EC99EE)
    (at 10.922 -9.398)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /PG))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vpull-up))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-1206 (layer B.Cu) (tedit 57EC99EE)
    (at 11.176 -26.67)
    (attr smd)
    (fp_text reference R7 (at 0 -2.286) (layer B.SilkS))
    (fp_text value 0R (at 0 0.127) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 11 /OUT))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 14 /OUT2))
    (model MLAB_3D/Resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:DJNR5040 (layer B.Cu) (tedit 57EC99EE)
    (at 23.876 -23.114 180)
    (descr DJNR5040)
    (fp_text reference L1 (at 0 0 180) (layer B.SilkS))
    (fp_text value DJNR5040-3R3-S (at 0.0127 -2.8956 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -1.8 0 180) (size 1.6 4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at 1.8 0 180) (size 1.6 4) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(L1-Pad1)"))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:DJNR5040 (layer B.Cu) (tedit 57EC99EE)
    (at 23.876 -17.018 180)
    (descr DJNR5040)
    (fp_text reference L2 (at 0 0 180) (layer B.SilkS))
    (fp_text value DJNR5040-3R3-S (at 0.0127 -2.8956 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -1.8 0 180) (size 1.6 4) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at 1.8 0 180) (size 1.6 4) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(L2-Pad1)"))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 57EC9C2B)
    (at 24.638 -10.16 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C4 (at 0.0127 -0.0381 90) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 /VIN))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text Vp (at 11.176 -1.778 270) (layer F.SilkS))
  (gr_text MLAB.CZ (at 12.954 -38.862 180) (layer B.Cu))
  (gr_text 2016 (at 27.813 -36.0045) (layer F.SilkS))
  (gr_text JACHO (at 27.7495 -38.4175) (layer F.SilkS))
  (gr_text MLAB.CZ (at 22.7965 -18.6055 90) (layer F.SilkS))
  (gr_text SUPERCAP01B (at 20.574 -17.3355 90) (layer F.SilkS))
  (gr_text VS (at 21.336 -3.048 270) (layer F.SilkS))
  (gr_text EN (at 18.796 -3.302 270) (layer F.SilkS))
  (gr_text IN (at 36.195 -10.922) (layer F.SilkS))
  (gr_text POWER (at 36.068 -12.827) (layer F.SilkS))
  (gr_text VIN (at 22.0345 -10.033) (layer F.SilkS))
  (gr_text "#PFO" (at 15.1765 -9.4615) (layer F.SilkS))
  (gr_text PG (at 13.716 -1.778 270) (layer F.SilkS))
  (gr_text OUT (at 1.2065 -24.3205 270) (layer F.SilkS))
  (gr_text POWER (at 8.509 -24.384 270) (layer F.SilkS))
  (gr_text + (at 15.875 -18.415) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -0.254) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -40.386) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -40.386) (end 40.386 -40.386) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /VIN) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.272 -17.399) (xy 17.526 -17.399) (xy 17.526 -16.637) (xy 17.526 -16.51) (xy 17.653 -16.383)
        (xy 17.907 -16.383) (xy 19.939 -14.351) (xy 23.876 -10.414) (xy 30.607 -10.414) (xy 32.512 -12.319)
        (xy 34.544 -12.319) (xy 34.544 -10.033) (xy 32.512 -8.001) (xy 26.162 -7.874) (xy 26.162 -7.62)
        (xy 26.162 -6.604) (xy 26.162 -6.096) (xy 17.78 -6.096) (xy 17.78 -6.477) (xy 17.78 -8.128)
        (xy 18.161 -8.763) (xy 18.415 -9.144) (xy 18.669 -9.525) (xy 18.669 -11.303) (xy 19.05 -11.684)
        (xy 19.685 -11.684) (xy 19.939 -11.938) (xy 19.939 -12.446) (xy 19.304 -13.081) (xy 19.05 -13.335)
        (xy 17.526 -13.335) (xy 17.145 -13.716) (xy 17.145 -17.399)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -0.381 -40.767) (xy 40.767 -40.767) (xy 40.767 0.635) (xy -1.397 0.635) (xy -1.397 -40.767)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.032 -41.783) (xy 42.291 -41.783) (xy 42.291 2.794) (xy -4.191 2.794) (xy -4.191 -41.783)
        (xy -1.778 -41.783)
      )
    )
  )
  (zone (net 9) (net_name "Net-(L2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.78 -17.526) (xy 22.86 -17.526) (xy 22.86 -14.986) (xy 19.812 -14.986) (xy 18.034 -16.764)
        (xy 17.78 -16.764)
      )
    )
  )
  (zone (net 8) (net_name "Net-(L1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.78 -19.558) (xy 18.542 -19.558) (xy 20.066 -21.082) (xy 23.114 -21.082) (xy 23.114 -25.4)
        (xy 21.082 -25.4) (xy 17.78 -22.098)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.638 -14.986) (xy 26.924 -14.986) (xy 26.924 -18.542) (xy 28.956 -20.574) (xy 28.956 -25.654)
        (xy 21.336 -33.274) (xy 19.05 -33.274) (xy 19.05 -29.972) (xy 24.638 -24.384)
      )
    )
  )
  (zone (net 11) (net_name /OUT) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.526 -19.558) (xy 17.526 -22.098) (xy 17.526 -25.146) (xy 17.526 -29.464) (xy 14.732 -32.258)
        (xy 11.938 -32.512) (xy 11.938 -25.4) (xy 8.128 -21.59) (xy 8.128 -16.256) (xy 8.128 -16.002)
        (xy 12.192 -16.002) (xy 12.192 -22.606) (xy 13.208 -23.622) (xy 15.494 -23.622) (xy 16.764 -22.352)
        (xy 17.018 -22.098) (xy 17.018 -19.558)
      )
    )
  )
)
