(kicad_pcb (version 20170123) (host pcbnew "(2017-02-05 revision 431abcf)-makepkg")
  (general
    (links 85)
    (no_connects 0)
    (area -8.659285 -49.299286 37.465001 8.001001)
    (thickness 1.6)
    (drawings 21)
    (tracks 312)
    (zones 0)
    (modules 36)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 1.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(C10-Pad1)")
  (net 4 "Net-(C11-Pad2)")
  (net 5 /Vout+)
  (net 6 /Vout-)
  (net 7 "Net-(C16-Pad1)")
  (net 8 /EN+)
  (net 9 /EN-)
  (net 10 /PGOOD)
  (net 11 /C1-)
  (net 12 /C1+)
  (net 13 /CP)
  (net 14 /FB+)
  (net 15 /FB-)
  (net 16 "Net-(C1-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /C1+)
    (add_net /C1-)
    (add_net /CP)
    (add_net /EN+)
    (add_net /EN-)
    (add_net /FB+)
    (add_net /FB-)
    (add_net /PGOOD)
    (add_net /Vout+)
    (add_net /Vout-)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net VCC)
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 14.478 -23.622)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:WSON-12 (layer B.Cu) (tedit 58AE8669)
    (at 16.256 -20.066)
    (descr "WSON 12")
    (tags DRV8835)
    (fp_text reference U1 (at 0.254 -0.0508) (layer B.SilkS))
    (fp_text value LM27762 (at 0.1651 2.0574) (layer B.Fab) hide)
    (fp_text user * (at -1.7145 -1.7272) (layer B.SilkS))
    (pad 13 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.4) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 13 thru_hole circle (at -0.7 0) (size 0.5 0.5) (drill 0.4) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 13 thru_hole circle (at 0.7 0) (size 0.5 0.5) (drill 0.4) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 13 smd trapezoid (at -1.35 -0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd trapezoid (at -1.35 0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd trapezoid (at 1.35 0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd trapezoid (at 1.35 -0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd trapezoid (at 0 0) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd trapezoid (at -1.25 0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /EN+))
    (pad 11 smd trapezoid (at -0.75 0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 10 smd trapezoid (at -0.25 0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 /C1+))
    (pad 9 smd trapezoid (at 0.25 0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 /C1-))
    (pad 8 smd trapezoid (at 0.75 0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /EN-))
    (pad 7 smd trapezoid (at 1.25 0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 /FB-))
    (pad 6 smd trapezoid (at 1.25 -0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (pad 5 smd trapezoid (at 0.75 -0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 13 /CP))
    (pad 4 smd trapezoid (at 0.25 -0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd trapezoid (at -0.25 -0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd trapezoid (at -0.75 -0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 14 /FB+))
    (pad 1 smd trapezoid (at -1.25 -0.95) (size 0.28 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 /PGOOD))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 7 "Net-(C16-Pad1)") (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 25.4 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 7 "Net-(C16-Pad1)") (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 25.4 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 7 "Net-(C16-Pad1)") (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 589027DC)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 7 "Net-(C16-Pad1)") (clearance 1) (zone_connect 2))
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 58AFFEDA)
    (at 14.732 -30.988 180)
    (fp_text reference C1 (at 0 0 180) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0 0 180) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 180) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 14.478 -25.654)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 14.478 -27.686)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 16.51 -16.764)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /C1-))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /C1+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 16.51 -14.732)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /C1+))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /C1-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.78 -23.622 180)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /CP))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.636 -18.542 90)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 23.622 -20.574 90)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.668 -18.542 90)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.59 -20.574 90)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 12.7 -18.542 90)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 58AFFED2)
    (at 9.906 -14.605)
    (fp_text reference C14 (at 0.254 0) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.35 0) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vout+))
    (pad 2 smd rect (at 0 0) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 58AFFECC)
    (at 23.7236 -16.5354 180)
    (fp_text reference C15 (at 0 0 180) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 180) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /Vout-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.843 -4.0005 90)
    (attr smd)
    (fp_text reference C16 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMA_Standard (layer B.Cu) (tedit 58AFFEC7)
    (at 21.336 -29.972 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0.254 180) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 180) (layer B.SilkS))
    (pad 1 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55DC1460)
    (at 15.24 -35.56 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J1 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value HEADER_2x03_PARALLEL (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C1-Pad1)"))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C1-Pad1)"))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 5.08 -26.162)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value HEADER_2x01_PARALLEL (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /EN+))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /EN+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 5.08 -28.702)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value HEADER_2x01_PARALLEL (at 0 2.54) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /EN-))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /EN-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 5.08 -23.622)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value HEADER_2x01_PARALLEL (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /PGOOD))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /PGOOD))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x05 (layer F.Cu) (tedit 58AFF2DF)
    (at 15.24 -9.906 90)
    (descr "pin header straight 2x05")
    (tags "pin header straight 2x05")
    (fp_text reference J5 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value HEADER_2x05_PARALLEL (at 0 7.62 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -5.08 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Vout-))
    (pad 4 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Vout-))
    (pad 5 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /Vout+))
    (pad 6 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /Vout+))
    (pad 7 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Vout-))
    (pad 8 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Vout-))
    (pad 9 thru_hole rect (at -1.27 5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole rect (at 1.27 5.08 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x05.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.414 -26.162 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /EN+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.414 -28.702 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 /EN-))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.414 -23.876 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 /PGOOD))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 6.604 -18.542 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 210k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /FB+))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vout+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 8.128 -21.082)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 120k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /FB+))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 20.3454 -16.764 270)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 120k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /FB-))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 21.2471 -14.097)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 210 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /FB-))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /Vout-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 11.176 -4.0005 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C16-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 19.558 -20.574 90)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.78 -25.654)
    (attr smd)
    (fp_text reference C17 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /CP))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Uset (at 16.1544 -2.0066) (layer F.SilkS))
  (gr_text ±1V8 (at 15.367 -4.0894) (layer F.SilkS))
  (gr_text JACHO (at 4.572 -12.7) (layer F.SilkS))
  (gr_text Uout (at 15.1638 -6.223) (layer F.SilkS))
  (gr_text ±3V3 (at 10.2616 -1.9558) (layer F.SilkS))
  (gr_text ±5V (at 12.2174 -3.9624) (layer F.SilkS))
  (gr_text + (at 15.24 -13.462) (layer F.SilkS))
  (gr_text - (at 17.78 -13.462) (layer F.SilkS))
  (gr_text - (at 12.7 -13.462) (layer F.SilkS))
  (gr_text 2.7-5.5V (at 15.24 -31.75) (layer F.SilkS))
  (gr_text "POWER IN" (at 15.24 -39.116) (layer F.SilkS))
  (gr_text PG (at 8.128 -23.622) (layer F.SilkS))
  (gr_text EN+ (at 8.128 -26.162) (layer F.SilkS))
  (gr_text mlab.cz (at 21.6408 -25.1968 90) (layer F.SilkS))
  (gr_text SYMPOWER02A (at 26.1366 -20.193 90) (layer F.SilkS))
  (gr_text 2017 (at 4.826 -10.668) (layer F.SilkS))
  (gr_text EN- (at 8.128 -28.702) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 30.226 -40.386) (end 30.226 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 30.226 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name "Net-(C16-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.433 4.318) (xy -7.493 8.001) (xy -2.159 -42.291) (xy 37.465 -43.688)
      )
    )
  )
  (zone (net 7) (net_name "Net-(C16-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.623 0.762) (xy -1.905 2.159) (xy -1.016 -41.148) (xy 32.131 -41.91)
      )
    )
  )
  (zone (net 11) (net_name /C1-) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.256 -19.431) (xy 16.256 -18.796) (xy 16.764 -17.653) (xy 16.764 -13.843) (xy 18.161 -13.843)
        (xy 18.161 -17.653) (xy 17.526 -18.288) (xy 17.018 -18.288) (xy 16.764 -18.542) (xy 16.637 -18.669)
        (xy 16.637 -19.431)
      )
    )
  )
  (zone (net 12) (net_name /C1+) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15.748 -19.431) (xy 15.748 -18.542) (xy 14.986 -17.653) (xy 14.986 -13.843) (xy 16.129 -13.843)
        (xy 16.129 -19.431)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C10-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15.621 -19.431) (xy 15.621 -18.542) (xy 14.097 -17.018) (xy 7.874 -17.018) (xy 7.874 -18.161)
        (xy 14.351 -18.161) (xy 14.605 -18.161) (xy 15.24 -18.669) (xy 15.24 -19.431)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C11-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.511 -20.701) (xy 17.272 -20.701) (xy 17.272 -21.336) (xy 17.907 -21.336) (xy 18.669 -22.098)
        (xy 24.511 -22.098)
      )
    )
  )
  (zone (net 13) (net_name /CP) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.764 -20.701) (xy 16.764 -21.59) (xy 18.034 -22.86) (xy 18.034 -26.543) (xy 19.431 -26.543)
        (xy 19.431 -22.733) (xy 19.177 -22.479) (xy 18.669 -22.479) (xy 18.034 -21.844) (xy 17.526 -21.844)
        (xy 17.272 -21.59) (xy 17.272 -20.701)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.129 -20.701) (xy 16.129 -21.717) (xy 15.494 -22.352) (xy 14.605 -22.352) (xy 14.224 -22.733)
        (xy 14.224 -28.575) (xy 12.827 -28.575) (xy 12.827 -22.733) (xy 13.335 -22.733) (xy 13.843 -22.225)
        (xy 14.097 -21.971) (xy 15.113 -21.971) (xy 15.24 -21.971) (xy 15.748 -21.463) (xy 15.748 -21.336)
        (xy 15.748 -20.701)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27.051 -4.318) (xy 3.175 -4.318) (xy 3.175 -33.147) (xy 7.112 -33.909) (xy 7.112 -38.989)
        (xy 23.27998 -38.989) (xy 23.495 -34.29) (xy 27.051 -33.02)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.003 -6.985) (xy 22.479 -4.318) (xy 7.874 -4.318) (xy 5.969 -6.731) (xy 3.175 -7.239)
        (xy 3.175 -33.655) (xy 5.588 -35.433) (xy 6.2484 -38.5064) (xy 23.5204 -38.5064) (xy 23.622 -34.544)
        (xy 27.051 -33.02) (xy 27.051 -7.493)
      )
    )
  )
)
