(kicad_pcb (version 4) (host pcbnew 0.201508310901+6136~28~ubuntu14.04.1-product)
  (general
    (links 56)
    (no_connects 0)
    (area -2.794 -40.442 56.387 12.700001)
    (thickness 1.6)
    (drawings 31)
    (tracks 216)
    (zones 0)
    (modules 26)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF6F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(T1-Pad2)")
  (net 10 "Net-(T2-Pad2)")
  (net 11 /VAUX)
  (net 12 /T-)
  (net 13 /T+)
  (net 14 /V_OUT)
  (net 15 /C+)
  (net 16 /V_OUT2)
  (net 17 /VS1)
  (net 18 /VS2)
  (net 19 /VOUT2_EN)
  (net 20 /PGOOD)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /C+)
    (add_net /PGOOD)
    (add_net /T+)
    (add_net /T-)
    (add_net /VAUX)
    (add_net /VOUT2_EN)
    (add_net /VS1)
    (add_net /VS2)
    (add_net /V_OUT)
    (add_net /V_OUT2)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(T1-Pad2)")
    (add_net "Net-(T2-Pad2)")
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.97 -12.192 90)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 1uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /VAUX))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 55DC14DA)
    (at 7.366 -12.954 90)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J1 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP1X3 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54 90) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /VAUX))
    (pad 2 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 /VS1))
    (pad 1 thru_hole rect (at 0 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 18.034 -14.478 90)
    (attr smd)
    (fp_text reference C7 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2,2uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.686 -14.224 90)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 470pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 25.146 -15.113)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 27.432 -4.318 270)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 470pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 25.4 -4.445 270)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 54BBE3C9)
    (at 15.748 -3.81 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C1 (at -0.20066 3.29946 270) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 270) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 270) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 12 /T-))
    (pad 1 smd rect (at -2.52476 0 270) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 13 /T+))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 54BBE3ED)
    (at 14.224 -19.05 180)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C8 (at -0.20066 0 180) (layer B.SilkS))
    (fp_text value 470uF (at -0.09906 -3.59918 180) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908 180) (layer B.SilkS))
    (pad 2 smd rect (at 3.175 0 180) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.175 0 180) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 14 /V_OUT))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Energy_harv:Step-Up_TRANSF (layer B.Cu) (tedit 55A7B4FA)
    (at 33.02 -3.175 180)
    (fp_text reference T1 (at 0 0.381 180) (layer B.SilkS))
    (fp_text value Step-Up_TRANSFO (at 0 5.25 180) (layer B.Fab))
    (pad 1 smd rect (at -2.5 1.9 180) (size 1.4 2.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /T+))
    (pad 2 smd rect (at 1.9 2.5 180) (size 2.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(T1-Pad2)"))
    (pad 3 smd rect (at 2.5 -1.9 180) (size 1.4 2.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.9 -2.4 180) (size 2.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Energy_harv:Step-Up_TRANSF (layer B.Cu) (tedit 55A7B4FA)
    (at 33.02 -12.065)
    (fp_text reference T2 (at -0.254 0.889) (layer B.SilkS))
    (fp_text value Step-Up_TRANSFO (at 0 5.25) (layer B.Fab))
    (pad 1 smd rect (at -2.5 1.9) (size 1.4 2.6) (layers B.Cu B.Paste B.Mask)
      (net 12 /T-))
    (pad 2 smd rect (at 1.9 2.5) (size 2.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(T2-Pad2)"))
    (pad 3 smd rect (at 2.5 -1.9) (size 1.4 2.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.9 -2.4) (size 2.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
  )
  (module SMD_Packages:SSOP-20 (layer B.Cu) (tedit 0)
    (at 22.71876 -10.7033 90)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U2 (at 0 0.635 90) (layer B.SilkS))
    (fp_text value LTC3109GN (at 0 -0.635 90) (layer B.Fab))
    (pad 1 smd rect (at -2.921 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 17 /VS1))
    (pad 2 smd rect (at -2.286 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 18 /VS2))
    (pad 3 smd rect (at -1.6256 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 15 /C+))
    (pad 4 smd rect (at -0.9652 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 11 /VAUX))
    (pad 5 smd rect (at -0.3302 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 14 /V_OUT))
    (pad 6 smd rect (at 0.3302 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 16 /V_OUT2))
    (pad 7 smd rect (at 0.9906 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 19 /VOUT2_EN))
    (pad 8 smd rect (at 1.6256 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 20 /PGOOD))
    (pad 9 smd rect (at 2.286 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 10 smd rect (at 2.921 -2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.921 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 12 smd rect (at 2.286 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 13 smd rect (at 1.6256 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 0.9906 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(T2-Pad2)"))
    (pad 15 smd rect (at 0.3302 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 13 /T+))
    (pad 16 smd rect (at -0.3302 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 12 /T-))
    (pad 17 smd rect (at -0.9652 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(T1-Pad2)"))
    (pad 18 smd rect (at -1.6256 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 19 smd rect (at -2.286 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 20 smd rect (at -2.921 2.667 90) (size 0.4064 1.27) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 55DC14DE)
    (at 7.366 -15.494 90)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J2 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP1X3 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54 90) (layer F.SilkS))
    (pad 3 thru_hole rect (at 0 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /VAUX))
    (pad 2 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 /VS2))
    (pad 1 thru_hole rect (at 0 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 10.922 -25.4)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP1X2 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VOUT2_EN))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VOUT2_EN))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 13.462 -25.4)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP1X2 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PGOOD))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PGOOD))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55DC1460)
    (at 27.686 -25.4 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J5 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP2X3 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /V_OUT2))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /V_OUT2))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 55DC1460)
    (at 19.05 -25.4 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J6 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP2X3 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /V_OUT))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /V_OUT))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55DC14C2)
    (at 7.62 -6.35)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P1 (at -4.826 -3.556) (layer F.SilkS) hide)
    (fp_text value WAGO256 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 /T+))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 /T+))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55DC14C8)
    (at 7.62 -1.27)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P2 (at -4.826 -3.556) (layer F.SilkS) hide)
    (fp_text value WAGO256 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 /T-))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 /T-))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55DC14D2)
    (at 26.67 2.54 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P3 (at -4.826 -3.556 90) (layer F.SilkS) hide)
    (fp_text value WAGO256 (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Mlab_Con:WAGO256 (layer F.Cu) (tedit 55DC14CD)
    (at 21.59 2.54 90)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P4 (at -4.826 -3.556 90) (layer F.SilkS) hide)
    (fp_text value WAGO256 (at 0.254 4.064 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 /C+))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 /C+))
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 54BBE3C9)
    (at 27.686 -20.066)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C10 (at 0 0) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 16 /V_OUT2))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 49.737 -10.16 90) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -30.226) (xy 51.087 -30.226)))
    (feature2 (pts (xy 40.386 9.906) (xy 51.087 9.906)))
    (crossbar (pts (xy 48.387 9.906) (xy 48.387 -30.226)))
    (arrow1a (pts (xy 48.387 -30.226) (xy 48.973421 -29.099496)))
    (arrow1b (pts (xy 48.387 -30.226) (xy 47.800579 -29.099496)))
    (arrow2a (pts (xy 48.387 9.906) (xy 48.973421 8.779496)))
    (arrow2b (pts (xy 48.387 9.906) (xy 47.800579 8.779496)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "40,132 mm" (at 20.32 -38.942) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -30.226) (xy 40.386 -40.292)))
    (feature2 (pts (xy 0.254 -30.226) (xy 0.254 -40.292)))
    (crossbar (pts (xy 0.254 -37.592) (xy 40.386 -37.592)))
    (arrow1a (pts (xy 40.386 -37.592) (xy 39.259496 -37.005579)))
    (arrow1b (pts (xy 40.386 -37.592) (xy 39.259496 -38.178421)))
    (arrow2a (pts (xy 0.254 -37.592) (xy 1.380504 -37.005579)))
    (arrow2b (pts (xy 0.254 -37.592) (xy 1.380504 -38.178421)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 45.292 -10.16 90) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -30.226) (xy 46.642 -30.226)))
    (feature2 (pts (xy 40.386 9.906) (xy 46.642 9.906)))
    (crossbar (pts (xy 43.942 9.906) (xy 43.942 -30.226)))
    (arrow1a (pts (xy 43.942 -30.226) (xy 44.528421 -29.099496)))
    (arrow1b (pts (xy 43.942 -30.226) (xy 43.355579 -29.099496)))
    (arrow2a (pts (xy 43.942 9.906) (xy 44.528421 8.779496)))
    (arrow2b (pts (xy 43.942 9.906) (xy 43.355579 8.779496)))
  )
  (dimension 40.132 (width 0.3) (layer Dwgs.User)
    (gr_text "1,5800 in" (at 20.32 -34.751) (layer Dwgs.User))
    (feature1 (pts (xy 40.386 -30.226) (xy 40.386 -36.101)))
    (feature2 (pts (xy 0.254 -30.226) (xy 0.254 -36.101)))
    (crossbar (pts (xy 0.254 -33.401) (xy 40.386 -33.401)))
    (arrow1a (pts (xy 40.386 -33.401) (xy 39.259496 -32.814579)))
    (arrow1b (pts (xy 40.386 -33.401) (xy 39.259496 -33.987421)))
    (arrow2a (pts (xy 0.254 -33.401) (xy 1.380504 -32.814579)))
    (arrow2b (pts (xy 0.254 -33.401) (xy 1.380504 -33.987421)))
  )
  (gr_text 4 (at 13.462 -28.956) (layer F.SilkS))
  (gr_text 3 (at 10.922 -28.956) (layer F.SilkS))
  (gr_text 2015 (at 13.716 6.096) (layer B.Cu))
  (gr_text MLAB.CZ (at 13.716 3.81) (layer B.Cu))
  (gr_text THERMOGEN01A (at 21.082 -18.542) (layer F.SilkS))
  (gr_text 2015 (at 35.179 -5.842) (layer F.SilkS))
  (gr_text MLAB.CZ (at 21.082 -20.828) (layer F.SilkS))
  (gr_text Vout2 (at 27.686 -28.956) (layer F.SilkS))
  (gr_text Vout (at 18.796 -28.956) (layer F.SilkS))
  (gr_text "VOUT SET" (at 7.366 -20.32) (layer F.SilkS))
  (gr_text 4-PGOOD (at 16.51 -13.462) (layer F.SilkS))
  (gr_text 3-Vout2_EN (at 16.51 -15.748) (layer F.SilkS))
  (gr_text C- (at 30.607 -1.143 90) (layer F.SilkS))
  (gr_text C+ (at 16.764 4.826 90) (layer F.SilkS))
  (gr_text "Vout\n2,35V\n3,3V\n4,1V\n5V" (at 33.274 -14.732) (layer F.SilkS))
  (gr_text "Y\n1\n2\n1\n2" (at 31.496 -14.732) (layer F.SilkS))
  (gr_text "X\n1\n1\n2\n2" (at 29.718 -14.732) (layer F.SilkS))
  (gr_text X (at 2.032 -15.494) (layer F.SilkS))
  (gr_text 1 (at 5.842 -18.034) (layer F.SilkS))
  (gr_text Y (at 2.032 -12.954) (layer F.SilkS))
  (gr_text 2 (at 8.636 -18.034) (layer F.SilkS))
  (gr_text T- (at 10.922 2.794) (layer F.SilkS))
  (gr_text T+ (at 10.668 -10.16) (layer F.SilkS))
  (gr_line (start 0.254 9.906) (end 0.254 -30.226) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 9.906) (end 0.254 9.906) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -30.226) (end 40.386 9.906) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -30.226) (end 40.386 -30.226) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.27 -31.242) (xy 43.18 -31.242) (xy 43.18 11.43) (xy -1.27 11.43)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.794 -31.242) (xy 46.736 -31.242) (xy 46.99 12.7) (xy -2.54 12.7)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.576 -4.064) (xy 29.718 -4.064) (xy 28.702 -4.064) (xy 27.686 -4.064) (xy 24.638 -4.064)
        (xy 24.638 -2.794) (xy 31.75 -2.794) (xy 33.528 0.254) (xy 36.576 0.254) (xy 36.576 0)
      )
    )
  )
  (zone (net 9) (net_name "Net-(T1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.512 -4.572) (xy 29.464 -4.572) (xy 29.464 -6.604) (xy 26.67 -9.398) (xy 24.638 -9.398)
        (xy 24.638 -10.16) (xy 26.67 -10.16) (xy 27.94 -10.16) (xy 30.988 -7.112) (xy 33.02 -7.112)
        (xy 33.02 -4.572)
      )
    )
  )
  (zone (net 12) (net_name /T-) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.242 -9.144) (xy 29.718 -9.144) (xy 28.448 -10.414) (xy 28.448 -10.541) (xy 29.591 -11.684)
        (xy 31.242 -11.684)
      )
    )
  )
  (zone (net 13) (net_name /T+) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.544 -3.302) (xy 37.338 -3.302) (xy 37.338 -6.858) (xy 31.242 -6.858) (xy 28.194 -9.906)
        (xy 28.194 -11.43) (xy 26.162 -11.43) (xy 26.162 -8.636) (xy 31.496 -3.302) (xy 34.544 -3.302)
      )
    )
  )
  (zone (net 13) (net_name /T+) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37.338 -3.302) (xy 34.544 -3.302) (xy 34.544 -6.858) (xy 37.338 -6.858)
      )
    )
  )
  (zone (net 10) (net_name "Net-(T2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.528 -8.89) (xy 30.734 -11.684) (xy 26.416 -11.684) (xy 26.416 -12.7) (xy 36.83 -12.7)
        (xy 36.83 -8.636) (xy 33.528 -8.636)
      )
    )
  )
  (zone (net 6) (net_name "Net-(C4-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.972 -16.256) (xy 30.48 -15.748) (xy 32.766 -15.748) (xy 32.766 -13.462) (xy 28.956 -13.462)
        (xy 28.956 -14.224) (xy 25.4 -14.224) (xy 25.4 -16.256)
      )
    )
  )
  (zone (net 15) (net_name /C+) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.304 -9.398) (xy 22.606 -9.398) (xy 22.606 -2.286) (xy 23.876 -2.286) (xy 23.876 7.62)
        (xy 19.05 7.62) (xy 19.05 -2.286) (xy 21.082 -2.286) (xy 21.082 -8.636) (xy 19.304 -8.636)
      )
    )
  )
  (zone (net 14) (net_name /V_OUT) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.05 -10.668) (xy 18.542 -10.668) (xy 16.764 -12.446) (xy 16.764 -15.748) (xy 18.796 -17.78)
        (xy 18.796 -20.574) (xy 20.066 -21.844) (xy 20.066 -27.686) (xy 18.034 -27.686) (xy 18.034 -23.114)
        (xy 15.494 -20.574) (xy 15.494 -17.526) (xy 14.986 -17.018) (xy 14.986 -11.938) (xy 16.764 -10.16)
        (xy 19.05 -10.16)
      )
    )
  )
  (zone (net 16) (net_name /V_OUT2) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21.336 -11.938) (xy 21.336 -11.557) (xy 22.098 -11.557) (xy 22.098 -12.192) (xy 22.098 -16.764)
        (xy 23.876 -18.542) (xy 26.67 -18.542) (xy 26.67 -21.59) (xy 27.686 -22.606) (xy 28.702 -22.606)
        (xy 28.702 -27.686) (xy 26.67 -27.686) (xy 26.67 -23.114) (xy 26.162 -22.606) (xy 23.622 -22.606)
        (xy 23.622 -21.59) (xy 21.336 -19.304) (xy 21.336 -11.938)
      )
    )
  )
  (zone (net 16) (net_name /V_OUT2) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19.558 -11.176) (xy 21.209 -11.176) (xy 21.209 -13.335) (xy 22.225 -13.335) (xy 22.225 -10.922)
        (xy 20.828 -10.922) (xy 19.558 -10.922)
      )
    )
  )
  (zone (net 16) (net_name /V_OUT2) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.67 -27.686) (xy 26.67 -23.114) (xy 26.162 -22.606) (xy 23.622 -22.606) (xy 23.622 -18.542)
        (xy 26.67 -18.542) (xy 26.67 -21.59) (xy 28.448 -23.368) (xy 28.448 -27.686)
      )
    )
  )
)
