(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 40)
    (no_connects 0)
    (area 0.178999 -40.461001 40.461001 -0.178999)
    (thickness 1.6)
    (drawings 14)
    (tracks 51)
    (zones 0)
    (modules 32)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1.3)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.89)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(CON1-Pad3)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad1)")
  (net 10 "Net-(F1-Pad1)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J4-Pad1)")
  (net 13 VCC)
  (net 14 "Net-(D5-Pad1)")
  (net 15 "Net-(D5-Pad2)")
  (net 16 "Net-(CON1-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net VCC)
  )
  (net_class gnd ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net GND)
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -15.24)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 5535DB57)
    (at 28.702 -5.9055 180)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J8 (at 0 -6.35 180) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 4 thru_hole rect (at 1.27 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 5 thru_hole rect (at -1.27 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 6 thru_hole rect (at 1.27 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 7 thru_hole rect (at -1.27 3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_CON:DC2,1MM placed (layer F.Cu) (tedit 56C181FF)
    (at 14.351 -10.922 90)
    (tags "DC2,1MM nap. konektor")
    (fp_text reference CON1 (at 5.842 0.0635 180) (layer F.SilkS))
    (fp_text value JACK_DC2.1 (at 2.2225 3.5433 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 2.39 0 90) (size 3.81 3.81) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 3.81 3.81) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(CON1-Pad1)"))
    (pad 3 thru_hole rect (at -0.71 -5 90) (size 3.81 3.81) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(CON1-Pad3)"))
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 54BBE5C1)
    (at 23.8125 -4.699)
    (fp_text reference FI1 (at 0 2.413) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 22.352 -15.4305)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(CON1-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(CON1-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 22.352 -22.606)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 24.892 -22.606)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J4-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J4-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 24.892 -15.4305)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN1_2 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(F1-Pad1)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(F1-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56C2B848)
    (at 38.354 -35.052)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D2-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56C2B850)
    (at 38.354 -29.972)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D3-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 56C18311)
    (at 29.083 -27.4955 180)
    (attr smd)
    (fp_text reference R1 (at -1.9685 0.0635 270) (layer F.SilkS))
    (fp_text value 2k2 (at 0.127 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 56C18326)
    (at 29.0195 -37.465 180)
    (attr smd)
    (fp_text reference R2 (at -1.9685 0.0635 270) (layer F.SilkS))
    (fp_text value 2k2 (at 0.0635 -1.3335 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 56C18316)
    (at 29.083 -29.718 180)
    (attr smd)
    (fp_text reference R3 (at -1.9685 0 270) (layer F.SilkS))
    (fp_text value 2k2 (at 0.127 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_SW:Prepinaci_3A_SL19121 placed (layer B.Cu) (tedit 56C182DE)
    (at 23.622 -33.02 180)
    (tags "Prepinaci tlacitko 3A")
    (fp_text reference SW1 (at -4.318 1.8415 270) (layer B.SilkS))
    (fp_text value SL19121 (at -4.5593 0.2667 450) (layer B.SilkS) hide)
    (pad 3 thru_hole rect (at 0 -4.7 180) (size 3.4 3.4) (drill 2.3) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole rect (at 0 0 180) (size 3.4 3.4) (drill 2.3) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(J4-Pad1)"))
    (pad 1 thru_hole rect (at 0 4.7 180) (size 3.4 3.4) (drill 2.3) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(J2-Pad1)"))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -15.24)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M5 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M8 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 56C2B84D)
    (at 38.354 -32.512)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J12 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D5-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer F.Cu) (tedit 56C18309)
    (at 29.0195 -32.512 180)
    (attr smd)
    (fp_text reference R4 (at -1.9685 0.0635 270) (layer F.SilkS))
    (fp_text value 2k2 (at 0.0635 1.397 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer F.Cu) (tedit 56C18290)
    (at 33.9725 -22.5 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at -4.318 -0.021 180) (layer F.SilkS))
    (fp_text value RED (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user A (at -1.80086 1.5494 180) (layer F.SilkS))
    (fp_text user K (at 1.80086 1.5494 180) (layer F.SilkS))
    (pad 2 smd rect (at -2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer F.Cu) (tedit 56C182C0)
    (at 33.9725 -37.5 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 -2.5115 180) (layer F.SilkS))
    (fp_text value RED (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user A (at -1.80086 1.5494 180) (layer F.SilkS))
    (fp_text user K (at 1.80086 1.5494 180) (layer F.SilkS))
    (pad 2 smd rect (at -2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer F.Cu) (tedit 56C182CC)
    (at 33.9725 -27.4955 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at -0.0635 -2.6035 180) (layer F.SilkS))
    (fp_text value GREEN (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user A (at -1.80086 1.5494 180) (layer F.SilkS))
    (fp_text user K (at 1.80086 1.5494 180) (layer F.SilkS))
    (pad 2 smd rect (at -2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at 2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 56BDB339)
    (at 13.0175 -2.54)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D4 (at -2.4765 0.0635) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926) (layer B.SilkS))
    (pad 2 smd rect (at -1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.99898 0) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer F.Cu) (tedit 56C182C6)
    (at 33.9725 -32.5 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D5 (at 0 -2.5915 180) (layer F.SilkS))
    (fp_text value ORANGE (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user A (at -1.80086 1.5494 180) (layer F.SilkS))
    (fp_text user K (at 1.80086 1.5494 180) (layer F.SilkS))
    (pad 2 smd rect (at -2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at 2 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 29.972 -15.4305)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 VCC))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 29.972 -22.606)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 27.432 -22.606)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 27.432 -15.4305)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_F:Drzak_2410 (layer B.Cu) (tedit 564C162A)
    (at 19.3675 -7.493 270)
    (descr "F 2410 s držákem")
    (tags "F 2410 s držákem")
    (attr smd)
    (fp_text reference F1 (at 0.13462 3.15468 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.91 0 270) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.91 0 270) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 568A4984)
    (at 1.9685 -10.287)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J13 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(CON1-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text JACHO (at 35.4965 -10.16) (layer F.SilkS))
  (gr_text 2016 (at 22.1615 -8.5725 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 20.2565 -8.4455 90) (layer F.SilkS))
  (gr_text POWER (at 24.7015 -5.842 90) (layer F.SilkS))
  (gr_text UNIPOWER03A (at 14.7955 -2.667) (layer F.SilkS))
  (gr_text MLAB (at 36.3855 -10.2235) (layer B.Cu))
  (gr_text UNIPOWER03A (at 13.2715 -18.161) (layer B.Cu))
  (gr_line (start 0.254 -20.066) (end 40.386 -20.066) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.386 -40.386) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 40.386 -0.254) (end 40.386 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 16) (net_name "Net-(CON1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.2555 -5.0165) (xy 16.4465 -5.0165) (xy 20.0025 -5.0165) (xy 23.5585 -8.5725) (xy 23.5585 -17.653)
        (xy 21.209 -17.653) (xy 21.209 -12.192) (xy 18.288 -9.271) (xy 12.192 -9.271) (xy 12.192 -5.1435)
        (xy 12.192 -5.0165)
      )
    )
  )
  (zone (net 9) (net_name "Net-(D4-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13.589 -1.397) (xy 22.987 -1.397) (xy 22.987 -6.477) (xy 17.2085 -6.477) (xy 17.2085 -4.8895)
        (xy 16.0655 -3.7465) (xy 13.589 -3.7465)
      )
    )
  )
  (zone (net 13) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.9245 -5.588) (xy 24.511 -5.588) (xy 24.511 -3.937) (xy 30.734 -3.937) (xy 30.9245 -3.937)
      )
    )
  )
  (zone (net 13) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.4795 -8.128) (xy 26.4795 -5.334) (xy 30.9245 -5.3975) (xy 32.131 -6.604) (xy 32.893 -7.366)
        (xy 32.893 -12.0015) (xy 31.242 -13.6525) (xy 31.242 -17.9705) (xy 28.8925 -17.9705) (xy 28.8925 -12.954)
        (xy 28.8925 -12.065) (xy 29.5275 -11.43) (xy 30.9245 -11.43) (xy 31.3055 -11.049) (xy 31.3055 -8.5725)
        (xy 30.988 -8.255) (xy 26.4795 -8.255)
      )
    )
  )
  (zone (net 10) (net_name "Net-(F1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.3355 -8.509) (xy 22.9235 -8.509) (xy 25.8445 -11.43) (xy 25.8445 -17.653) (xy 23.9395 -17.653)
        (xy 23.9395 -13.0175) (xy 23.241 -12.319) (xy 17.272 -12.319) (xy 17.272 -8.509)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0.254 -40.386) (xy 41.021 -40.386) (xy 41.402 0.127) (xy -0.635 0.254) (xy -1.3335 -40.386)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.3815 -41.3385) (xy 42.545 -41.148) (xy 42.926 1.3335) (xy -3.4925 1.7145)
      )
    )
  )
  (zone (net 11) (net_name "Net-(J2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.3045 -20.447) (xy 23.3045 -24.8285) (xy 22.098 -26.035) (xy 21.717 -26.035) (xy 21.717 -35.306)
        (xy 22.1615 -35.7505) (xy 25.5905 -35.7505) (xy 25.5905 -39.6875) (xy 19.431 -39.6875) (xy 19.431 -25.654)
        (xy 21.082 -23.876) (xy 21.082 -20.447)
      )
    )
  )
  (zone (net 12) (net_name "Net-(J4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.13 -20.447) (xy 24.13 -24.8285) (xy 25.5905 -26.289) (xy 25.5905 -30.5435) (xy 25.273 -30.861)
        (xy 21.717 -30.861) (xy 21.717 -34.925) (xy 26.7335 -34.925) (xy 27.051 -34.6075) (xy 27.051 -25.908)
        (xy 25.908 -24.765) (xy 25.908 -20.3835) (xy 24.13 -20.3835)
      )
    )
  )
)
