(kicad_pcb (version 20170123) (host pcbnew "(2017-02-05 revision 431abcf)-makepkg")
  (general
    (links 179)
    (no_connects 0)
    (area -11.176 -45.466 85.598001 5.080001)
    (thickness 1.6)
    (drawings 40)
    (tracks 507)
    (zones 0)
    (modules 82)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.9)
    (user_trace_width 1.3)
    (user_trace_width 6)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(CON1-Pad3)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(F1-Pad1)")
  (net 10 VCC)
  (net 11 "Net-(CON1-Pad1)")
  (net 12 "Net-(D8-Pad1)")
  (net 13 "Net-(D12-Pad1)")
  (net 14 "Net-(D13-Pad1)")
  (net 15 "Net-(D9-Pad1)")
  (net 16 "Net-(D10-Pad1)")
  (net 17 "Net-(D10-Pad2)")
  (net 18 "Net-(D11-Pad2)")
  (net 19 "Net-(D11-Pad1)")
  (net 20 "Net-(D16-Pad1)")
  (net 21 "Net-(D16-Pad2)")
  (net 22 "Net-(D18-Pad1)")
  (net 23 "Net-(D18-Pad2)")
  (net 24 "Net-(F2-Pad1)")
  (net 25 "Net-(F3-Pad1)")
  (net 26 "Net-(F5-Pad1)")
  (net 27 "Net-(F6-Pad1)")
  (net 28 "Net-(F7-Pad1)")
  (net 29 "Net-(F8-Pad1)")
  (net 30 "Net-(F9-Pad1)")
  (net 31 "Net-(F11-Pad1)")
  (net 32 "Net-(J2-Pad3)")
  (net 33 "Net-(J3-Pad3)")
  (net 34 "Net-(J4-Pad3)")
  (net 35 "Net-(J5-Pad3)")
  (net 36 "Net-(J6-Pad3)")
  (net 37 "Net-(J7-Pad3)")
  (net 38 "Net-(J8-Pad3)")
  (net 39 "Net-(J9-Pad3)")
  (net 40 "Net-(J11-Pad3)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F11-Pad1)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(F3-Pad1)")
    (add_net "Net-(F5-Pad1)")
    (add_net "Net-(F6-Pad1)")
    (add_net "Net-(F7-Pad1)")
    (add_net "Net-(F8-Pad1)")
    (add_net "Net-(F9-Pad1)")
    (add_net "Net-(J11-Pad3)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J9-Pad3)")
    (add_net VCC)
  )
  (net_class gnd ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net GND)
  )
  (module Mlab_CON:DC2,1MM placed (layer F.Cu) (tedit 5899794F)
    (at 14.224 -30.48 90)
    (tags "DC2,1MM nap. konektor")
    (fp_text reference CON1 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value JACK_DC2.1 (at 2.2225 3.5433 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 2.39 0 90) (size 3.81 3.81) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -3.81 0 90) (size 3.81 3.81) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(CON1-Pad1)"))
    (pad 3 thru_hole rect (at -0.71 -5 90) (size 3.81 3.81) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(CON1-Pad3)"))
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 2.794 -22.352 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D1 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 11.811 -3.556 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 38.354 -3.556 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089C0)
    (at 26.67 -24.892 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D4 (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089AE)
    (at 2.794 -15.24 90)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D5 (at 0 0 90) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 90) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 90) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -2.14884 0 90) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089D8)
    (at 17.018 -3.556 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D6 (at 0 0 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089E3)
    (at 43.688 -3.81 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D7 (at 0 0 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 51.816 -37.592 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D8 (at 0 0 180) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (pad 1 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 36.83 -37.592 180)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D9 (at 0 0 180) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 180) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 180) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at -2 0 180) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D13-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 78.486 -24.892 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D10 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D10-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 25.146 -3.556 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D11 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D11-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 58808986)
    (at 58.166 -37.592 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D12 (at 0 0 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 58808989)
    (at 43.18 -37.592 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D13 (at 0 -0.254 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089F1)
    (at 65.786 -23.114 90)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D14 (at 0 0 90) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.95072 90) (layer B.SilkS))
    (fp_text user A (at -3.2004 -1.95072 90) (layer B.SilkS))
    (pad 2 smd rect (at -2.14884 0 90) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.14884 0 90) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D10-Pad2)"))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089D4)
    (at 30.48 -3.556 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D15 (at 0 0 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 51.562 -3.556 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D16 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D16-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:LED_1206 (layer B.Cu) (tedit 58806C2B)
    (at 78.486 -13.97 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D18 (at 0 0 90) (layer B.SilkS))
    (fp_text value RED (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -1.80086 -1.5494 90) (layer B.SilkS))
    (fp_text user K (at 1.80086 -1.5494 90) (layer B.SilkS))
    (pad 2 smd rect (at -2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at 2 0 90) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D18-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask B.SilkS))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089E7)
    (at 57.15 -3.81 180)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D19 (at 0 0 180) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 180) (layer B.SilkS) hide)
    (fp_text user K (at 2.99974 -1.95072 180) (layer B.SilkS))
    (fp_text user A (at -3.2004 -1.95072 180) (layer B.SilkS))
    (pad 2 smd rect (at -2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.14884 0 180) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:SMB_Standard (layer B.Cu) (tedit 588089EA)
    (at 68.326 -8.382 90)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D21 (at 0.254 0 90) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -3.81 90) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072 90) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072 90) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0 90) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D18-Pad2)"))
    (pad 2 smd rect (at -2.14884 0 90) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 58806C2B)
    (at 16.002 -18.542 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 588089A9)
    (at 23.876 -15.875 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F2 (at 0.127 0 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(F2-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 588089CF)
    (at 46.736 -15.748 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F3 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(F3-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:Drzak_2410 (layer B.Cu) (tedit 58808A24)
    (at 19.304 -27.432 270)
    (descr "F 2410 s držákem")
    (tags "F 2410 s držákem")
    (attr smd)
    (fp_text reference F4 (at 0 0 270) (layer B.SilkS))
    (fp_text value 10A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.91 0 270) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 2.91 0 270) (size 3.33 3.81) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 58808A07)
    (at 52.832 -24.638)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F5 (at 0 0) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(F5-Pad1)"))
    (pad 2 smd rect (at 2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 5880899D)
    (at 40.64 -24.638)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F6 (at 0 0) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D13-Pad1)"))
    (pad 1 smd rect (at -2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(F6-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 588089F4)
    (at 62.992 -29.21)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F7 (at 0 0) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(F7-Pad1)"))
    (pad 2 smd rect (at 2.5 0) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D10-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 588089CC)
    (at 35.56 -15.748 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F8 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(F8-Pad1)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 58808A01)
    (at 58.166 -16.002 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F9 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(F9-Pad1)"))
    (pad 2 smd rect (at 2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_F:2410 (layer B.Cu) (tedit 588089FF)
    (at 62.992 -13.97 270)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference F11 (at 0 0 270) (layer B.SilkS))
    (fp_text value 1,1A (at 0 -3.81 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(F11-Pad1)"))
    (pad 2 smd rect (at 2.5 0 270) (size 2 3.18) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D18-Pad2)"))
    (model MLAB_3D/Diodes/MiniMELF_DO213AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089A7)
    (at 20.066 -18.796 270)
    (fp_text reference FI1 (at 0 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 270) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089B7)
    (at 27.94 -18.542 270)
    (fp_text reference FI2 (at 0.254 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(F2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089CA)
    (at 39.878 -18.542 270)
    (fp_text reference FI3 (at 0 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 270) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(F3-Pad1)"))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 58808A0A)
    (at 46.99 -23.368 90)
    (fp_text reference FI4 (at 0.254 0 90) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (pad 2 smd rect (at 0 0 90) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(F5-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089C7)
    (at 34.798 -23.368 90)
    (fp_text reference FI5 (at 0 0 90) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (pad 2 smd rect (at 0 0 90) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(F6-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089F6)
    (at 60.452 -24.892 90)
    (fp_text reference FI6 (at 0 0 90) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 90) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.35 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(F7-Pad1)"))
    (pad 2 smd rect (at 0 0 90) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089BA)
    (at 31.496 -18.542 270)
    (fp_text reference FI7 (at 0 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(F8-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 58808A05)
    (at 53.848 -18.796 270)
    (fp_text reference FI8 (at 0 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 270) (layer B.SilkS) hide)
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(F9-Pad1)"))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_L:FIR1 (layer B.Cu) (tedit 588089F9)
    (at 61.722 -20.32 270)
    (fp_text reference FI10 (at 0.254 0 270) (layer B.SilkS))
    (fp_text value NFM21PC105 (at 2.794 -1.905 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 VCC))
    (pad 2 smd rect (at 0 0 270) (size 0.7 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.35 0 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(F11-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.13 0.13))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x01 (layer F.Cu) (tedit 58806C2B)
    (at 6.604 -25.908)
    (descr "pin header straight 1x01")
    (tags "pin header straight 1x01")
    (fp_text reference J1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value CONN1_1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 0) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(CON1-Pad3)"))
    (model Pin_Headers/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 8.382 -17.78)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J2 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J2-Pad3)"))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J2-Pad3)"))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 16.256 -9.144 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J3 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D2-Pad2)"))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D2-Pad2)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J3-Pad3)"))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J3-Pad3)"))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 41.656 -9.144 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J4 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J4-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(J4-Pad3)"))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D3-Pad2)"))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D3-Pad2)"))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 51.816 -32.004 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J5 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J5-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(J5-Pad3)"))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D12-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D12-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 39.116 -32.004 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J6 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J6-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(J6-Pad3)"))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D13-Pad1)"))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D13-Pad1)"))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 73.914 -25.654)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J7 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D10-Pad2)"))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D10-Pad2)"))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J7-Pad3)"))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J7-Pad3)"))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 28.956 -9.144 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J8 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J8-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J8-Pad3)"))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D11-Pad2)"))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D11-Pad2)"))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 54.356 -9.144 90)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J9 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J9-Pad3)"))
    (pad 4 thru_hole rect (at 1.27 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J9-Pad3)"))
    (pad 5 thru_hole rect (at -1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D16-Pad2)"))
    (pad 6 thru_hole rect (at 1.27 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D16-Pad2)"))
    (pad 7 thru_hole rect (at -1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole rect (at 1.27 3.81 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 58806C2B)
    (at 73.914 -14.732)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J11 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D18-Pad2)"))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D18-Pad2)"))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J11-Pad3)"))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J11-Pad3)"))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 58806C2B)
    (at 76.2 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 58806C2B)
    (at 76.2 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 58806C2B)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 58806C2B)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value _ (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 2.794 -27.432 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 10.033 -8.255 90)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 35.56 -4.572 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 12.7 -20.828 90)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 12.7 -16.51 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 13.97 -13.462 180)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J3-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 17.78 -13.462)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 39.624 -13.462 180)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J4-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 43.18 -13.462)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J4-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 48.006 -36.576 270)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 33.02 -36.576 270)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 78.486 -29.464 90)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 22.098 -4.572 270)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D11-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 48.514 -27.94 180)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J5-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 52.324 -27.94)
    (attr smd)
    (fp_text reference R15 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(J5-Pad3)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D12-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 36.068 -27.94 180)
    (attr smd)
    (fp_text reference R16 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 39.878 -27.94)
    (attr smd)
    (fp_text reference R17 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D13-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 69.596 -30.48 90)
    (attr smd)
    (fp_text reference R18 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J7-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 69.596 -26.416 270)
    (attr smd)
    (fp_text reference R19 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J7-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 27.94 -13.462 180)
    (attr smd)
    (fp_text reference R20 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J8-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 31.75 -13.462)
    (attr smd)
    (fp_text reference R21 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J8-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 48.768 -4.572 270)
    (attr smd)
    (fp_text reference R22 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 78.486 -18.542 90)
    (attr smd)
    (fp_text reference R24 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 2k2 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 50.8 -13.462 180)
    (attr smd)
    (fp_text reference R25 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J9-Pad3)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 54.356 -13.462)
    (attr smd)
    (fp_text reference R26 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J9-Pad3)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D16-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 69.596 -18.542 90)
    (attr smd)
    (fp_text reference R29 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J11-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 58806C2B)
    (at 69.596 -14.732 270)
    (attr smd)
    (fp_text reference R30 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 0 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J11-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D18-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 58806C2B)
    (at 24.384 -32.766 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J12 (at -5.842 0) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(CON1-Pad1)"))
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(CON1-Pad1)"))
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 58806C2B)
    (at 29.464 -32.766 270)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference J13 (at -5.842 0) (layer F.SilkS))
    (fp_text value CONN1_1 (at 0.254 4.064 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.46 0) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (gr_text MLAB.CZ (at 67.056 -38.1) (layer B.Cu))
  (gr_text 2017 (at 66.294 -35.306) (layer B.Cu))
  (gr_text * (at 55.626 -34.798) (layer F.SilkS))
  (gr_text * (at 42.926 -34.798) (layer F.SilkS))
  (gr_text * (at 11.684 -13.462) (layer F.SilkS))
  (gr_text * (at 20.066 -11.938) (layer F.SilkS))
  (gr_text * (at 32.766 -11.938) (layer F.SilkS))
  (gr_text * (at 45.466 -11.938) (layer F.SilkS))
  (gr_text * (at 58.166 -11.938) (layer F.SilkS))
  (gr_text * (at 77.216 -10.414) (layer F.SilkS))
  (gr_text * (at 77.216 -21.336) (layer F.SilkS))
  (gr_text OUT (at 51.816 -27.94) (layer F.SilkS))
  (gr_text OUT (at 39.37 -27.94) (layer F.SilkS))
  (gr_text OUT (at 4.572 -18.034 90) (layer F.SilkS))
  (gr_text OUT (at 70.104 -25.654 90) (layer F.SilkS))
  (gr_text OUT (at 70.104 -14.732 90) (layer F.SilkS))
  (gr_text OUT (at 54.356 -12.954) (layer F.SilkS))
  (gr_text OUT (at 41.656 -12.954) (layer F.SilkS))
  (gr_text OUT (at 28.956 -12.954) (layer F.SilkS))
  (gr_text OUT (at 16.51 -12.954) (layer F.SilkS))
  (gr_text "POWER IN" (at 20.32 -32.004 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 46.482 -20.066) (layer F.SilkS))
  (gr_text 2017 (at 65.786 -35.306) (layer F.SilkS))
  (gr_text JACHO (at 65.786 -37.846) (layer F.SilkS))
  (gr_text UNIPOWER04A (at 46.482 -22.86) (layer F.SilkS))
  (gr_text - (at 29.464 -24.638) (layer F.SilkS))
  (gr_text + (at 24.384 -24.638) (layer F.SilkS))
  (gr_line (start 81.026 -0.254) (end 81.026 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 81.026 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 81.026 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17.272 -26.162) (xy 25.908 -26.162) (xy 25.908 -23.622) (xy 58.674 -23.622) (xy 59.436 -24.384)
        (xy 62.738 -24.384) (xy 62.738 -21.082) (xy 60.452 -21.082) (xy 59.69 -20.32) (xy 58.928 -19.558)
        (xy 18.542 -19.558) (xy 18.542 -21.59) (xy 17.272 -22.86)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.016 -41.91) (xy 83.566 -43.18) (xy 83.058 2.032) (xy -4.318 1.778)
      )
    )
  )
  (zone (net 11) (net_name "Net-(CON1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.192 -24.638) (xy 16.256 -24.638) (xy 16.256 -26.924) (xy 17.78 -28.448) (xy 26.416 -28.448)
        (xy 26.416 -37.338) (xy 21.082 -37.338) (xy 17.272 -33.528) (xy 17.272 -30.734) (xy 15.24 -28.702)
        (xy 12.192 -28.702) (xy 12.192 -28.448)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -8.89 -44.958) (xy 85.598 -45.466) (xy 84.836 5.08) (xy -11.176 2.794)
      )
    )
  )
)
