(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 79)
    (no_connects 0)
    (area 0.178999 -40.461001 50.621001 -0.178999)
    (thickness 1.6)
    (drawings 22)
    (tracks 479)
    (zones 0)
    (modules 47)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 1.5)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.500000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(C10-Pad1)")
  (net 4 "Net-(C11-Pad1)")
  (net 5 "Net-(C12-Pad1)")
  (net 6 "Net-(C13-Pad2)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 /EN)
  (net 9 /12V)
  (net 10 /5V)
  (net 11 /ADJ)
  (net 12 /Vout)
  (net 13 "Net-(C6-Pad1)")
  (net 14 "Net-(R3-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /12V)
    (add_net /5V)
    (add_net /ADJ)
    (add_net /EN)
    (add_net /Vout)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net VCC)
  )
  (module Mlab_IO:SOP-8_EP_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57FDF0F6)
    (at 30.988 -18.288 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.5 90) (layer B.SilkS))
    (fp_text value PAM2423 (at 0 -3.5 90) (layer B.SilkS))
    (pad 8 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 7 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 6 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C13-Pad2)"))
    (pad 5 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (pad 3 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 /EN))
    (pad 2 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0 0 90) (size 2.41 3.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_SOIC/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 25.4 -14.732 270)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value - (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /ADJ))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 20.32 -14.732 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 28k7 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 /5V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 22.86 -14.732 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 /12V))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 24.384 -23.368 180)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 84k5 (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C13-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R3-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 29.464 -11.176 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 8 /EN))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 24.384 -10.16 180)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 51k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 57FDF0F6)
    (at 43.18 -12.7 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P4 (at -5.842 0 270) (layer F.SilkS))
    (fp_text value WAGO256 (at 0.254 4.064 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 57FDF0F6)
    (at 43.18 -17.78 180)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P3 (at -5.842 0 270) (layer F.SilkS))
    (fp_text value WAGO256 (at 0.254 4.064 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 /Vout))
    (pad 1 thru_hole rect (at -2.46 0 270) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 /Vout))
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 57FDF0F6)
    (at 7.62 -12.7)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P2 (at -5.842 0 90) (layer F.SilkS))
    (fp_text value WAGO256 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Mlab_CON:WAGO256 (layer F.Cu) (tedit 57FDF0F6)
    (at 7.62 -17.78)
    (descr "WAGO-Series 236, 2Stift, 1pol, RM 5mm,")
    (tags "WAGO-Series 236, 2Stift, 1pol, RM 5mm, Anreibare Leiterplattenklemme")
    (fp_text reference P1 (at -5.842 0 90) (layer F.SilkS))
    (fp_text value WAGO256 (at 0.254 4.064) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 2.54 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 1 thru_hole rect (at -2.46 0 90) (size 3.81 3.81) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57FDF0F6)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57FDF0F6)
    (at 45.72 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57FDF0F6)
    (at 5.08 -35.56)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 57FDF0F6)
    (at 45.72 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (clearance 1) (zone_connect 2))
  )
  (module Mlab_L:DE1205-10 (layer B.Cu) (tedit 57FDF0F6)
    (at 21.336 -33.02 180)
    (descr "L DE1207")
    (fp_text reference L1 (at 0 0 180) (layer B.SilkS))
    (fp_text value "DE1207-10, EPCOS  B82477G4682M" (at 0 -5.842 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at -5 0 180) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 5 0 180) (size 3 5.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Capacitors_SMD/c_elec_10x10_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 5.08 -23.876 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J12 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 5.08 -26.416 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J11 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 14.732 -4.064)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 32.512 -4.064 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J9 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C6-Pad1)"))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C6-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 35.052 -4.064 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J8 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C6-Pad1)"))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C6-Pad1)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 37.592 -4.064 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J7 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 25.4 -19.304 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J6 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /ADJ))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C13-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 20.32 -19.304 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J5 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /5V))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C13-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 22.86 -19.304 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J4 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 9 /12V))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C13-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 5.08 -28.956 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 17.272 -4.064)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /EN))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /EN))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 57FDF0F6)
    (at 29.972 -4.064 180)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J1 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 180) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 -1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 0 1.27 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:Diode-SMB_Standard (layer B.Cu) (tedit 57FDF0F6)
    (at 33.02 -27.94)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D3 (at 0 0) (layer B.SilkS))
    (fp_text value STPS340U (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (pad 2 smd rect (at -2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMB_Standard (layer B.Cu) (tedit 57FDF0F6)
    (at 33.02 -34.544)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer B.SilkS))
    (fp_text value STPS340U (at 0 -3.81) (layer B.SilkS) hide)
    (fp_text user A (at -3.2004 -1.95072) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.95072) (layer B.SilkS))
    (pad 1 smd rect (at 2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (pad 2 smd rect (at -2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMA_Standard (layer B.Cu) (tedit 57FDF0F6)
    (at 11.176 -26.924 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0 270) (layer B.SilkS))
    (fp_text value M4 (at 0 -3.81 270) (layer B.SilkS) hide)
    (fp_text user A (at -3.29946 -1.6002 270) (layer B.SilkS))
    (fp_text user K (at 2.99974 -1.69926 270) (layer B.SilkS))
    (pad 1 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Diodes/SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 19.304 -24.384 90)
    (attr smd)
    (fp_text reference C15 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 470pF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C13-Pad2)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 37.1475 -21.844 180)
    (attr smd)
    (fp_text reference C14 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF/25V (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 21.844 -24.384 270)
    (attr smd)
    (fp_text reference C13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C13-Pad2)"))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 27.94 -24.384 180)
    (attr smd)
    (fp_text reference C12 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 25.908 -7.112 270)
    (attr smd)
    (fp_text reference C11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 47pF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 23.368 -7.112 270)
    (attr smd)
    (fp_text reference C10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 2.2nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 33.02 -11.176)
    (attr smd)
    (fp_text reference C9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF/25V (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 12.192 -32.004 180)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF/25V (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 12.192 -34.544 180)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 57FDF0F6)
    (at 15.748 -18.796 270)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer B.SilkS))
    (fp_text value 470uF/6V (at -0.09906 -3.59918 270) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908 270) (layer B.SilkS))
    (pad 1 smd rect (at -3.175 0 270) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 3.175 0 270) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 57FDF0F6)
    (at 45.212 -28.956)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C5 (at 0 0) (layer B.SilkS))
    (fp_text value 220uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908) (layer B.SilkS))
    (pad 1 smd rect (at -3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (pad 2 smd rect (at 3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_C:TantalC_SizeD_Reflow (layer B.Cu) (tedit 57FDF0F6)
    (at 45.212 -23.368)
    (descr "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (tags "Tantal Cap. , Size D, EIA-7343, Reflow,")
    (attr smd)
    (fp_text reference C7 (at 0 0) (layer B.SilkS))
    (fp_text value 220uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -5.6515 2.79908) (layer B.SilkS))
    (pad 1 smd rect (at -3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (pad 2 smd rect (at 3.175 0) (size 2.55016 2.70002) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model MLAB_3D/Capacitors/c_tant_D.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 37.084 -8.636)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C6-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 36.068 -11.684 270)
    (attr smd)
    (fp_text reference L2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value BLM21PG300SN1 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_C:C_Radial_D10_L13_P5 (layer F.Cu) (tedit 57FDF0F6)
    (at 40.466 -26.162)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 13mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C21 (at 0.508 -3.048) (layer F.SilkS))
    (fp_text value 470uF/35V (at 2.5 6.3) (layer F.Fab))
    (fp_text user + (at 0 -1.6891) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5 0) (size 4 4) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 /Vout))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L13_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 57FDF0F6)
    (at 24.384 -25.4)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 499R (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R3-Pad1)"))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /Vout))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text MLAB.cz (at 17.4752 -8.6868) (layer B.Cu))
  (gr_text "MAX 5.5V" (at 9.144 -26.416 270) (layer F.SilkS))
  (gr_text "POWER IN" (at 11.176 -26.416 270) (layer F.SilkS))
  (gr_text GND (at 12.192 -4.064 90) (layer F.SilkS))
  (gr_text EN (at 19.812 -4.064 90) (layer F.SilkS))
  (gr_text - (at 15.748 -12.192) (layer F.SilkS))
  (gr_text - (at 31.496 -12.7) (layer F.SilkS))
  (gr_text + (at 15.748 -17.78) (layer F.SilkS))
  (gr_text + (at 31.496 -17.78) (layer F.SilkS))
  (gr_text "POWER OUT" (at 34.036 -8.128) (layer F.SilkS))
  (gr_text ADJ (at 25.4 -16.256 270) (layer F.SilkS))
  (gr_text 12V (at 22.86 -16.256 270) (layer F.SilkS))
  (gr_text 5V (at 20.32 -16.256 270) (layer F.SilkS))
  (gr_text "SET OUTPUT" (at 22.86 -23.368) (layer F.SilkS))
  (gr_text JACHO (at 40.64 -5.08 90) (layer F.SilkS))
  (gr_text 2016 (at 40.132 -36.068 90) (layer F.SilkS))
  (gr_text MLAB.CZ (at 24.892 -35.052) (layer F.SilkS))
  (gr_text UPCONV01A (at 24.892 -32.512) (layer F.SilkS))
  (gr_line (start 0.254 -0.254) (end 0.254 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.546 -0.254) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.546 -40.386) (end 50.546 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 50.546 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 3.048 -15.748) (xy 12.192 -15.748) (xy 16.256 -19.812) (xy 17.272 -19.812) (xy 17.272 -23.368)
        (xy 17.272 -29.464) (xy 17.78 -29.972) (xy 17.78 -36.068) (xy 12.7 -36.068) (xy 12.7 -27.432)
        (xy 12.7 -26.924) (xy 12.192 -26.416) (xy 10.16 -26.416) (xy 9.144 -26.416) (xy 8.128 -27.432)
        (xy 3.048 -27.432) (xy 3.048 -25.4) (xy 7.112 -25.4) (xy 8.128 -25.4) (xy 8.128 -22.352)
        (xy 8.128 -21.336) (xy 8.128 -20.828) (xy 3.048 -20.828)
      )
    )
  )
  (zone (net 12) (net_name /Vout) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.528 -36.068) (xy 37.084 -36.068) (xy 37.592 -36.068) (xy 43.688 -30.48) (xy 43.688 -23.876)
        (xy 43.688 -22.352) (xy 47.752 -20.32) (xy 47.752 -15.748) (xy 38.1 -15.748) (xy 38.1 -19.812)
        (xy 38.1 -24.892) (xy 33.528 -24.892)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D2-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.512 -19.812) (xy 33.528 -19.812) (xy 33.528 -23.368) (xy 32.512 -24.384) (xy 32.512 -36.068)
        (xy 24.384 -36.068) (xy 24.384 -29.972) (xy 27.432 -26.416) (xy 28.956 -26.416) (xy 30.48 -24.892)
        (xy 32.512 -22.86)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 0 -40.64) (xy 50.8 -40.64) (xy 50.8 0) (xy 0 0)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -5.588 -45.72) (xy 53.34 -45.212) (xy 53.34 2.032) (xy -2.54 3.048)
      )
    )
  )
)
