(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 132)
    (no_connects 0)
    (area 0.203999 -50.596001 40.436001 -0.203999)
    (thickness 1.6)
    (drawings 44)
    (tracks 420)
    (zones 0)
    (modules 55)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.89)
    (via_drill 0.5)
    (via_min_size 0.7)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /VDD1)
  (net 4 /VDD2)
  (net 5 /VddB)
  (net 6 /VddA)
  (net 7 "Net-(J2-Pad12)")
  (net 8 /READY)
  (net 9 "Net-(J2-Pad10)")
  (net 10 /PIDENT)
  (net 11 /INT+)
  (net 12 /INT-)
  (net 13 /SCL-)
  (net 14 /SCL+)
  (net 15 /SDA+)
  (net 16 /SDA-)
  (net 17 "Net-(J14-Pad2)")
  (net 18 SDA)
  (net 19 SCL)
  (net 20 /EN)
  (net 21 VDD)
  (net 22 "Net-(C8-Pad1)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /EN)
    (add_net /PIDENT)
    (add_net /READY)
    (add_net /VDD1)
    (add_net /VDD2)
    (add_net /VddA)
    (add_net /VddB)
    (add_net GND)
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J14-Pad2)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
    (add_net VDD)
  )
  (net_class dif ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /INT+)
    (add_net /INT-)
    (add_net /SCL+)
    (add_net /SCL-)
    (add_net /SDA+)
    (add_net /SDA-)
  )
  (module "Mlab_CON:RJHSE-5384(RJ45)" (layer F.Cu) (tedit 56B1E39D)
    (at 13.97 -5.842)
    (fp_text reference J2 (at 4.445 -9.271) (layer F.SilkS))
    (fp_text value RJ45_RJHSE-5384 (at 6.4516 4.1275) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 12.7 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 14.48 -3.43) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at -1.78 -3.43) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C8-Pad1)"))
    (pad 7 thru_hole circle (at 3.81 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 12 /INT-))
    (pad 5 thru_hole circle (at 5.84 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.87 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL-))
    (pad 1 thru_hole circle (at 9.9 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA-))
    (pad 8 thru_hole circle (at 2.79 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 11 /INT+))
    (pad 6 thru_hole circle (at 4.82 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCL+))
    (pad 4 thru_hole circle (at 6.85 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 8.88 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SDA+))
    (pad 9 thru_hole circle (at 13.21 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 10 /PIDENT))
    (pad 10 thru_hole circle (at 10.92 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 1.78 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 8 /READY))
    (pad 12 thru_hole circle (at -0.51 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J2-Pad12)"))
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 56B0BB66)
    (at 36.83 -13.716)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 30.861 -24.384 270)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 10uF/16V (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 21 VDD))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 31.877 -36.322 90)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /VDD1))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 24.892 -34.925 180)
    (attr smd)
    (fp_text reference C3 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /VDD1))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 28.702 -42.037 90)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 4 /VDD2))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 2.794 -24.13 180)
    (attr smd)
    (fp_text reference C6 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /VddA))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 14.224 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /INT+))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /INT+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 16.764 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /INT-))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /INT-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 19.304 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCL+))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCL+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 21.844 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL-))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCL-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 24.384 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SDA+))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 15 /SDA+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 26.924 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA-))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 568CEB4A)
    (at 36.449 -37.719)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J10 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VDD1))
    (pad 4 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VDD1))
    (pad 5 thru_hole rect (at -1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 28.702 -37.719 270)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54 270) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VDD2))
    (pad 2 thru_hole rect (at 1.27 0 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VDD1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 568CEB15)
    (at 14.986 -39.624)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J12 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 0 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VDD1))
    (pad 2 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /VddB))
    (pad 1 thru_hole rect (at 0 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VDD2))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x03 (layer F.Cu) (tedit 569E5521)
    (at 23.368 -46.863 90)
    (descr "pin header straight 2x03")
    (tags "pin header straight 2x03")
    (fp_text reference J13 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value JUMP_3X2 (at 0 5.08 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VDD2))
    (pad 4 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VDD2))
    (pad 5 thru_hole rect (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole rect (at 1.27 2.54 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 5.0165 -37.9095)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J14 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J14-Pad2)"))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 5.0165 -40.4495 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J16 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value EN (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /EN))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 20 /EN))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 4.953 -21.209 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J19 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 4.953 -13.589 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J20 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 SDA))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 18 SDA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 4.953 -16.129 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J21 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /VddA))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /VddA))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 4.953 -18.669 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J22 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 SCL))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 19 SCL))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 4.953 -11.049 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J23 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -45.72)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -45.72)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 25.781 -12.573)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad10)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 13.716 -12.827 180)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J2-Pad12)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.9578 -32.004 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 620 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /INT+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.9451 -28.4607 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 120 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 /INT+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /INT-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 17.9705 -25.146 270)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 620 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /INT-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 23.2664 -31.7754 270)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 620 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /SCL+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 23.2664 -28.3464 270)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 120 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 /SCL+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /SCL-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 23.2664 -24.6126 270)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 620 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /SCL-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 28.702 -31.6484 270)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 620 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /SDA+))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 28.702 -28.2194 270)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 120 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 /SDA+))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA-))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 28.702 -24.4856 270)
    (attr smd)
    (fp_text reference R11 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 620 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA-))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.541 -32.9565)
    (attr smd)
    (fp_text reference R12 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J14-Pad2)"))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /VddA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.87552 -17.94002 90)
    (attr smd)
    (fp_text reference R14 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /VddA))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 SCL))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SOT-223 (layer B.Cu) (tedit 56A0F3AE)
    (at 35.433 -29.083 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 0.762 180) (layer B.SilkS))
    (fp_text value "LM1117 5V" (at 0.3175 -0.0635 180) (layer B.SilkS) hide)
    (pad 4 smd rect (at 0 3.302 180) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 /VDD1))
    (pad 2 smd rect (at 0 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 /VDD1))
    (pad 3 smd rect (at 2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 21 VDD))
    (pad 1 smd rect (at -2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SOT-223 (layer B.Cu) (tedit 0)
    (at 22.352 -39.751 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0.762 270) (layer B.SilkS))
    (fp_text value "LM1117 3V3" (at 0 -0.762 270) (layer B.Fab))
    (pad 4 smd rect (at 0 3.302 270) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask)
      (net 4 /VDD2))
    (pad 2 smd rect (at 0 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 4 /VDD2))
    (pad 3 smd rect (at 2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 /VDD1))
    (pad 1 smd rect (at -2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 54130A77)
    (at 6.7564 -28.194)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 3.55) (layer B.SilkS))
    (fp_text value PCA9616 (at 0 -3.55) (layer B.Fab))
    (pad 1 smd rect (at -2.95 2.275) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 /VddA))
    (pad 2 smd rect (at -2.95 1.625) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 18 SDA))
    (pad 3 smd rect (at -2.95 0.975) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 20 /EN))
    (pad 4 smd rect (at -2.95 0.325) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 19 SCL))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 /PIDENT))
    (pad 6 smd rect (at -2.95 -0.975) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /READY))
    (pad 7 smd rect (at -2.95 -1.625) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -2.95 -2.275) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.95 -2.275) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J14-Pad2)"))
    (pad 10 smd rect (at 2.95 -1.625) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 /INT+))
    (pad 11 smd rect (at 2.95 -0.975) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 /INT-))
    (pad 12 smd rect (at 2.95 -0.325) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 13 /SCL-))
    (pad 13 smd rect (at 2.95 0.325) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 14 /SCL+))
    (pad 14 smd rect (at 2.95 0.975) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 15 /SDA+))
    (pad 15 smd rect (at 2.95 1.625) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA-))
    (pad 16 smd rect (at 2.95 2.275) (size 1.5 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 35.56 -19.939)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C7 (at 0.0127 -0.0381) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 VDD))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.652 -23.368 270)
    (attr smd)
    (fp_text reference C5 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /VddB))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_IO:SOT-553 (layer B.Cu) (tedit 568CF2D9)
    (at 12.827 -23.368 90)
    (descr SOT553)
    (attr smd)
    (fp_text reference D2 (at 0.0635 0 90) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.70104 0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -0.70104 -0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0.70104 0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 15 /SDA+))
    (pad 2 smd rect (at -0.70104 0 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.70104 -0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDA-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module MLAB_IO:SOT-553 (layer B.Cu) (tedit 568CF2D4)
    (at 14.224 -30.099 270)
    (descr SOT553)
    (attr smd)
    (fp_text reference D3 (at 0.0635 0.0635 270) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.70104 0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 11 /INT+))
    (pad 3 smd rect (at -0.70104 -0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 12 /INT-))
    (pad 5 smd rect (at 0.70104 0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 13 /SCL-))
    (pad 2 smd rect (at -0.70104 0 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.70104 -0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 14 /SCL+))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x03 (layer F.Cu) (tedit 568CEB10)
    (at 12.446 -39.624)
    (descr "pin header straight 1x03")
    (tags "pin header straight 1x03")
    (fp_text reference J15 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value CONN_3 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -2.54) (layer F.SilkS) hide)
    (pad 3 thru_hole rect (at 0 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /VDD1))
    (pad 2 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /VddA))
    (pad 1 thru_hole rect (at 0 -2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /VDD2))
    (model Pin_Headers/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 34.4805 -23.1775)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J17 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 21 VDD))
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.8425 -14.5415 270)
    (attr smd)
    (fp_text reference R13 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 4k7 (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 6 /VddA))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 SDA))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 5.0165 -35.3695 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /READY))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /READY))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.398 -9.271 180)
    (attr smd)
    (fp_text reference C8 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.398 -10.9855)
    (attr smd)
    (fp_text reference R15 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_D:Diode-SMC_Standard (layer B.Cu) (tedit 54799AAC)
    (at 31.75 -13.1445 90)
    (descr "Diode SMC Standard")
    (tags "Diode SMC Standard")
    (attr smd)
    (fp_text reference D1 (at 0 5.08 90) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0 -5.08 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -3.40106 0) (size 3.29946 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.40106 0) (size 3.29946 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 21 VDD))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SCL- (at 21.7805 -22.4155 90) (layer F.SilkS))
  (gr_text SCL+ (at 19.304 -22.4155 90) (layer F.SilkS))
  (gr_text 3V3 (at 3.81 -27.1145) (layer F.SilkS))
  (gr_text READY (at 4.826 -32.9565) (layer F.SilkS))
  (gr_text EXT (at 33.2105 -13.716 90) (layer F.SilkS))
  (gr_text 2016 (at 20.32 -5.842) (layer F.SilkS))
  (gr_text MLAB.CZ (at 13.0175 -48.006) (layer B.Cu))
  (gr_text JACHO (at 20.066 -12.7) (layer F.SilkS))
  (gr_text 5V (at 9.652 -25.146) (layer F.SilkS))
  (gr_text 3V3 (at 9.652 -27.178) (layer F.SilkS))
  (gr_text 1V8 (at 9.525 -29.21) (layer F.SilkS))
  (gr_text 5V (at 3.81 -25.146) (layer F.SilkS))
  (gr_text 1V8 (at 3.81 -29.083) (layer F.SilkS))
  (gr_text VDD1 (at 3.683 -30.988) (layer F.SilkS))
  (gr_text VDD2 (at 9.398 -30.988) (layer F.SilkS))
  (gr_text MLAB.CZ (at 30.099 -29.21 90) (layer F.SilkS))
  (gr_text I2CDIFF01A (at 20.5105 -30.734) (layer F.SilkS))
  (gr_text VDD2 (at 27.178 -36.449) (layer F.SilkS))
  (gr_text VDD1 (at 27.178 -38.989) (layer F.SilkS))
  (gr_text VDD (at 35.814 -25.4 90) (layer F.SilkS))
  (gr_text EXT (at 33.274 -25.4 90) (layer F.SilkS))
  (gr_text SDA (at 7.62 -13.589) (layer F.SilkS))
  (gr_text VDDA (at 7.62 -16.129) (layer F.SilkS))
  (gr_text SCL (at 7.62 -18.669) (layer F.SilkS))
  (gr_text I2C (at 1.397 -16.002 90) (layer F.SilkS))
  (gr_text SDA- (at 26.924 -22.352 90) (layer F.SilkS))
  (gr_text SDA+ (at 24.384 -22.352 90) (layer F.SilkS))
  (gr_text INT- (at 16.764 -22.352 90) (layer F.SilkS))
  (gr_text INT+ (at 14.224 -22.352 90) (layer F.SilkS))
  (gr_text OUT (at 36.322 -32.258) (layer F.SilkS))
  (gr_text OUT (at 18.288 -46.99 90) (layer F.SilkS))
  (gr_text POWER (at 30.988 -13.716 90) (layer F.SilkS))
  (gr_text VDD1 (at 32.385 -37.719 90) (layer F.SilkS))
  (gr_text VDD2 (at 23.368 -42.926) (layer F.SilkS))
  (gr_text VDDB (at 17.78 -39.751 90) (layer F.SilkS))
  (gr_text VDDA (at 9.779 -39.37 90) (layer F.SilkS))
  (gr_text VDD2 (at 13.716 -44.831) (layer F.SilkS))
  (gr_text VDD1 (at 13.716 -34.417) (layer F.SilkS))
  (gr_text SEL (at 1.397 -37.9095 90) (layer F.SilkS))
  (gr_text EN (at 1.4605 -42.3545 90) (layer F.SilkS))
  (gr_line (start 0.254 -50.546) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -50.546) (end 0.254 -50.546) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -0.254) (end 40.386 -50.546) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.91 -51.7525) (xy 41.529 0.8255) (xy -2.7305 2.794) (xy -1.4605 -51.6255)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.2385 -53.467) (xy 44.577 -53.213) (xy 43.18 3.2385) (xy -4.6355 4.953)
      )
    )
  )
)
