(kicad_pcb (version 20160815) (host pcbnew 201609191018+7178~55~ubuntu16.04.1-)
  (general
    (links 106)
    (no_connects 15)
    (area 39.116 109.982 95.504001 166.116001)
    (thickness 1.6)
    (drawings 4)
    (tracks 272)
    (zones 0)
    (modules 41)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFCF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C8-Pad1)")
  (net 4 /MISO+)
  (net 5 /MISO-)
  (net 6 /MOSI-)
  (net 7 /MOSI+)
  (net 8 /CS+)
  (net 9 /CS-)
  (net 10 /SCLK-)
  (net 11 /SCLK+)
  (net 12 "Net-(J2-Pad10)")
  (net 13 /SLAVE_K)
  (net 14 "Net-(J2-Pad12)")
  (net 15 /MASTER_A)
  (net 16 /MISO)
  (net 17 /MOSI)
  (net 18 /CS)
  (net 19 /SCLK)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2)
    (add_net /CS)
    (add_net /CS+)
    (add_net /CS-)
    (add_net /MASTER_A)
    (add_net /MISO)
    (add_net /MISO+)
    (add_net /MISO-)
    (add_net /MOSI)
    (add_net /MOSI+)
    (add_net /MOSI-)
    (add_net /SCLK)
    (add_net /SCLK+)
    (add_net /SCLK-)
    (add_net /SLAVE_K)
    (add_net GND)
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net VDD)
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 81.28 136.144 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 10uF/16V (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 58.42 133.35 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 74.422 133.35 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 50.165 129.667 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 66.802 133.604 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 54.102 150.876 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMB_Standard (layer B.Cu) (tedit 57E1216F)
    (at 81.28 140.208)
    (descr "Diode SMB Standard")
    (tags "Diode SMB Standard")
    (attr smd)
    (fp_text reference D1 (at 0.05 3.1) (layer B.SilkS))
    (fp_text value SMBJ15A-E3/52 (at 0.05 -4.7) (layer B.Fab))
    (fp_text user K (at -3.25 -3.3) (layer B.SilkS))
    (fp_text user A (at 3 -3.2) (layer B.SilkS))
    (pad 2 smd rect (at 2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -2.14884 0) (size 2.49936 2.30124) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SMB_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-553 (layer B.Cu) (tedit 57E1216F)
    (at 61.214 136.144)
    (descr SOT553)
    (attr smd)
    (fp_text reference D2 (at 0 1.19888) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874) (layer B.Fab))
    (pad 4 smd rect (at 0.70104 -0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 9 /CS-))
    (pad 2 smd rect (at -0.70104 0) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.70104 0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 8 /CS+))
    (pad 3 smd rect (at -0.70104 -0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 4 /MISO+))
    (pad 1 smd rect (at -0.70104 0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 5 /MISO-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-553 (layer B.Cu) (tedit 57E1216F)
    (at 72.39 136.144)
    (descr SOT553)
    (attr smd)
    (fp_text reference D3 (at 0 1.19888) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874) (layer B.Fab))
    (pad 4 smd rect (at 0.70104 -0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCLK-))
    (pad 2 smd rect (at -0.70104 0) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.70104 0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCLK+))
    (pad 3 smd rect (at -0.70104 -0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 7 /MOSI+))
    (pad 1 smd rect (at -0.70104 0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 6 /MOSI-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 67.31 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MOSI+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MOSI+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Connect:RJHSE-5384(RJ45)" (layer F.Cu) (tedit 57E1216F)
    (at 59.69 155.575)
    (fp_text reference J2 (at 4.445 -9.271) (layer F.SilkS))
    (fp_text value RJ45_RJHSE-5384 (at 6.4516 4.1275) (layer F.Fab) hide)
    (pad 12 thru_hole circle (at -0.51 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad12)"))
    (pad 11 thru_hole circle (at 1.78 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SLAVE_K))
    (pad 10 thru_hole circle (at 10.92 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J2-Pad10)"))
    (pad 9 thru_hole circle (at 13.21 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 8.88 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCLK+))
    (pad 4 thru_hole circle (at 6.85 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MOSI-))
    (pad 6 thru_hole circle (at 4.82 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 8 /CS+))
    (pad 8 thru_hole circle (at 2.79 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 4 /MISO+))
    (pad 1 thru_hole circle (at 9.9 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCLK-))
    (pad 3 thru_hole circle (at 7.87 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 9 /CS-))
    (pad 5 thru_hole circle (at 5.84 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MOSI+))
    (pad 7 thru_hole circle (at 3.81 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MISO-))
    (pad 13 thru_hole circle (at -1.78 -3.43) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C8-Pad1)"))
    (pad 14 thru_hole circle (at 14.48 -3.43) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 12.7 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 69.85 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MOSI-))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MOSI-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 57.15 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /MISO+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /MISO+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 59.69 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J5 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MISO-))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MISO-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 62.23 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J6 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /CS+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /CS+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 64.77 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J7 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /CS-))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /CS-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 72.39 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J8 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCLK+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCLK+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 57E1216F)
    (at 74.93 140.208 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J9 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCLK-))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCLK-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 57E1216F)
    (at 80.01 145.796)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J10 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JUMP_3X2 (at 0 -3.1) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57E1216F)
    (at 51.435 142.748 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J11 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value Slave/Master (at 0 -3.1 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /SLAVE_K))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57E1216F)
    (at 48.895 142.748 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J12 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value Slave/Master (at 0 -3.1 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /MASTER_A))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57E1216F)
    (at 60.452 116.332)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J19 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /MISO))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /MISO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57E1216F)
    (at 62.992 116.332)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J20 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MOSI))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MOSI))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57E1216F)
    (at 68.072 116.332)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J21 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /CS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /CS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57E1216F)
    (at 65.532 116.332)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J22 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SCLK))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SCLK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57E1216F)
    (at 70.612 116.332)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J23 (at 0 -5.1) (layer F.SilkS))
    (fp_text value JUMP_2x1 (at 0 -3.1) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 57E1216F)
    (at 50.8 157.48)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference M1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value HOLE (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 57E1216F)
    (at 81.28 157.48)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference M2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value HOLE (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 57E1216F)
    (at 50.8 116.84)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference M3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value HOLE (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 57E1216F)
    (at 81.28 116.84)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference M4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value HOLE (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 76.454 148.844 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 90) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J2-Pad10)"))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /MASTER_A))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 54.102 145.796)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 54.864 133.35 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 120 (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /MISO-))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /MISO+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 61.468 133.35 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 120 (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /CS-))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /CS+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 77.978 133.35 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 120 (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCLK-))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCLK+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 70.866 133.35 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 120 (at 0 -2.1 180) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 /MOSI-))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /MOSI+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 57E1216F)
    (at 54.102 148.336)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C8-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57E1216F)
    (at 61.468 127.762 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value SN65176 (at 0 -3.5 270) (layer B.Fab))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 /CS-))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 /CS+))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 /CS))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SLAVE_K))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SLAVE_K))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 /CS))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57E1216F)
    (at 54.61 127.762 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value SN65176 (at 0 -3.5 270) (layer B.Fab))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /MISO-))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 /MISO+))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 /MISO))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 /MASTER_A))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 /MASTER_A))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 /MISO))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57E1216F)
    (at 77.978 128.016 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value SN65176 (at 0 -3.5 270) (layer B.Fab))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCLK-))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCLK+))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /SCLK))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SLAVE_K))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SLAVE_K))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 /SCLK))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 57E1216F)
    (at 70.866 128.016 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value SN65176 (at 0 -3.5 270) (layer B.Fab))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /MOSI-))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 /MOSI+))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 /MOSI))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SLAVE_K))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /SLAVE_K))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 /MOSI))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 45.974 162.306) (end 45.974 112.014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.106 112.014) (end 45.974 112.014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.106 162.306) (end 86.106 112.014) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.974 162.306) (end 86.106 162.306) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.37 109.982) (xy 39.116 162.814) (xy 94.234 165.862) (xy 95.504 109.982)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39.37 109.982) (xy 39.116 163.576) (xy 94.488 166.116) (xy 95.25 110.236)
      )
    )
  )
  (zone (net 15) (net_name /MASTER_A) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.467 127) (xy 55.88 127) (xy 55.88 124.206) (xy 53.467 124.206)
      )
    )
  )
  (zone (net 15) (net_name /MASTER_A) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.325 124.206) (xy 60.325 127.762) (xy 62.611 127.762) (xy 62.611 124.206)
      )
    )
  )
  (zone (net 13) (net_name /SLAVE_K) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.80809 127.762) (xy 71.96709 127.762) (xy 71.96709 124.46) (xy 69.80809 124.46)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.169 132.969) (xy 82.169 141.478) (xy 84.836 141.478) (xy 84.836 139.065) (xy 84.836 134.874)
      )
    )
  )
)
