(kicad_pcb (version 3) (host pcbnew "(2014-jan-25)-product")
  (general
    (links 262)
    (no_connects 0)
    (area 153.376019 59.899953 216.964134 139.150001)
    (thickness 1.6)
    (drawings 18)
    (tracks 1349)
    (zones 0)
    (modules 31)
    (nets 88)
  )
  (page A4)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.4)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed yes)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 190.5 130.4)
    (grid_origin 190.5 130.4)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 283148289)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 3V3)
  (net 3 CLK0_M2C_N)
  (net 4 CLK0_M2C_P)
  (net 5 CLK1_M2C_N)
  (net 6 CLK1_M2C_P)
  (net 7 DGND)
  (net 8 LA00_N_CC)
  (net 9 LA00_P_CC)
  (net 10 LA01_N_CC)
  (net 11 LA01_P_CC)
  (net 12 LA02_N)
  (net 13 LA02_P)
  (net 14 LA03_N)
  (net 15 LA03_P)
  (net 16 LA04_N)
  (net 17 LA04_P)
  (net 18 LA06_N)
  (net 19 LA06_P)
  (net 20 LA07_N)
  (net 21 LA07_P)
  (net 22 LA08_N)
  (net 23 LA08_P)
  (net 24 LA09_N)
  (net 25 LA09_P)
  (net 26 LA10_N)
  (net 27 LA10_P)
  (net 28 LA11_N)
  (net 29 LA11_P)
  (net 30 LA12_N)
  (net 31 LA12_P)
  (net 32 LA13_N)
  (net 33 LA13_P)
  (net 34 LA15_N)
  (net 35 LA15_P)
  (net 36 LA16_N)
  (net 37 LA16_P)
  (net 38 LA17_N_CC)
  (net 39 LA17_P_CC)
  (net 40 LA19_N)
  (net 41 LA19_P)
  (net 42 LA20_N)
  (net 43 LA20_P)
  (net 44 LA21_N)
  (net 45 LA21_P)
  (net 46 LA22_N)
  (net 47 LA22_P)
  (net 48 LA23_P)
  (net 49 LA24_N)
  (net 50 LA24_P)
  (net 51 LA25_N)
  (net 52 LA25_P)
  (net 53 LA26_N)
  (net 54 LA26_P)
  (net 55 LA28_N)
  (net 56 LA28_P)
  (net 57 LA29_N)
  (net 58 LA29_P)
  (net 59 LA30_N)
  (net 60 LA30_P)
  (net 61 LA31_N)
  (net 62 LA31_P)
  (net 63 LA32_N)
  (net 64 LA32_P)
  (net 65 LA33_N)
  (net 66 LA33_P)
  (net 67 SCL)
  (net 68 SDA)
  (net 69 VDD)
  (net 70 LA23_N)
  (net 71 "Net-(J2-Pad2)")
  (net 72 "Net-(J2-Pad3)")
  (net 73 "Net-(J2-Pad5)")
  (net 74 "Net-(J2-Pad6)")
  (net 75 "Net-(J3-Pad2)")
  (net 76 "Net-(J3-Pad3)")
  (net 77 "Net-(J3-Pad5)")
  (net 78 "Net-(J3-Pad6)")
  (net 79 TRST_L)
  (net 80 LA27_P)
  (net 81 LA27_N)
  (net 82 LA18_P_CC)
  (net 83 LA18_N_CC)
  (net 84 LA05_P)
  (net 85 LA05_N)
  (net 86 LA14_P)
  (net 87 LA14_N)
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +12V)
    (add_net CLK0_M2C_N)
    (add_net CLK0_M2C_P)
    (add_net CLK1_M2C_N)
    (add_net CLK1_M2C_P)
    (add_net DGND)
    (add_net LA00_N_CC)
    (add_net LA00_P_CC)
    (add_net LA01_N_CC)
    (add_net LA01_P_CC)
    (add_net LA02_N)
    (add_net LA02_P)
    (add_net LA03_N)
    (add_net LA03_P)
    (add_net LA04_N)
    (add_net LA04_P)
    (add_net LA05_N)
    (add_net LA05_P)
    (add_net LA06_N)
    (add_net LA06_P)
    (add_net LA07_N)
    (add_net LA07_P)
    (add_net LA08_N)
    (add_net LA08_P)
    (add_net LA09_N)
    (add_net LA09_P)
    (add_net LA10_N)
    (add_net LA10_P)
    (add_net LA11_N)
    (add_net LA11_P)
    (add_net LA12_N)
    (add_net LA12_P)
    (add_net LA13_N)
    (add_net LA13_P)
    (add_net LA14_N)
    (add_net LA14_P)
    (add_net LA15_N)
    (add_net LA15_P)
    (add_net LA16_N)
    (add_net LA16_P)
    (add_net LA17_N_CC)
    (add_net LA17_P_CC)
    (add_net LA18_N_CC)
    (add_net LA18_P_CC)
    (add_net LA19_N)
    (add_net LA19_P)
    (add_net LA20_N)
    (add_net LA20_P)
    (add_net LA21_N)
    (add_net LA21_P)
    (add_net LA22_N)
    (add_net LA22_P)
    (add_net LA23_N)
    (add_net LA23_P)
    (add_net LA24_N)
    (add_net LA24_P)
    (add_net LA25_N)
    (add_net LA25_P)
    (add_net LA26_N)
    (add_net LA26_P)
    (add_net LA27_N)
    (add_net LA27_P)
    (add_net LA28_N)
    (add_net LA28_P)
    (add_net LA29_N)
    (add_net LA29_P)
    (add_net LA30_N)
    (add_net LA30_P)
    (add_net LA31_N)
    (add_net LA31_P)
    (add_net LA32_N)
    (add_net LA32_P)
    (add_net LA33_N)
    (add_net LA33_P)
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net SCL)
    (add_net SDA)
    (add_net TRST_L)
    (add_net VDD)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net 3V3)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 164.4904 126.5646)
    (fp_text reference G*** (at 0 6.62432) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -6.62432) (layer F.SilkS) hide)
  )
  (module Kaklik_konektory:SAS_mini_1888174 (layer F.Cu) (tedit 5328CBF6)
    (at 178 116.69 270)
    (descr "36pin mini SAS connector")
    (tags "SAS mini connector")
    (fp_text reference J6 (at -0.9712 -7.5216 270) (layer F.SilkS))
    (fp_text value SAS_mini_1888174 (at 0 0 270) (layer F.SilkS) hide)
    (pad B1 smd oval (at -7 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B2 smd oval (at -6.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 43 LA20_P))
    (pad B3 smd oval (at -5.4 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 42 LA20_N))
    (pad B4 smd oval (at -4.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B5 smd oval (at -3.8 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 47 LA22_P))
    (pad B6 smd oval (at -3 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 46 LA22_N))
    (pad B7 smd oval (at -2.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B8 smd oval (at -1.4 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 52 LA25_P))
    (pad B9 smd oval (at -0.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 51 LA25_N))
    (pad B10 smd oval (at 0.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 58 LA29_P))
    (pad B11 smd oval (at 1 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 57 LA29_N))
    (pad B12 smd oval (at 1.8 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B13 smd oval (at 2.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 62 LA31_P))
    (pad B14 smd oval (at 3.4 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 61 LA31_N))
    (pad B15 smd oval (at 4.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B16 smd oval (at 5 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 66 LA33_P))
    (pad B17 smd oval (at 5.8 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 65 LA33_N))
    (pad A1 smd oval (at -6.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A2 smd oval (at -5.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 41 LA19_P))
    (pad A3 smd oval (at -4.9 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 40 LA19_N))
    (pad A4 smd oval (at -4.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A5 smd oval (at -3.3 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 45 LA21_P))
    (pad A6 smd oval (at -2.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 44 LA21_N))
    (pad A7 smd oval (at -1.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A8 smd oval (at -0.9 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 50 LA24_P))
    (pad A9 smd oval (at -0.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 49 LA24_N))
    (pad A10 smd oval (at 0.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 56 LA28_P))
    (pad A11 smd oval (at 1.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 55 LA28_N))
    (pad A12 smd oval (at 2.3 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A13 smd oval (at 3.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 60 LA30_P))
    (pad A14 smd oval (at 3.9 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 59 LA30_N))
    (pad A15 smd oval (at 4.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A16 smd oval (at 5.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 64 LA32_P))
    (pad A17 smd oval (at 6.3 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 63 LA32_N))
    (pad 1 thru_hole circle (at -8.9 -5.24 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 2 thru_hole circle (at -8.9 -2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 4 thru_hole circle (at -8.9 4.03 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 3 thru_hole circle (at -8.9 2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 5 thru_hole circle (at 8.9 -6.24 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 6 thru_hole circle (at 8.9 -2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad "" np_thru_hole circle (at -8 0 270) (size 1.55 1.55) (drill 1.55) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 8 0 270) (size 1.55 1.55) (drill 1.55) (layers *.Mask B.Cu F.SilkS))
    (pad 8 thru_hole circle (at 8.9 4.03 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 7 thru_hole circle (at 8.9 2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad B18 smd oval (at 6.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A18 smd oval (at 7.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (model /home/kaklik/git/Connect.pretty/SAS_mini_1888174.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kaklik_konektory:FMC_LPC_ASP-134604-01 locked (layer B.Cu) (tedit 53245C3A)
    (at 192.5 99.2 90)
    (descr http://www.samtec.com/standards/vita.aspx)
    (tags "FMC LPC VITA ")
    (solder_mask_margin 0.05)
    (clearance 0.1)
    (attr smd)
    (fp_text reference J1 (at 29.32 1.65 180) (layer B.SilkS))
    (fp_text value "ASP-134604-01_(FMC)" (at -0.45 5.78 90) (layer B.SilkS) hide)
    (pad G40 thru_hole circle (at -31.19 -2 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 7 DGND) (clearance 0.1) (zone_connect 2))
    (pad C02 smd circle (at 23.495 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad "" np_thru_hole circle (at 27.19 0 90) (size 1.27 1.27) (drill 1.27) (layers *.Cu *.Mask B.SilkS)
      (clearance 0.1))
    (pad G01 smd circle (at 24.765 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G02 smd circle (at 23.495 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 6 CLK1_M2C_P) (clearance 0.1))
    (pad H01 smd circle (at 24.765 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad H02 smd circle (at 23.495 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad G07 smd circle (at 17.145 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 8 LA00_N_CC) (clearance 0.1))
    (pad H07 smd circle (at 17.145 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 13 LA02_P) (clearance 0.1))
    (pad H08 smd circle (at 15.875 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 12 LA02_N) (clearance 0.1))
    (pad G08 smd circle (at 15.875 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G10 smd circle (at 13.335 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 14 LA03_N) (clearance 0.1))
    (pad H10 smd circle (at 13.335 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 17 LA04_P) (clearance 0.1))
    (pad H09 smd circle (at 14.605 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G09 smd circle (at 14.605 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 15 LA03_P) (clearance 0.1))
    (pad G05 smd circle (at 19.685 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H05 smd circle (at 19.685 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 3 CLK0_M2C_N) (clearance 0.1))
    (pad H06 smd circle (at 18.415 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G06 smd circle (at 18.415 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 9 LA00_P_CC) (clearance 0.1))
    (pad G04 smd circle (at 20.955 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H04 smd circle (at 20.955 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 4 CLK0_M2C_P) (clearance 0.1))
    (pad H03 smd circle (at 22.225 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G03 smd circle (at 22.225 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 5 CLK1_M2C_N) (clearance 0.1))
    (pad G19 smd circle (at 1.905 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 36 LA16_N) (clearance 0.1))
    (pad H19 smd circle (at 1.905 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 35 LA15_P) (clearance 0.1))
    (pad H20 smd circle (at 0.635 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 34 LA15_N) (clearance 0.1))
    (pad G20 smd circle (at 0.635 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G21 smd circle (at -0.635 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 43 LA20_P) (clearance 0.1))
    (pad H21 smd circle (at -0.625 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G24 smd circle (at -4.445 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 47 LA22_P) (clearance 0.1))
    (pad H24 smd circle (at -4.445 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H25 smd circle (at -5.715 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 45 LA21_P) (clearance 0.1))
    (pad G25 smd circle (at -5.715 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 46 LA22_N) (clearance 0.1))
    (pad G23 smd circle (at -3.175 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H23 smd circle (at -3.175 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 40 LA19_N) (clearance 0.1))
    (pad H22 smd circle (at -1.905 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 41 LA19_P) (clearance 0.1))
    (pad G22 smd circle (at -1.905 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 42 LA20_N) (clearance 0.1))
    (pad G15 smd circle (at 6.985 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 31 LA12_P) (clearance 0.1))
    (pad H15 smd circle (at 6.985 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H16 smd circle (at 5.715 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 29 LA11_P) (clearance 0.1))
    (pad G16 smd circle (at 5.715 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 30 LA12_N) (clearance 0.1))
    (pad G18 smd circle (at 3.175 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 37 LA16_P) (clearance 0.1))
    (pad H18 smd circle (at 3.175 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H17 smd circle (at 4.445 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 28 LA11_N) (clearance 0.1))
    (pad G17 smd circle (at 4.445 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G13 smd circle (at 9.525 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 22 LA08_N) (clearance 0.1))
    (pad H13 smd circle (at 9.525 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 21 LA07_P) (clearance 0.1))
    (pad H14 smd circle (at 8.255 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 20 LA07_N) (clearance 0.1))
    (pad G14 smd circle (at 8.255 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G12 smd circle (at 10.795 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 23 LA08_P) (clearance 0.1))
    (pad H12 smd circle (at 10.795 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H11 smd circle (at 12.065 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 16 LA04_N) (clearance 0.1))
    (pad G11 smd circle (at 12.065 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G29 smd circle (at -10.795 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H29 smd circle (at -10.795 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 49 LA24_N) (clearance 0.1))
    (pad H30 smd circle (at -12.065 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G30 smd circle (at -12.065 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 58 LA29_P) (clearance 0.1))
    (pad G32 smd circle (at -14.605 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H32 smd circle (at -14.605 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 55 LA28_N) (clearance 0.1))
    (pad H31 smd circle (at -13.335 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 56 LA28_P) (clearance 0.1))
    (pad G31 smd circle (at -13.335 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 57 LA29_N) (clearance 0.1))
    (pad H28 smd circle (at -9.525 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 50 LA24_P) (clearance 0.1))
    (pad G28 smd circle (at -9.525 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 51 LA25_N) (clearance 0.1))
    (pad G27 smd circle (at -8.255 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 52 LA25_P) (clearance 0.1))
    (pad H27 smd circle (at -8.255 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H26 smd circle (at -6.985 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 44 LA21_N) (clearance 0.1))
    (pad G26 smd circle (at -6.985 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G35 smd circle (at -18.415 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H35 smd circle (at -18.415 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 59 LA30_N) (clearance 0.1))
    (pad H36 smd circle (at -19.685 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G36 smd circle (at -19.685 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 66 LA33_P) (clearance 0.1))
    (pad G37 smd circle (at -20.955 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 65 LA33_N) (clearance 0.1))
    (pad H37 smd circle (at -20.955 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 64 LA32_P) (clearance 0.1))
    (pad G40 smd circle (at -24.765 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H40 smd circle (at -24.765 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 69 VDD) (clearance 0.1))
    (pad G39 smd circle (at -23.495 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 69 VDD) (clearance 0.1))
    (pad H39 smd circle (at -23.495 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad H38 smd circle (at -22.225 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 63 LA32_N) (clearance 0.1))
    (pad G38 smd circle (at -22.225 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G34 smd circle (at -17.145 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 61 LA31_N) (clearance 0.1))
    (pad H34 smd circle (at -17.145 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 60 LA30_P) (clearance 0.1))
    (pad H33 smd circle (at -15.875 -3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad G33 smd circle (at -15.875 -1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 62 LA31_P) (clearance 0.1))
    (pad C33 smd circle (at -15.875 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D33 smd circle (at -15.875 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad D34 smd circle (at -17.145 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 79 TRST_L) (clearance 0.1))
    (pad C34 smd circle (at -17.145 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C38 smd circle (at -22.225 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D38 smd circle (at -22.225 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3) (clearance 0.1))
    (pad D39 smd circle (at -23.495 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C39 smd circle (at -23.495 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3) (clearance 0.1))
    (pad D40 smd circle (at -24.765 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3) (clearance 0.1))
    (pad C40 smd circle (at -24.765 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D37 smd circle (at -20.955 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C37 smd circle (at -20.955 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V) (clearance 0.1))
    (pad C36 smd circle (at -19.685 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D36 smd circle (at -19.685 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3) (clearance 0.1))
    (pad D35 smd circle (at -18.415 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C35 smd circle (at -18.415 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V) (clearance 0.1))
    (pad C26 smd circle (at -6.985 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 80 LA27_P) (clearance 0.1))
    (pad D26 smd circle (at -6.985 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 54 LA26_P) (clearance 0.1))
    (pad D27 smd circle (at -8.255 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 53 LA26_N) (clearance 0.1))
    (pad C27 smd circle (at -8.255 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 81 LA27_N) (clearance 0.1))
    (pad C28 smd circle (at -9.525 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D28 smd circle (at -9.525 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C31 smd circle (at -13.335 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 68 SDA) (clearance 0.1))
    (pad D31 smd circle (at -13.335 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad D32 smd circle (at -14.605 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C32 smd circle (at -14.605 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C30 smd circle (at -12.065 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 67 SCL) (clearance 0.1))
    (pad D30 smd circle (at -12.065 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad D29 smd circle (at -10.795 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C29 smd circle (at -10.795 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C11 smd circle (at 12.065 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 18 LA06_N) (clearance 0.1))
    (pad D11 smd circle (at 12.065 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 84 LA05_P) (clearance 0.1))
    (pad D12 smd circle (at 10.795 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 85 LA05_N) (clearance 0.1))
    (pad C12 smd circle (at 10.795 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C14 smd circle (at 8.255 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 27 LA10_P) (clearance 0.1))
    (pad D14 smd circle (at 8.255 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 25 LA09_P) (clearance 0.1))
    (pad D13 smd circle (at 9.525 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C13 smd circle (at 9.525 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C17 smd circle (at 4.445 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D17 smd circle (at 4.445 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 33 LA13_P) (clearance 0.1))
    (pad D18 smd circle (at 3.175 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 32 LA13_N) (clearance 0.1))
    (pad C18 smd circle (at 3.175 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 86 LA14_P) (clearance 0.1))
    (pad C16 smd circle (at 5.715 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D16 smd circle (at 5.715 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D15 smd circle (at 6.985 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 24 LA09_N) (clearance 0.1))
    (pad C15 smd circle (at 6.985 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 26 LA10_N) (clearance 0.1))
    (pad C22 smd circle (at -1.905 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 82 LA18_P_CC) (clearance 0.1))
    (pad D22 smd circle (at -1.905 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D23 smd circle (at -3.175 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 48 LA23_P) (clearance 0.1))
    (pad C23 smd circle (at -3.175 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 83 LA18_N_CC) (clearance 0.1))
    (pad C25 smd circle (at -5.715 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D25 smd circle (at -5.715 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D24 smd circle (at -4.445 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 70 LA23_N) (clearance 0.1))
    (pad C24 smd circle (at -4.445 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D21 smd circle (at -0.625 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 38 LA17_N_CC) (clearance 0.1))
    (pad C21 smd circle (at -0.635 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C20 smd circle (at 0.635 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D20 smd circle (at 0.635 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 39 LA17_P_CC) (clearance 0.1))
    (pad D19 smd circle (at 1.905 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C19 smd circle (at 1.905 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 87 LA14_N) (clearance 0.1))
    (pad C03 smd circle (at 22.225 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad D03 smd circle (at 22.225 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D04 smd circle (at 20.955 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C04 smd circle (at 20.955 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C06 smd circle (at 18.415 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad D06 smd circle (at 18.415 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D05 smd circle (at 19.685 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C05 smd circle (at 19.685 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C09 smd circle (at 14.605 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D09 smd circle (at 14.605 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 10 LA01_N_CC) (clearance 0.1))
    (pad D10 smd circle (at 13.335 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C10 smd circle (at 13.335 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 19 LA06_P) (clearance 0.1))
    (pad C08 smd circle (at 15.875 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D08 smd circle (at 15.875 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 11 LA01_P_CC) (clearance 0.1))
    (pad D07 smd circle (at 17.145 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad C07 smd circle (at 17.145 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad D02 smd circle (at 23.495 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND) (clearance 0.1))
    (pad D01 smd circle (at 24.765 1.905 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (clearance 0.1))
    (pad C01 smd circle (at 24.765 3.175 90) (size 0.64 0.64) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (pad "" np_thru_hole circle (at -27.19 -3.05 90) (size 1.27 1.27) (drill 1.27) (layers *.Cu *.Mask B.SilkS)
      (clearance 0.1))
    (pad C01 thru_hole circle (at 31.19 -2 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 7 DGND) (zone_connect 2))
  )
  (module Kaklik_konektory:SATA-7_THT_VERT (layer F.Cu) (tedit 5329A83A)
    (at 162.2 74.5 270)
    (fp_text reference J2 (at -1.9866 3.323 270) (layer F.SilkS))
    (fp_text value SATA7-67491-1030 (at 0.5 -1.7 270) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at 6.27 0 270) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J2-Pad2)"))
    (pad 8 thru_hole circle (at -6.56 -1 270) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 3 thru_hole oval (at 1.27 0 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J2-Pad3)"))
    (pad 5 thru_hole oval (at -1.27 0 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 0 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at -3.81 1.5 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole oval (at 0 1.5 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 1 thru_hole oval (at 3.81 1.5 270) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
  )
  (module Jumpery_MLAB:Pin_Header_Straight_2x03 placed (layer F.Cu) (tedit 53297683)
    (at 161.6 107.6 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J8 (at -5.2994 -0.1322 180) (layer F.SilkS))
    (fp_text value JUMP_3X2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 3V3))
    (pad 3 thru_hole rect (at 2.54 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole rect (at 2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 5 thru_hole rect (at 0 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 3V3))
    (pad 6 thru_hole rect (at -2.54 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 placed (layer B.Cu) (tedit 53235B43)
    (at 179.25 84.85)
    (attr smd)
    (fp_text reference C1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value C (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53235B43)
    (at 172.4 72.75 180)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value C (at 0 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_tant_B (layer B.Cu) (tedit 53235B44)
    (at 167.1 109.2 90)
    (descr "SMT capacitor, tantalum size B")
    (fp_text reference C3 (at 0 1.9685 90) (layer B.SilkS))
    (fp_text value CP1 (at 0 -1.9685 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.524 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at -1.524 0 90) (size 1.95072 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/capacitors/c_tant_B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:MSOP10-0.5 (layer B.Cu) (tedit 53235B43)
    (at 175.6 75.4 270)
    (descr "MSOP10 10pins pitch 0.5mm")
    (attr smd)
    (fp_text reference U1 (at 0 0.635 270) (layer B.SilkS))
    (fp_text value SY55857L (at 0 -0.762 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.016 -2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 19 LA06_P))
    (pad 2 smd rect (at -0.508 -2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 18 LA06_N))
    (pad 3 smd rect (at 0 -2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 11 LA01_P_CC))
    (pad 4 smd rect (at 0.508 -2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 10 LA01_N_CC))
    (pad 5 smd rect (at 1.016 -2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (pad 6 smd rect (at 1.016 2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(J2-Pad2)"))
    (pad 7 smd rect (at 0.508 2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(J2-Pad3)"))
    (pad 8 smd rect (at 0 2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(J2-Pad5)"))
    (pad 9 smd rect (at -0.508 2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(J2-Pad6)"))
    (pad 10 smd rect (at -1.016 2.2225 270) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (model smd\MSOP_10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.35 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:MSOP10-0.5 (layer B.Cu) (tedit 5323756D)
    (at 175.5 82.3 90)
    (descr "MSOP10 10pins pitch 0.5mm")
    (attr smd)
    (fp_text reference U2 (at 0 0.635 270) (layer B.SilkS))
    (fp_text value SY55855V (at 0 -0.762 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.016 -2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(J3-Pad6)"))
    (pad 2 smd rect (at -0.508 -2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(J3-Pad5)"))
    (pad 3 smd rect (at 0 -2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 0.508 -2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(J3-Pad2)"))
    (pad 5 smd rect (at 1.016 -2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (pad 6 smd rect (at 1.016 2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 4 CLK0_M2C_P))
    (pad 7 smd rect (at 0.508 2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 CLK0_M2C_N))
    (pad 8 smd rect (at 0 2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 13 LA02_P))
    (pad 9 smd rect (at -0.508 2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 12 LA02_N))
    (pad 10 smd rect (at -1.016 2.2225 90) (size 0.26924 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (model smd\MSOP_10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.35 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_Jumpery:Pin_Header_Straight_2x02 placed (layer F.Cu) (tedit 53236E99)
    (at 203.8 120.5 90)
    (descr "1 pin")
    (tags "CONN DEV")
    (fp_text reference J11 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value JUMP_2X2_CONN (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 68 SDA))
    (pad 2 thru_hole rect (at 1.27 1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 67 SCL))
    (pad 3 thru_hole rect (at 1.27 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 67 SCL))
    (pad 4 thru_hole rect (at -1.27 -1.27 90) (size 1.651 1.651) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 68 SDA))
    (model Pin_Headers/Pin_Header_Straight_2x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 181.95 78.35 90)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 10 LA01_N_CC))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 11 LA01_P_CC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 181.95 74.75 90)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 100R (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 18 LA06_N))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 19 LA06_P))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 161.05 91.95)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 127R (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J3-Pad3)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 169.8 88.05 270)
    (attr smd)
    (fp_text reference R4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 82R (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(J3-Pad3)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 161.1 96.2)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 127R (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(J3-Pad6)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 167.7 97 270)
    (attr smd)
    (fp_text reference R6 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 82R (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(J3-Pad6)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 161.1 94.3)
    (attr smd)
    (fp_text reference R7 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 127R (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(J3-Pad5)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 167.7 93.3 90)
    (attr smd)
    (fp_text reference R8 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 82R (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(J3-Pad5)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 161.05 90.15)
    (attr smd)
    (fp_text reference R9 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 127R (at 0 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(J3-Pad2)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53237AA1)
    (at 167.9 86.1 90)
    (attr smd)
    (fp_text reference R10 (at 0 0.3175 90) (layer B.SilkS))
    (fp_text value 82R (at 0 -0.381 90) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kaklik_konektory:SATA-7_THT_VERT (layer F.Cu) (tedit 53238422)
    (at 163.8 93 90)
    (fp_text reference J3 (at 0.6 -3.9 90) (layer F.SilkS))
    (fp_text value SATA7-67491-1030 (at 0.5 -1.7 90) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at 6.27 0 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J3-Pad2)"))
    (pad 8 thru_hole circle (at -6.56 -1 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J3-Pad3)"))
    (pad 5 thru_hole oval (at -1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at -3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole oval (at 0 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 1 thru_hole oval (at 3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
  )
  (module Kaklik_konektory:SATA-7_THT_VERT (layer F.Cu) (tedit 53238422)
    (at 203.9 73.7 90)
    (fp_text reference J4 (at 0.6 -3.9 90) (layer F.SilkS))
    (fp_text value SATA7-67491-1030 (at 0.5 -1.7 90) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at 6.27 0 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 84 LA05_P))
    (pad 8 thru_hole circle (at -6.56 -1 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 85 LA05_N))
    (pad 5 thru_hole oval (at -1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 27 LA10_P))
    (pad 6 thru_hole oval (at -2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 26 LA10_N))
    (pad 7 thru_hole oval (at -3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole oval (at 0 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 1 thru_hole oval (at 3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
  )
  (module Kaklik_konektory:SATA-7_THT_VERT (layer F.Cu) (tedit 53247905)
    (at 176 68.3)
    (fp_text reference J5 (at 0.05 3.65) (layer F.SilkS))
    (fp_text value SATA7-67491-1030 (at 0.5 -1.7) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at 6.27 0) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 6 CLK1_M2C_P))
    (pad 8 thru_hole circle (at -6.56 -1) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 3 thru_hole oval (at 1.27 0) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 5 CLK1_M2C_N))
    (pad 5 thru_hole oval (at -1.27 0) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 9 LA00_P_CC))
    (pad 6 thru_hole oval (at -2.54 0) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 8 LA00_N_CC))
    (pad 7 thru_hole oval (at -3.81 1.5) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole oval (at 0 1.5) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 1 thru_hole oval (at 3.81 1.5) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
  )
  (module Kaklik_konektory:SAS_mini_1888174 (layer F.Cu) (tedit 5329A846)
    (at 177.9 95.69 270)
    (descr "36pin mini SAS connector")
    (tags "SAS mini connector")
    (fp_text reference J7 (at -0.9262 -7.4184 270) (layer F.SilkS))
    (fp_text value SAS_mini_1888174 (at 0 0 270) (layer F.SilkS) hide)
    (pad B1 smd oval (at -7 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B2 smd oval (at -6.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 15 LA03_P))
    (pad B3 smd oval (at -5.4 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 LA03_N))
    (pad B4 smd oval (at -4.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B5 smd oval (at -3.8 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 LA08_P))
    (pad B6 smd oval (at -3 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 LA08_N))
    (pad B7 smd oval (at -2.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B8 smd oval (at -1.4 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 31 LA12_P))
    (pad B9 smd oval (at -0.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 30 LA12_N))
    (pad B10 smd oval (at 0.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 86 LA14_P))
    (pad B11 smd oval (at 1 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 87 LA14_N))
    (pad B12 smd oval (at 1.8 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B13 smd oval (at 2.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 37 LA16_P))
    (pad B14 smd oval (at 3.4 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 36 LA16_N))
    (pad B15 smd oval (at 4.2 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad B16 smd oval (at 5 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 39 LA17_P_CC))
    (pad B17 smd oval (at 5.8 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 38 LA17_N_CC))
    (pad A1 smd oval (at -6.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A2 smd oval (at -5.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 LA04_P))
    (pad A3 smd oval (at -4.9 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 16 LA04_N))
    (pad A4 smd oval (at -4.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A5 smd oval (at -3.3 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 21 LA07_P))
    (pad A6 smd oval (at -2.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 LA07_N))
    (pad A7 smd oval (at -1.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A8 smd oval (at -0.9 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 25 LA09_P))
    (pad A9 smd oval (at -0.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 24 LA09_N))
    (pad A10 smd oval (at 0.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 33 LA13_P))
    (pad A11 smd oval (at 1.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 32 LA13_N))
    (pad A12 smd oval (at 2.3 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A13 smd oval (at 3.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 29 LA11_P))
    (pad A14 smd oval (at 3.9 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 28 LA11_N))
    (pad A15 smd oval (at 4.7 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A16 smd oval (at 5.5 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 35 LA15_P))
    (pad A17 smd oval (at 6.3 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 34 LA15_N))
    (pad 1 thru_hole circle (at -8.9 -5.24 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 2 thru_hole circle (at -8.9 -2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 4 thru_hole circle (at -8.9 4.03 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 3 thru_hole circle (at -8.9 2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 5 thru_hole circle (at 8.9 -6.24 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 6 thru_hole circle (at 8.9 -2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad "" np_thru_hole circle (at -8 0 270) (size 1.55 1.55) (drill 1.55) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 8 0 270) (size 1.55 1.55) (drill 1.55) (layers *.Mask B.Cu F.SilkS))
    (pad 8 thru_hole circle (at 8.9 4.03 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad 7 thru_hole circle (at 8.9 2 270) (size 1.55 1.55) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND) (zone_connect 2))
    (pad B18 smd oval (at 6.6 -2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (pad A18 smd oval (at 7.1 2.91 270) (size 0.35 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 DGND))
    (model /home/kaklik/git/Connect.pretty/SAS_mini_1888174.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Kaklik_konektory:SATA-7_THT_VERT (layer F.Cu) (tedit 53238422)
    (at 203.8 108.8 90)
    (fp_text reference J9 (at 0.6 -3.9 90) (layer F.SilkS))
    (fp_text value SATA7-67491-1030 (at 0.5 -1.7 90) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at 6.27 0 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 48 LA23_P))
    (pad 8 thru_hole circle (at -6.56 -1 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 70 LA23_N))
    (pad 5 thru_hole oval (at -1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 54 LA26_P))
    (pad 6 thru_hole oval (at -2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 53 LA26_N))
    (pad 7 thru_hole oval (at -3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole oval (at 0 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 1 thru_hole oval (at 3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
  )
  (module Kaklik_konektory:SATA-7_THT_VERT (layer F.Cu) (tedit 53238422)
    (at 203.8 91.3 90)
    (fp_text reference J10 (at 0.6 -3.9 90) (layer F.SilkS))
    (fp_text value SATA7-67491-1030 (at 0.5 -1.7 90) (layer F.SilkS) hide)
    (pad 9 thru_hole circle (at 6.27 0 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 82 LA18_P_CC))
    (pad 8 thru_hole circle (at -6.56 -1 90) (size 2.5 2.5) (drill 1.35) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 83 LA18_N_CC))
    (pad 5 thru_hole oval (at -1.27 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 80 LA27_P))
    (pad 6 thru_hole oval (at -2.54 0 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 81 LA27_N))
    (pad 7 thru_hole oval (at -3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 4 thru_hole oval (at 0 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
    (pad 1 thru_hole oval (at 3.81 1.5 90) (size 1.1 1.3) (drill 0.74) (layers *.Cu *.Mask F.SilkS)
      (net 7 DGND))
  )
  (module SMD_Packages:SM0805 (layer B.Cu) (tedit 53247790)
    (at 180.8 130.2 270)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value C (at 0 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 DGND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 5329A851)
    (at 192.95 116.55)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P1 (at 0.6996 -2.3044) (layer F.SilkS))
    (fp_text value CONN_1 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 79 TRST_L))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 532979C7)
    (at 198.65 122.75)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P2 (at -2.689 0.0808) (layer F.SilkS))
    (fp_text value CONN_1 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 53297936)
    (at 187.1 124.65)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P3 (at 0 -2.54) (layer F.SilkS))
    (fp_text value CONN_1 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 69 VDD))
  )
  (gr_text "PECL OUT" (at 165.862 74.6724 90) (layer F.SilkS))
  (gr_text "PECL IN" (at 167.64 92.7826 90) (layer F.SilkS))
  (gr_text 3.3V (at 165.4048 107.54 90) (layer F.SilkS))
  (dimension 68.9864 (width 0.25) (layer Dwgs.User)
    (gr_text "68,986 mm" (at 212.5058 98.904 90) (layer Dwgs.User))
    (feature1 (pts (xy 208.6102 64.4108) (xy 213.5058 64.4108)))
    (feature2 (pts (xy 208.6102 133.3972) (xy 213.5058 133.3972)))
    (crossbar (pts (xy 211.5058 133.3972) (xy 211.5058 64.4108)))
    (arrow1a (pts (xy 211.5058 64.4108) (xy 212.092221 65.537304)))
    (arrow1b (pts (xy 211.5058 64.4108) (xy 210.919379 65.537304)))
    (arrow2a (pts (xy 211.5058 133.3972) (xy 212.092221 132.270696)))
    (arrow2b (pts (xy 211.5058 133.3972) (xy 210.919379 132.270696)))
  )
  (dimension 18.1 (width 0.25) (layer Dwgs.User)
    (gr_text "18,100 mm" (at 199.55 138.15) (layer Dwgs.User))
    (feature1 (pts (xy 208.6 130.4) (xy 208.6 139.15)))
    (feature2 (pts (xy 190.5 130.4) (xy 190.5 139.15)))
    (crossbar (pts (xy 190.5 137.15) (xy 208.6 137.15)))
    (arrow1a (pts (xy 208.6 137.15) (xy 207.473496 137.736421)))
    (arrow1b (pts (xy 208.6 137.15) (xy 207.473496 136.563579)))
    (arrow2a (pts (xy 190.5 137.15) (xy 191.626504 137.736421)))
    (arrow2b (pts (xy 190.5 137.15) (xy 191.626504 136.563579)))
  )
  (dimension 51.100024 (width 0.25) (layer Dwgs.User)
    (gr_text "51,100 mm" (at 183.046624 60.974953 0.05606238868) (layer Dwgs.User))
    (feature1 (pts (xy 208.6 64.4) (xy 208.595646 59.949954)))
    (feature2 (pts (xy 157.5 64.45) (xy 157.495646 59.999954)))
    (crossbar (pts (xy 157.497603 61.999953) (xy 208.597603 61.949953)))
    (arrow1a (pts (xy 208.597603 61.949953) (xy 207.471674 62.537476)))
    (arrow1b (pts (xy 208.597603 61.949953) (xy 207.470526 61.364635)))
    (arrow2a (pts (xy 157.497603 61.999953) (xy 158.62468 62.585271)))
    (arrow2b (pts (xy 157.497603 61.999953) (xy 158.623532 61.41243)))
  )
  (gr_text FMC2DIFF01A (at 163.5 123.2 90) (layer B.Cu))
  (gr_text "Kaklik 2014" (at 180.975 78.584 90) (layer F.SilkS))
  (gr_text www.mlab.cz (at 171.2214 78.2284 90) (layer F.SilkS))
  (gr_text FMC2DIFF01A (at 169.4434 78.457 90) (layer F.SilkS))
  (gr_text "KAKLIK 2014" (at 165.6 123.2 90) (layer B.Cu))
  (gr_line (start 190.6 133.4) (end 190.6 133.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.5 133.4) (end 190.6 133.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.5 64.4) (end 157.5 133.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.5 64.4) (end 157.5 64.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 208.6 64.4) (end 160.5 64.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 208.6 133.4) (end 208.6 64.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 133.4) (end 208.6 133.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name DGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157.85 64.8) (xy 208.25 64.75) (xy 208.1 132.95) (xy 157.85 133) (xy 157.7 64.8)
        (xy 157.85 64.8)
      )
    )
  )
  (zone (net 7) (net_name DGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.35 64.65) (xy 208.2 133) (xy 157.75 133.1) (xy 157.7 64.75)
      )
    )
  )
)
