(kicad_pcb (version 20160815) (host pcbnew "(2016-09-17 revision 679eef1)-makepkg")
  (general
    (links 53)
    (no_connects 0)
    (area -7.239 -44.831 81.026001 4.572001)
    (thickness 1.6)
    (drawings 24)
    (tracks 180)
    (zones 0)
    (modules 23)
    (nets 8)
  )
  (page A4)
  (title_block
    (title NAME)
    (date "%d. %m. %Y")
    (rev REV)
    (company "Mlab www.mlab.cz")
    (comment 1 VERSION)
    (comment 2 "Short description\\nTwo lines are maximum")
    (comment 3 "nickname <email@example.com>")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /3)
  (net 4 /1)
  (net 5 /5)
  (net 6 /6)
  (net 7 /2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.25)
    (add_net /1)
    (add_net /2)
    (add_net /3)
    (add_net /5)
    (add_net /6)
    (add_net GND)
    (add_net VCC)
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 587C7558)
    (at 45.72 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 587C7558)
    (at 5.08 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 587C7558)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 587C7558)
    (at 45.72 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 1 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 13.97 -25.4 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J1 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 16.51 -25.4 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J2 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /2))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /2))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 19.05 -25.4 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 21.59 -25.4 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /3))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /3))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 24.13 -25.4 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 587C7558)
    (at 21.7805 -21.336)
    (attr smd)
    (fp_text reference C4 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10uF (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 5 /5))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_IO:SOT-553 (layer B.Cu) (tedit 587C7558)
    (at 26.42362 -13.52296 90)
    (descr SOT553)
    (attr smd)
    (fp_text reference D2 (at 2.22504 -0.00762 90) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.70104 0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 7 /2))
    (pad 3 smd rect (at -0.70104 -0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 5 smd rect (at 0.70104 0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 4 /1))
    (pad 2 smd rect (at -0.70104 0 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.70104 -0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 3 /3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:SOT-553 (layer B.Cu) (tedit 587C7558)
    (at 24.13 -13.462 90)
    (descr SOT553)
    (attr smd)
    (fp_text reference D3 (at 2.286 0 90) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874 90) (layer B.Fab) hide)
    (pad 4 smd rect (at 0.70104 -0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 5 /5))
    (pad 2 smd rect (at -0.70104 0 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.70104 0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -0.70104 -0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 6 /6))
    (pad 1 smd rect (at -0.70104 0.50038 90) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x02 (layer F.Cu) (tedit 587C7558)
    (at 35.56 -25.4 270)
    (descr "pin header straight 2x02")
    (tags "pin header straight 2x02")
    (fp_text reference J6 (at 0 -3.81 270) (layer F.SilkS) hide)
    (fp_text value JUMP_2X2 (at 0 3.81 270) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /6))
    (pad 2 thru_hole rect (at 1.27 -1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /6))
    (pad 3 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /1))
    (pad 4 thru_hole rect (at 1.27 1.27 270) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /1))
    (model Pin_Headers/Pin_Header_Straight_2x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 12.7 -21.59)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 45.72 -19.05 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /1))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 45.72 -16.51 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /6))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /2))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 587C7558)
    (at 17.526 -19.304)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381) (layer B.SilkS))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 7 /2))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_R:SMD-0805 (layer B.Cu) (tedit 587C7558)
    (at 20.828 -19.304 180)
    (attr smd)
    (fp_text reference R5 (at 0 0.3175 180) (layer B.SilkS))
    (fp_text value 10k (at 0.127 -0.381 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 3 /3))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Mlab_CON:RJ12GLP-AMP(RJ12)" (layer F.Cu) (tedit 587C7558)
    (at 32.512 -7.874 90)
    (fp_text reference J8 (at -1.6764 0.254) (layer F.SilkS))
    (fp_text value RJ12GLP-AMP (at -5.9055 0.3302) (layer F.Fab) hide)
    (pad 5 thru_hole circle (at 7.3125 2.3572 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5))
    (pad 3 thru_hole circle (at 7.3125 -0.1828 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3))
    (pad 1 thru_hole circle (at 7.3125 -2.7228 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /1))
    (pad 2 thru_hole circle (at 4.7725 -1.4528 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /2))
    (pad 6 thru_hole circle (at 4.7725 3.6272 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /6))
    (pad 4 thru_hole circle (at 4.7725 1.0872 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 8 thru_hole circle (at -1.5875 5.5372 270) (size 4 4) (drill 3.25) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.5875 -4.6228 270) (size 4 4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module "Mlab_CON:RJ12GLP-AMP(RJ12)" (layer F.Cu) (tedit 587C7558)
    (at 17.272 -7.874 90)
    (fp_text reference J9 (at -1.6764 0.254) (layer F.SilkS))
    (fp_text value RJ12GLP-AMP (at -5.9055 0.3302) (layer F.Fab) hide)
    (pad 7 thru_hole circle (at -1.5875 -4.6228 270) (size 4 4) (drill 3.25) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -1.5875 5.5372 270) (size 4 4) (drill 3.25) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 4.7725 1.0872 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 6 thru_hole circle (at 4.7725 3.6272 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /6))
    (pad 2 thru_hole circle (at 4.7725 -1.4528 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /2))
    (pad 1 thru_hole circle (at 7.3125 -2.7228 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /1))
    (pad 3 thru_hole circle (at 7.3125 -0.1828 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3))
    (pad 5 thru_hole circle (at 7.3125 2.3572 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5))
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 45.72 -13.97 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J12 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /3))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 587C7558)
    (at 45.72 -11.43 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J13 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP2_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 587C7558)
    (at 5.08 -15.24)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J14 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (dimension 50.292 (width 0.3) (layer Dwgs.User)
    (gr_text "1,9800 in" (at 25.4 -33.9636) (layer Dwgs.User))
    (feature1 (pts (xy 50.546 -30.226) (xy 50.546 -35.3136)))
    (feature2 (pts (xy 0.254 -30.226) (xy 0.254 -35.3136)))
    (crossbar (pts (xy 0.254 -32.6136) (xy 50.546 -32.6136)))
    (arrow1a (pts (xy 50.546 -32.6136) (xy 49.419496 -32.027179)))
    (arrow1b (pts (xy 50.546 -32.6136) (xy 49.419496 -33.200021)))
    (arrow2a (pts (xy 0.254 -32.6136) (xy 1.380504 -32.027179)))
    (arrow2b (pts (xy 0.254 -32.6136) (xy 1.380504 -33.200021)))
  )
  (dimension 29.972 (width 0.3) (layer Dwgs.User)
    (gr_text "1,1800 in" (at 54.7408 -15.24 90) (layer Dwgs.User))
    (feature1 (pts (xy 50.546 -30.226) (xy 56.0908 -30.226)))
    (feature2 (pts (xy 50.546 -0.254) (xy 56.0908 -0.254)))
    (crossbar (pts (xy 53.3908 -0.254) (xy 53.3908 -30.226)))
    (arrow1a (pts (xy 53.3908 -30.226) (xy 53.977221 -29.099496)))
    (arrow1b (pts (xy 53.3908 -30.226) (xy 52.804379 -29.099496)))
    (arrow2a (pts (xy 53.3908 -0.254) (xy 53.977221 -1.380504)))
    (arrow2b (pts (xy 53.3908 -0.254) (xy 52.804379 -1.380504)))
  )
  (gr_text 6 (at 48.514 -16.51) (layer F.SilkS))
  (gr_text 5 (at 48.514 -19.05) (layer F.SilkS))
  (gr_text 4 (at 42.926 -11.43) (layer F.SilkS))
  (gr_text 3 (at 42.926 -13.97) (layer F.SilkS))
  (gr_text 2 (at 42.926 -16.51) (layer F.SilkS))
  (gr_text 1 (at 42.926 -19.05) (layer F.SilkS))
  (gr_text 6 (at 36.83 -22.352 90) (layer F.SilkS))
  (gr_text 1 (at 34.29 -22.352 90) (layer F.SilkS))
  (gr_text GND (at 24.13 -22.352 90) (layer F.SilkS))
  (gr_text SCL (at 21.59 -22.352 90) (layer F.SilkS))
  (gr_text SDA (at 19.05 -22.352 90) (layer F.SilkS))
  (gr_text SDA (at 16.51 -22.352 90) (layer F.SilkS))
  (gr_text JACHO (at 33.02 -4.572) (layer F.SilkS))
  (gr_text "MLAB.CZ\nRJ12V01A" (at 29.21 -23.114 90) (layer F.SilkS))
  (gr_text 2017 (at 33.02 -2.54) (layer F.SilkS))
  (gr_text 2017 (at 33.02 -2.54) (layer B.Cu))
  (gr_text MLAB (at 33.02 -4.572) (layer B.Cu))
  (gr_line (start 0.254 -40.386) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -0.254) (end 50.546 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.546 -40.386) (end 50.546 -0.254) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 0.254 -40.386) (end 50.546 -40.386) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.026 -44.196) (xy 75.946 4.572) (xy -7.239 3.556) (xy -4.572 -44.831)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.676 -42.545) (xy 73.66 1.524) (xy -2.921 1.524) (xy -1.651 -43.434)
      )
    )
  )
)
