(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 50)
    (no_connects 0)
    (area 86.5505 40.513 135.763001 98.933001)
    (thickness 1.6)
    (drawings 21)
    (tracks 118)
    (zones 0)
    (modules 24)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (user_trace_width 0.8)
    (user_trace_width 0.9)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.89)
    (via_drill 0.5)
    (via_min_size 0.89)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.3)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.300000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../CAM_PROFI/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /INT+)
  (net 4 /INT-)
  (net 5 /SCL-)
  (net 6 /SCL+)
  (net 7 /SDA+)
  (net 8 /SDA-)
  (net 9 "Net-(C2-Pad1)")
  (net 10 /D1_K)
  (net 11 /D2_K)
  (net 12 /D2_A)
  (net 13 /D1_A)
  (net 14 "Net-(J7-Pad10)")
  (net 15 "Net-(J7-Pad12)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /D1_A)
    (add_net /D1_K)
    (add_net /D2_A)
    (add_net /D2_K)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J7-Pad10)")
    (add_net "Net-(J7-Pad12)")
    (add_net VCC)
  )
  (net_class dif ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.89)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.127)
    (add_net /INT+)
    (add_net /INT-)
    (add_net /SCL+)
    (add_net /SCL-)
    (add_net /SDA+)
    (add_net /SDA-)
  )
  (module Mlab_IO:SOT-553 (layer B.Cu) (tedit 5703B5F6)
    (at 25.5905 -25.273 270)
    (descr SOT553)
    (attr smd)
    (fp_text reference D1 (at 0 -0.0635 270) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.70104 0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -0.70104 -0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 0.70104 0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 7 /SDA+))
    (pad 2 smd rect (at -0.70104 0 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.70104 -0.50038 270) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 8 /SDA-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Mlab_CON:RJHSE-5384(RJ45)" (layer F.Cu) (tedit 56B2FDC0)
    (at 13.97 -5.842)
    (fp_text reference J7 (at 4.445 -9.271) (layer F.SilkS))
    (fp_text value RJ45_RJHSE-5384 (at 6.4516 4.1275) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 12.7 0) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 14.48 -3.43) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at -1.78 -3.43) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C2-Pad1)"))
    (pad 7 thru_hole circle (at 3.81 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 4 /INT-))
    (pad 5 thru_hole circle (at 5.84 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.87 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL-))
    (pad 1 thru_hole circle (at 9.9 -2.54) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA-))
    (pad 8 thru_hole circle (at 2.79 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 3 /INT+))
    (pad 6 thru_hole circle (at 4.82 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL+))
    (pad 4 thru_hole circle (at 6.85 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 8.88 -4.32) (size 1.3 1.3) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA+))
    (pad 9 thru_hole circle (at 13.21 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D2_K))
    (pad 10 thru_hole circle (at 10.92 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J7-Pad10)"))
    (pad 11 thru_hole circle (at 1.78 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D1_K))
    (pad 12 thru_hole circle (at -0.51 -9.14) (size 1.5 1.5) (drill 0.93) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J7-Pad12)"))
  )
  (module Mlab_Pin_Headers:Straight_2x04 (layer F.Cu) (tedit 56B0BB66)
    (at 36.83 -15.6845)
    (descr "pin header straight 2x04")
    (tags "pin header straight 2x04")
    (fp_text reference J1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value JUMP_4X2 (at 0 6.35) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.921 -3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.27 -3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at -1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole rect (at 1.27 -1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 5 thru_hole rect (at -1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 6 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 7 thru_hole rect (at -1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole rect (at 1.27 3.81) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_2x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 10.668 -4.953 270)
    (attr smd)
    (fp_text reference C2 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 100nF (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 4.8895 -12.3825 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J4 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D2_K))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D2_K))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 4.8895 -14.9225 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J5 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D2_A))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D2_A))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 4.8895 -17.4625 180)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J6 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /D1_A))
    (pad 2 thru_hole rect (at 1.27 0 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 13 /D1_A))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 14.224 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J8 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /INT+))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 3 /INT+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 16.764 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J9 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /INT-))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 4 /INT-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M1 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M2 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 5.08 -5.08)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M3 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module Mlab_Mechanical:MountingHole_3mm placed (layer F.Cu) (tedit 5535DB2C)
    (at 35.56 -25.4)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference M4 (at 0 -4.191) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 4.191) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Adhes *.Mask)
      (net 2 GND) (clearance 1) (zone_connect 2))
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.652 -14.9225)
    (attr smd)
    (fp_text reference R1 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 12 /D2_A))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J7-Pad10)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.652 -17.526)
    (attr smd)
    (fp_text reference R2 (at 0 0.3175) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 13 /D1_A))
    (pad 2 smd rect (at 0.9525 0) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J7-Pad12)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MLAB_R:SMD-0805 (layer B.Cu) (tedit 54799E0C)
    (at 9.0805 -9.779 270)
    (attr smd)
    (fp_text reference R3 (at 0 0.3175 270) (layer B.SilkS))
    (fp_text value 1k (at 0.127 -0.381 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (model MLAB_3D/Resistors/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mlab_Pin_Headers:Straight_1x02 (layer F.Cu) (tedit 5535DB0D)
    (at 4.8895 -20.0025 90)
    (descr "pin header straight 1x02")
    (tags "pin header straight 1x02")
    (fp_text reference J3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text user 1 (at -1.651 -1.27 90) (layer F.SilkS) hide)
    (pad 2 thru_hole rect (at 0 1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D1_K))
    (pad 1 thru_hole rect (at 0 -1.27 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D1_K))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_C:TantalC_SizeC_Reflow (layer B.Cu) (tedit 564C624B)
    (at 30.5435 -22.606 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (tags "Tantal Cap. , Size C, EIA-6032, Reflow,")
    (attr smd)
    (fp_text reference C1 (at 0.0127 -0.0381 90) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 90) (layer B.SilkS) hide)
    (fp_text user + (at -4.99872 2.55016 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Capacitors/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 19.304 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J10 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL+))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SCL+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 21.844 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J11 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL-))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SCL-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 26.924 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J13 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA-))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA-))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_Pin_Headers:Straight_2x01 (layer F.Cu) (tedit 5545E8D2)
    (at 24.384 -19.304 90)
    (descr "pin header straight 2x01")
    (tags "pin header straight 2x01")
    (fp_text reference J12 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value JUMP_2x1 (at 0 2.54 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA+))
    (pad 2 thru_hole rect (at 1.27 0 90) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SDA+))
    (model Pin_Headers/Pin_Header_Straight_2x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_IO:SOT-553 (layer B.Cu) (tedit 5703B5EF)
    (at 18.034 -25.654)
    (descr SOT553)
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer B.SilkS))
    (fp_text value SP1001-04XTG (at 0 -1.34874) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.70104 0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 4 /INT-))
    (pad 3 smd rect (at -0.70104 -0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 3 /INT+))
    (pad 5 smd rect (at 0.70104 0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCL+))
    (pad 2 smd rect (at -0.70104 0) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.70104 -0.50038) (size 0.44958 0.29972) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCL-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mlab_D:Diode-SMC_Standard (layer B.Cu) (tedit 54799AAC)
    (at 31.75 -12.7635 90)
    (descr "Diode SMC Standard")
    (tags "Diode SMC Standard")
    (attr smd)
    (fp_text reference D3 (at 0 5.08 90) (layer B.SilkS))
    (fp_text value SM15T18A (at 0 -5.08 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -3.40106 0) (size 3.29946 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.40106 0) (size 3.29946 2.49936) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model MLAB_3D/Diodes/SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text D2K (at 7.6835 -12.319) (layer F.SilkS))
  (gr_text D2A (at 7.62 -14.9225) (layer F.SilkS))
  (gr_text D1A (at 7.62 -17.526) (layer F.SilkS))
  (gr_text SCL+ (at 19.304 -22.4155 90) (layer F.SilkS))
  (gr_text INT- (at 16.764 -22.352 90) (layer F.SilkS))
  (gr_text SCL- (at 21.7805 -22.4155 90) (layer F.SilkS))
  (gr_text EXT (at 33.147 -15.748 90) (layer F.SilkS))
  (gr_text 2016 (at 20.32 -5.842) (layer F.SilkS))
  (gr_text MLAB.CZ (at 11.2395 -24.0665 90) (layer B.Cu))
  (gr_text JACHO (at 20.066 -12.7) (layer F.SilkS))
  (gr_text MLAB.CZ (at 31.115 -5.588 90) (layer F.SilkS))
  (gr_text RJ45V01A (at 9.3345 -5.6515 90) (layer F.SilkS))
  (gr_text SDA- (at 26.924 -22.352 90) (layer F.SilkS))
  (gr_text SDA+ (at 24.384 -22.352 90) (layer F.SilkS))
  (gr_text INT+ (at 14.224 -22.352 90) (layer F.SilkS))
  (gr_text POWER (at 30.9245 -15.8115 90) (layer F.SilkS))
  (gr_text D1K (at 7.62 -20.0025) (layer F.SilkS))
  (gr_line (start 0.254 -30.224) (end 0.254 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -30.224) (end 0.254 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.386 -0.254) (end 40.386 -30.224) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0.254 -0.254) (end 40.386 -0.254) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.91 -51.7525) (xy 41.529 0.8255) (xy -2.7305 2.794) (xy -1.4605 -51.6255)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.2385 -53.467) (xy 44.577 -53.213) (xy 43.18 3.2385) (xy -4.6355 4.953)
      )
    )
  )
)
