{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Nabijec_ucinnost"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Nabijec_ucinnost","index":0,"n_rows":14,"n_cols":15,"rows_kept":14,"cut":false,"hidden":false,"merged":[[3,8,3,10],[3,11,3,13]],"flags":["formulas_cached_only"]}
[]
[]
[{"$nulls":6},"Ri [ohm]",0.8246]
[{"$nulls":8},"měnič se snímáním proudu",null,null,"měnič bez snímání proudu"]
[null,null,null,"Uin [V]","Iin [A]","Pin [W]","URi [mV]","Iout [A]","Ubat [V]","Pbat [W]","Nbat [%]","Ubat+Uri [V]","Pbat+Pri [W]","Nbat+Ri [%]","PRi [W]"]
[null,null,null,8,1.307,10.456,548,0.6645646373999515,13.68,9.091244239631337,86.9476304478896,14.228,9.45542566092651,90.43062032255652,0.3641814212951733]
[null,null,null,9,1.16,10.44,549,0.6657773465922872,13.71,9.127807421780258,87.43110557260783,14.259,9.493319185059423,90.93217610210176,0.3655117632791658]
[null,null,null,10,1.043,10.43,550,0.6669900557846229,13.74,9.164443366480718,87.86618759808934,14.290000000000001,9.531287897162262,91.3833930696286,0.36684453068154355]
[null,null,null,11,0.95,10.45,550,0.6669900557846229,13.75,9.171113267038566,87.76184944534513,14.3,9.537957797720107,91.27232342315892,0.36684453068154177]
[null,null,null,12,0.875,10.5,553,0.6706281833616299,13.77,9.234550084889642,87.94809604656803,14.323,9.605407470288625,91.48007114560596,0.37085738539898294]
[null,null,null,13,0.811,10.543000000000001,554,0.6718408925539655,13.79,9.264685908319183,87.87523388332717,14.344,9.636885762794082,91.40553697044561,0.3721998544748981]
[null,null,null,15,0.712,10.68,556,0.674266310938637,13.8,9.30487509095319,87.12429860443063,14.356000000000002,9.679767159835073,90.6345239684932,0.3748920688818824]
[null,null,null,18,0.603,10.854,558,0.6766917293233083,13.81,9.345112781954889,86.09833040312226,14.368,9.722706766917295,89.57717677277773,0.3775939849624059]
[null,null,null,20,0.549,10.98,559,0.677904438515644,13.83,9.375418384671356,85.38632408626007,14.389,9.754366965801601,88.83758620948635,0.37894858113024554]